<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.4.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="43.1675" y2="0" width="0" layer="20"/>
<wire x1="43.1675" y1="0" x2="43.1675" y2="17.77" width="0" layer="20"/>
<wire x1="43.1675" y1="17.77" x2="0" y2="17.77" width="0" layer="20"/>
<wire x1="0" y1="17.77" x2="0" y2="0" width="0" layer="20"/>
<text>RADglow 5V Button Board V2</text>
<text>www.radglow.com</text>
</plain>
<libraries>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
</package>
</packages>
</library>
<library name="GeekAmmo">
<description>&lt;h3&gt;GeekAmmo  Library&lt;/h3&gt;

These are parts used by the GeekAmmo company (now part of SparkFun Electronics)!

 If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt;Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TAC-SWITCH-PTH">
</package>
</packages>
</library>
<library name="nano_shields">
<packages>
<package name="NANO_LED_SHIELD">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="PCB1" library="nano_shields" package="NANO_LED_SHIELD" value="NANO_LED_SHEILD"/>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.3" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="AXIAL-0.3" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="GeekAmmo" package="TAC-SWITCH-PTH" value="TACTILE-SWITCH-PTH">
<attribute name="NAME"/>
</element>
<element name="U$2" library="GeekAmmo" package="TAC-SWITCH-PTH" value="TACTILE-SWITCH-PTH">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="N$5">
<contactref element="PCB1" pad="D2"/>
<contactref element="R1" pad="P$2"/>
<contactref element="U$1" pad="4"/>
</signal>
<signal name="N$3">
<contactref element="R2" pad="P$2"/>
<contactref element="PCB1" pad="D3"/>
<contactref element="U$2" pad="3"/>
</signal>
<signal name="GND">
<contactref element="PCB1" pad="GNDSTRIP"/>
<contactref element="PCB1" pad="GND"/>
<contactref element="R2" pad="P$1"/>
<contactref element="R1" pad="P$1"/>
<contactref element="PCB1" pad="GND."/>
<contactref element="PCB1" pad="GNDIN2"/>
<contactref element="PCB1" pad="GNDIN1"/>
</signal>
<signal name="REF">
<contactref element="PCB1" pad="REF"/>
</signal>
<signal name="3V3">
<contactref element="PCB1" pad="3V3"/>
</signal>
<signal name="VIN">
<contactref element="PCB1" pad="VDDIN1"/>
<contactref element="PCB1" pad="VDDIN2"/>
<contactref element="PCB1" pad="VIN"/>
</signal>
<signal name="5V">
<contactref element="U$2" pad="2"/>
<contactref element="PCB1" pad="5V"/>
<contactref element="PCB1" pad="VDDSTRIP"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="PCB1" pad="D4"/>
<contactref element="PCB1" pad="CLKSTRIP"/>
</signal>
<signal name="N$7">
<contactref element="PCB1" pad="D5"/>
<contactref element="PCB1" pad="DATSTRIP"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
