<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="2.54" y1="0" x2="99.06" y2="0" width="0" layer="20"/>
<wire x1="99.06" y1="0" x2="101.6" y2="2.54" width="0" layer="20" curve="90"/>
<wire x1="101.6" y1="2.54" x2="101.6" y2="22.86" width="0" layer="20"/>
<wire x1="101.6" y1="22.86" x2="99.06" y2="25.4" width="0" layer="20" curve="90"/>
<wire x1="99.06" y1="25.4" x2="2.54" y2="25.4" width="0" layer="20"/>
<wire x1="2.54" y1="25.4" x2="0" y2="22.86" width="0" layer="20" curve="90"/>
<wire x1="0" y1="22.86" x2="0" y2="2.54" width="0" layer="20"/>
<wire x1="0" y1="2.54" x2="2.54" y2="0" width="0" layer="20" curve="90"/>
<hole x="86.36" y="1.905" drill="2.2"/>
<hole x="15.24" y="23.495" drill="2.2"/>
<hole x="15.24" y="1.905" drill="2.2"/>
<hole x="86.36" y="23.495" drill="2.2"/>
<hole x="50.8" y="23.495" drill="2.2"/>
<hole x="50.8" y="1.905" drill="2.2"/>
<text>Cherry Switch Teensy Breakout</text>
<text>Cherry Switch Teensy Breakout</text>
<text>by schizobovine
&lt;sean@yak.net&gt;</text>
<text>by schizobovine
&lt;sean@yak.net&gt;</text>
<text>&gt;VERSION</text>
<text>&gt;VERSION</text>
<text>Cherry Switch Teensy Breakout</text>
<text>&gt;VERSION</text>
<text>&gt;VERSION</text>
</plain>
<libraries>
<library name="A_butts">
<packages>
<package name="DUMMY">
<description>NOTHING HERE!!! For when you want a symbol with no package as an option against symbols with a package.</description>
</package>
<package name="CHERRY-MX-NONUBS">
</package>
<package name="DIODE-7.62MM">
</package>
<package name="1X01">
</package>
<package name="TEENSY_3.0_BASIC_ALT2">
</package>
<package name="C025-024X044">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 2.4 x 4.4 mm</description>
</package>
<package name="CC-BY-SA-4.0-URL-BOTTOM">
</package>
<package name="COW_SMALL_METAL">
</package>
<package name="OSHWLOGO_5MM_METAL">
</package>
</packages>
</library>
</libraries>
<attributes>
<attribute name="VERSION" value="v1.0"/>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="FRAME1" library="A_butts" package="DUMMY" value="FRAME-LETTERNO_PACKAGE">
<attribute name="VERSION" value="v01"/>
<attribute name="DESIGNER" value="Nobody"/>
</element>
<element name="SW1" library="A_butts" package="CHERRY-MX-NONUBS" value="CHERRY-MXNONUBS">
<attribute name="NAME"/>
</element>
<element name="SW2" library="A_butts" package="CHERRY-MX-NONUBS" value="CHERRY-MXNONUBS">
<attribute name="NAME"/>
</element>
<element name="SW3" library="A_butts" package="CHERRY-MX-NONUBS" value="CHERRY-MXNONUBS">
<attribute name="NAME"/>
</element>
<element name="SW4" library="A_butts" package="CHERRY-MX-NONUBS" value="CHERRY-MXNONUBS">
<attribute name="NAME"/>
</element>
<element name="SW5" library="A_butts" package="CHERRY-MX-NONUBS" value="CHERRY-MXNONUBS">
<attribute name="NAME"/>
</element>
<element name="SW6" library="A_butts" package="CHERRY-MX-NONUBS" value="CHERRY-MXNONUBS">
<attribute name="NAME"/>
</element>
<element name="D1" library="A_butts" package="DIODE-7.62MM" value="1N4148">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="A_butts" package="DIODE-7.62MM" value="1N4148">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="A_butts" package="DIODE-7.62MM" value="1N4148">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="A_butts" package="DIODE-7.62MM" value="1N4148">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D5" library="A_butts" package="DIODE-7.62MM" value="1N4148">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D6" library="A_butts" package="DIODE-7.62MM" value="1N4148">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VCC" library="A_butts" package="1X01" value="M01PTH"/>
<element name="SDA" library="A_butts" package="1X01" value="M01PTH"/>
<element name="SCL" library="A_butts" package="1X01" value="M01PTH"/>
<element name="GND" library="A_butts" package="1X01" value="M01PTH"/>
<element name="U1" library="A_butts" package="TEENSY_3.0_BASIC_ALT2" value="TEENSY_3.0_BASIC_ALTDIP"/>
<element name="C1" library="A_butts" package="C025-024X044" value="100n"/>
<element name="C2" library="A_butts" package="C025-024X044" value="100n"/>
<element name="U$1" library="A_butts" package="CC-BY-SA-4.0-URL-BOTTOM" value=""/>
<element name="U$3" library="A_butts" package="COW_SMALL_METAL" value=""/>
<element name="U$4" library="A_butts" package="OSHWLOGO_5MM_METAL" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="GND" pad="1"/>
<contactref element="U1" pad="GND"/>
<contactref element="U1" pad="GND"/>
<contactref element="D1" pad="K"/>
<contactref element="D2" pad="K"/>
<contactref element="D3" pad="K"/>
<contactref element="D4" pad="K"/>
<contactref element="D5" pad="K"/>
<contactref element="D6" pad="K"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="VCC" pad="1"/>
<contactref element="U1" pad="3.3V"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="SCL">
<contactref element="SCL" pad="1"/>
<contactref element="U1" pad="19/A5"/>
</signal>
<signal name="SDA">
<contactref element="SDA" pad="1"/>
<contactref element="U1" pad="18/A4"/>
</signal>
<signal name="VIN">
<contactref element="U1" pad="VIN"/>
</signal>
<signal name="AGND">
<contactref element="U1" pad="AGND"/>
</signal>
<signal name="N$1">
<contactref element="D1" pad="A"/>
<contactref element="SW1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="D2" pad="A"/>
<contactref element="SW2" pad="1"/>
</signal>
<signal name="KEY2">
<contactref element="SW2" pad="2"/>
<contactref element="U1" pad="9"/>
</signal>
<signal name="KEY1">
<contactref element="SW1" pad="2"/>
<contactref element="U1" pad="8"/>
</signal>
<signal name="N$3">
<contactref element="D3" pad="A"/>
<contactref element="SW3" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="D4" pad="A"/>
<contactref element="SW4" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="D5" pad="A"/>
<contactref element="SW5" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="D6" pad="A"/>
<contactref element="SW6" pad="1"/>
</signal>
<signal name="KEY3">
<contactref element="SW3" pad="2"/>
<contactref element="U1" pad="10"/>
</signal>
<signal name="KEY4">
<contactref element="SW4" pad="2"/>
<contactref element="U1" pad="11"/>
</signal>
<signal name="KEY5">
<contactref element="SW5" pad="2"/>
<contactref element="U1" pad="12"/>
</signal>
<signal name="KEY6">
<contactref element="SW6" pad="2"/>
<contactref element="U1" pad="13"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
