<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0.53" y1="9.26" x2="20.365" y2="9.26" width="0" layer="20"/>
<wire x1="20.365" y1="9.26" x2="20.365" y2="24.47" width="0" layer="20"/>
<wire x1="20.365" y1="24.47" x2="0.53" y2="24.45" width="0" layer="20"/>
<wire x1="0.53" y1="24.45" x2="0.53" y2="9.26" width="0" layer="20"/>
<text>EZ-I2C TINY BATTERY V2</text>
<text>VCC</text>
<text>BAT</text>
<text>EZ-I2C TINY BATTERY V2</text>
<text>GND</text>
<text>V+</text>
<text>V+</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>V+</text>
<text>V+</text>
<text>V+</text>
<text>V+</text>
</plain>
<libraries>
<library name="UniqueInteractionsLib">
<packages>
<package name="EZ-I2CHEADERV1">
</package>
<package name="BATTERY_1.25MM_PINHOLES">
</package>
<package name="JUMPER-3PAD">
</package>
</packages>
</library>
<library name="MiniWear_LOGO">
<packages>
<package name="LOGO2">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="UniqueInteractionsLib" package="EZ-I2CHEADERV1" value="EZ-I2CHEADERV1"/>
<element name="U$6" library="MiniWear_LOGO" package="LOGO2" value=""/>
<element name="U$2" library="MiniWear_LOGO" package="LOGO2" value=""/>
<element name="U$3" library="UniqueInteractionsLib" package="BATTERY_1.25MM_PINHOLES" value="BATTERY_1.25MM_PINHOLES">
<attribute name="NAME"/>
</element>
<element name="U$4" library="UniqueInteractionsLib" package="BATTERY_1.25MM_PINHOLES" value="BATTERY_1.25MM_PINHOLES">
<attribute name="NAME"/>
</element>
<element name="U$7" library="UniqueInteractionsLib" package="BATTERY_1.25MM_PINHOLES" value="BATTERY_1.25MM_PINHOLES">
<attribute name="NAME"/>
</element>
<element name="U$8" library="UniqueInteractionsLib" package="JUMPER-3PAD" value="JUMPER-3PAD"/>
<element name="U$9" library="UniqueInteractionsLib" package="BATTERY_1.25MM_PINHOLES" value="BATTERY_1.25MM_PINHOLES">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U$1" pad="GND"/>
<contactref element="U$1" pad="GND1"/>
<contactref element="U$3" pad="-"/>
<contactref element="U$4" pad="-"/>
<contactref element="U$7" pad="-"/>
<contactref element="U$9" pad="-"/>
</signal>
<signal name="SDA">
<contactref element="U$1" pad="SDA"/>
<contactref element="U$1" pad="SDA1"/>
</signal>
<signal name="SCL">
<contactref element="U$1" pad="SCL"/>
<contactref element="U$1" pad="SCL1"/>
</signal>
<signal name="VCC">
<contactref element="U$1" pad="VCC"/>
<contactref element="U$1" pad="VCC1"/>
<contactref element="U$8" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="LPOW"/>
<contactref element="U$1" pad="LPOW1"/>
</signal>
<signal name="BAT">
<contactref element="U$1" pad="BAT"/>
<contactref element="U$1" pad="BAT1"/>
<contactref element="U$8" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="U$3" pad="+"/>
<contactref element="U$4" pad="+"/>
<contactref element="U$7" pad="+"/>
<contactref element="U$8" pad="2"/>
<contactref element="U$9" pad="+"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
