<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="31.293" y2="0" width="0" layer="20"/>
<wire x1="31.293" y1="0" x2="31.293" y2="20.31" width="0" layer="20"/>
<wire x1="31.293" y1="20.31" x2="0" y2="20.31" width="0" layer="20"/>
<wire x1="0" y1="20.31" x2="0" y2="0" width="0" layer="20"/>
<text>3256</text>
<text>3160</text>
<text>IN
SNS
SRP
GND</text>
<text>12v</text>
<text>D</text>
<text>GND</text>
<text>BTS3256D
BTS3160D
Breakout</text>
</plain>
<libraries>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SCREWTERMINAL-3.5MM-3">
</package>
<package name="1X04_LONGPADS">
</package>
<package name="SJ_3">
</package>
</packages>
</library>
<library name="brandon">
<packages>
<package name="TO-252-5-13">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="SparkFun" package="SCREWTERMINAL-3.5MM-3" value="">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun" package="1X04_LONGPADS" value="">
<attribute name="VALUE"/>
</element>
<element name="SJ1" library="SparkFun" package="SJ_3" value="">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="brandon" package="TO-252-5-13" value="BTS3256D"/>
<element name="R1" library="adafruit" package="R0805" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$2">
<contactref element="SJ1" pad="3"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="SJ1" pad="2"/>
<contactref element="U$2" pad="4"/>
</signal>
<signal name="N$4">
<contactref element="U$2" pad="1"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="U$2" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="D">
<contactref element="U$2" pad="TAB"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="GND">
<contactref element="JP1" pad="3"/>
<contactref element="U$2" pad="5"/>
<contactref element="SJ1" pad="1"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="GND1">
</signal>
<signal name="GND2">
</signal>
<signal name="GND3">
</signal>
<signal name="N$1">
<contactref element="JP2" pad="3"/>
<contactref element="R1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
