<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="67.31" y2="0" width="0.2032" layer="20"/>
<wire x1="67.31" y1="0" x2="67.31" y2="49.53" width="0.2032" layer="20"/>
<wire x1="67.31" y1="49.53" x2="0" y2="49.53" width="0.2032" layer="20"/>
<wire x1="0" y1="49.53" x2="0" y2="0" width="0.2032" layer="20"/>
<text>GND</text>
<text>RSS</text>
<text>ASC</text>
<text>CTS</text>
<text>+5V</text>
<text>RX</text>
<text>TX</text>
<text>RTS</text>
<text>+5V</text>
<text>v1.1</text>
<text>J. Warnock</text>
<text>James'
XBee
Sensor
Node</text>
<hole x="3.81" y="29.21" drill="3.81"/>
<hole x="63.5" y="29.21" drill="3.81"/>
</plain>
<libraries>
<library name="SparkFun-RF">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find things that send or receive RF- GPS, cellular modules, Bluetooth, WiFi, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="XBEE-SMD">
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CREATIVE_COMMONS">
</package>
</packages>
</library>
<library name="james">
<packages>
<package name="SOT23">
</package>
<package name="SOIC-14">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="R3216">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="1X06">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-0603">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="RJ11-6">
</package>
<package name="POWER_JACK_SMD">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J4" library="SparkFun-RF" package="XBEE-SMD" value="XBEE-1B3">
<attribute name="PROD_ID" value="CONN-09042"/>
</element>
<element name="FRAME1" library="SparkFun-Aesthetics" package="CREATIVE_COMMONS" value="FRAME-LETTER"/>
<element name="U1" library="james" package="SOT23" value="MCP1700">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="1206" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="SparkFun-LED" package="LED-0603" value="RED">
<attribute name="PROD_ID" value="DIO-00819"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="SparkFun-LED" package="LED-0603" value="GREEN">
<attribute name="PROD_ID" value="DIO-00821"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="adafruit" package="R3216" value="200">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="adafruit" package="R3216" value="200">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="RJ11-6" value="RJ11-6PTH">
<attribute name="NAME"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="POWER_JACK_SMD" value="5.5x2.1mm Barrel">
<attribute name="PROD_ID" value="CONN-08106"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="1206" value=".1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="RJ11-6" value="RJ11-6PTH">
<attribute name="NAME"/>
</element>
<element name="J5" library="SparkFun-Connectors" package="RJ11-6" value="RJ11-6PTH">
<attribute name="NAME"/>
</element>
<element name="J6" library="SparkFun-Connectors" package="RJ11-6" value="RJ11-6PTH">
<attribute name="NAME"/>
</element>
<element name="JP1" library="adafruit" package="1X06" value=""/>
<element name="IC1" library="james" package="SOIC-14" value="74AHC125ND">
<attribute name="NAME"/>
</element>
<element name="R3" library="adafruit" package="R3216" value="10k"/>
<element name="R2" library="adafruit" package="R3216" value="1k"/>
<element name="C5" library="SparkFun-Capacitors" package="1206" value="8.2p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="1206" value="1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="1206" value="100u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$2">
<contactref element="D1" pad="C"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="GND">
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="J4" pad="10"/>
<contactref element="R4" pad="1"/>
<contactref element="J2" pad="6"/>
<contactref element="J2" pad="3"/>
<contactref element="U1" pad="1"/>
<contactref element="J1" pad="GND"/>
<contactref element="J1" pad="P$4"/>
<contactref element="C2" pad="2"/>
<contactref element="J3" pad="6"/>
<contactref element="J3" pad="3"/>
<contactref element="J5" pad="6"/>
<contactref element="J5" pad="3"/>
<contactref element="J6" pad="6"/>
<contactref element="J6" pad="3"/>
<contactref element="IC1" pad="1"/>
<contactref element="JP1" pad="6"/>
<contactref element="IC1" pad="4"/>
<contactref element="IC1" pad="7"/>
<contactref element="C1" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="J4" pad="15"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="N$4">
<contactref element="D2" pad="C"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="R3" pad="2"/>
<contactref element="J2" pad="1"/>
<contactref element="J2" pad="4"/>
<contactref element="U1" pad="2"/>
<contactref element="J3" pad="1"/>
<contactref element="J3" pad="4"/>
<contactref element="J5" pad="1"/>
<contactref element="J5" pad="4"/>
<contactref element="J6" pad="1"/>
<contactref element="J6" pad="4"/>
<contactref element="IC1" pad="14"/>
<contactref element="C1" pad="1"/>
<contactref element="J4" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="XBEE_DIO0">
<contactref element="J4" pad="20"/>
<contactref element="J2" pad="5"/>
</signal>
<signal name="XBEE_DIO2">
<contactref element="J4" pad="18"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="XBEE_DIO3">
<contactref element="J4" pad="17"/>
<contactref element="J3" pad="5"/>
</signal>
<signal name="XBEE_DIO1">
<contactref element="J4" pad="19"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="XBEE_DIO4">
<contactref element="J4" pad="11"/>
<contactref element="J5" pad="2"/>
</signal>
<signal name="XBEE_DIO12">
<contactref element="J4" pad="4"/>
<contactref element="J6" pad="5"/>
</signal>
<signal name="N$1">
<contactref element="J4" pad="6"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="XBEE_DIO11">
<contactref element="J4" pad="7"/>
<contactref element="J6" pad="2"/>
</signal>
<signal name="XBEE_DIO8">
<contactref element="J5" pad="5"/>
<contactref element="J4" pad="13"/>
</signal>
<signal name="RTS_5V">
<contactref element="JP1" pad="1"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="!RTS">
<contactref element="J4" pad="16"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="!CTS">
<contactref element="JP1" pad="5"/>
<contactref element="J4" pad="12"/>
</signal>
<signal name="RX_5V">
<contactref element="JP1" pad="3"/>
<contactref element="IC1" pad="5"/>
</signal>
<signal name="RX">
<contactref element="IC1" pad="6"/>
<contactref element="J4" pad="3"/>
</signal>
<signal name="TX">
<contactref element="JP1" pad="2"/>
<contactref element="J4" pad="2"/>
</signal>
<signal name="5V">
<contactref element="U1" pad="3"/>
<contactref element="J1" pad="VIN0"/>
<contactref element="C2" pad="1"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="!RESET">
<contactref element="J4" pad="5"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="J4" pad="9"/>
<contactref element="R2" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
