<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="39.37" x2="0" y2="2.54" width="0" layer="20"/>
<wire x1="0" y1="2.54" x2="2.54" y2="0" width="0" layer="20" curve="90"/>
<wire x1="2.54" y1="0" x2="85.09" y2="0" width="0" layer="20"/>
<wire x1="85.09" y1="0" x2="87.63" y2="2.54" width="0" layer="20" curve="90"/>
<wire x1="87.63" y1="2.54" x2="87.63" y2="39.37" width="0" layer="20"/>
<wire x1="87.63" y1="39.37" x2="85.09" y2="41.91" width="0" layer="20" curve="90"/>
<wire x1="85.09" y1="41.91" x2="2.54" y2="41.91" width="0" layer="20"/>
<wire x1="2.54" y1="41.91" x2="0" y2="39.37" width="0" layer="20" curve="90"/>
<hole x="3.81" y="3.81" drill="3.3"/>
<hole x="24.13" y="3.81" drill="3.3"/>
<hole x="3.81" y="38.1" drill="3.3"/>
<hole x="24.13" y="38.1" drill="3.3"/>
<hole x="83.82" y="38.1" drill="3.3"/>
<text>Trinket Keypad v1</text>
<text>Adafruit
Trinket M0</text>
<text>K00</text>
<text>K01</text>
<text>K02</text>
<text>K12</text>
<text>K11</text>
<text>K10</text>
<hole x="83.82" y="3.81" drill="3.3"/>
<text>CC BY-NC-SA 4.0
Rev 3. July 2020</text>
</plain>
<libraries>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DO35-7">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2 mm, horizontal, grid 7.62 mm</description>
</package>
</packages>
</library>
<library name="cherrymx">
<description>Cherry MX Keyswitch PCB footprints</description>
<packages>
<package name="CHERRY-MX">
<description>Cherry MX Keyswitch footprint</description>
</package>
</packages>
</library>
<library name="devboard_footprints">
<packages>
<package name="TRINKET-M0">
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Aesthetics&lt;/h3&gt;
This library contiains non-functional items such as logos, build/ordering notes, frame blocks, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-M">
<description>&lt;h3&gt;Open-Source Hardware (OSHW) Logo - Medium - Silkscreen&lt;/h3&gt;
&lt;p&gt;Silkscreen logo for open-source hardware designs.&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;OSHW_LOGO&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="D1" library="diode" package="DO35-7" value="1N4148DO35-7">
<attribute name="POPULARITY" value="58"/>
</element>
<element name="D2" library="diode" package="DO35-7" value="1N4148DO35-7">
<attribute name="POPULARITY" value="58"/>
</element>
<element name="D3" library="diode" package="DO35-7" value="1N4148DO35-7">
<attribute name="POPULARITY" value="58"/>
</element>
<element name="D4" library="diode" package="DO35-7" value="1N4148DO35-7">
<attribute name="POPULARITY" value="58"/>
</element>
<element name="D5" library="diode" package="DO35-7" value="1N4148DO35-7">
<attribute name="POPULARITY" value="58"/>
</element>
<element name="D6" library="diode" package="DO35-7" value="1N4148DO35-7">
<attribute name="POPULARITY" value="58"/>
</element>
<element name="K00" library="cherrymx" package="CHERRY-MX" value="CHERRY-MX"/>
<element name="K01" library="cherrymx" package="CHERRY-MX" value="CHERRY-MX"/>
<element name="K02" library="cherrymx" package="CHERRY-MX" value="CHERRY-MX"/>
<element name="K10" library="cherrymx" package="CHERRY-MX" value="CHERRY-MX"/>
<element name="K11" library="cherrymx" package="CHERRY-MX" value="CHERRY-MX"/>
<element name="K12" library="cherrymx" package="CHERRY-MX" value="CHERRY-MX"/>
<element name="TRINKETM0" library="devboard_footprints" package="TRINKET-M0" value="TRINKET-M0"/>
<element name="U$1" library="SparkFun-Aesthetics" package="OSHW-LOGO-M" value=""/>
</elements>
<signals>
<signal name="COL0">
<contactref element="K00" pad="SW1"/>
<contactref element="TRINKETM0" pad="0"/>
<contactref element="K10" pad="SW1"/>
</signal>
<signal name="N$2">
<contactref element="K00" pad="SW2"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="COL1">
<contactref element="K11" pad="SW1"/>
<contactref element="TRINKETM0" pad="1~"/>
<contactref element="K01" pad="SW1"/>
</signal>
<signal name="N$4">
<contactref element="K10" pad="SW2"/>
<contactref element="D4" pad="A"/>
</signal>
<signal name="N$6">
<contactref element="K11" pad="SW2"/>
<contactref element="D5" pad="A"/>
</signal>
<signal name="N$7">
<contactref element="K01" pad="SW2"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="N$10">
<contactref element="K02" pad="SW2"/>
<contactref element="D3" pad="A"/>
</signal>
<signal name="N$12">
<contactref element="K12" pad="SW2"/>
<contactref element="D6" pad="A"/>
</signal>
<signal name="ROW1">
<contactref element="D6" pad="C"/>
<contactref element="D4" pad="C"/>
<contactref element="D5" pad="C"/>
<contactref element="TRINKETM0" pad="3"/>
</signal>
<signal name="ROW0">
<contactref element="D1" pad="C"/>
<contactref element="D3" pad="C"/>
<contactref element="D2" pad="C"/>
<contactref element="TRINKETM0" pad="4"/>
</signal>
<signal name="GND">
<contactref element="TRINKETM0" pad="GND"/>
</signal>
<signal name="VCC">
<contactref element="TRINKETM0" pad="USB"/>
</signal>
<signal name="COL2">
<contactref element="TRINKETM0" pad="2"/>
<contactref element="K02" pad="SW1"/>
<contactref element="K12" pad="SW1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
