<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="15.5575" y2="0" width="0" layer="20"/>
<wire x1="15.5575" y1="0" x2="15.5575" y2="15.5575" width="0" layer="20"/>
<wire x1="15.5575" y1="15.5575" x2="0" y2="15.5575" width="0" layer="20"/>
<wire x1="0" y1="15.5575" x2="0" y2="0" width="0" layer="20"/>
<text>GND</text>
<text>VDD</text>
<text>VIO</text>
<text>SCL</text>
<text>SDA</text>
<text>SA0</text>
<text>CS</text>
<text>INT1</text>
<text>INT2</text>
<text>DSYNC</text>
<text>MCL</text>
<text>MDA</text>
<text>MAX21100</text>
<text>Technical
Toys
</text>
<hole x="10.16" y="2.38125" drill="2.8"/>
<hole x="5.3975" y="2.38125" drill="2.8"/>
<text>LED1</text>
<text>V3</text>
<text>1</text>
<text>0</text>
</plain>
<libraries>
<library name="max21100">
<packages>
<package name="MAX21100">
</package>
<package name="1X06">
</package>
<package name="SJ_2S-NO">
<description>Small solder jumper with no paste layer so it will open after reflow.</description>
</package>
<package name="SJ_2S-TRACE">
<description>Solder jumper, small, shorted with trace. No paste layer. Trace is cuttable.</description>
</package>
<package name="SJ_3">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="breakouts">
<packages>
<package name="CHIP-LED0603">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB Q993&lt;br&gt;
Source: http://www.osram.convergy.de/ ... Lb_q993.pdf</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="max21100" package="MAX21100" value="MAX21100"/>
<element name="JP1" library="max21100" package="1X06" value="JP1"/>
<element name="JP2" library="max21100" package="1X06" value="JP1"/>
<element name="C3" library="SparkFun-Passives" package="0603-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Passives" package="0603-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Passives" package="0603-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Passives" package="0603-RES" value="4K7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Passives" package="0603-RES" value="4K7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Passives" package="0603-RES" value="360R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="breakouts" package="CHIP-LED0603" value="RED"/>
<element name="VIO" library="max21100" package="SJ_2S-TRACE" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="I2C" library="max21100" package="SJ_2S-NO" value="SOLDERJUMPERNO">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SA0" library="max21100" package="SJ_3" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U$1" pad="5"/>
<contactref element="U$1" pad="10"/>
<contactref element="C3" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="LED1" pad="C"/>
<contactref element="JP2" pad="1"/>
<contactref element="SA0" pad="1"/>
</signal>
<signal name="VDD">
<contactref element="U$1" pad="14"/>
<contactref element="U$1" pad="15"/>
<contactref element="C2" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="JP1" pad="1"/>
<contactref element="VIO" pad="1"/>
</signal>
<signal name="VDDIO">
<contactref element="U$1" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="JP1" pad="2"/>
<contactref element="VIO" pad="2"/>
<contactref element="I2C" pad="1"/>
<contactref element="SA0" pad="3"/>
</signal>
<signal name="REGD">
<contactref element="U$1" pad="13"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="DSYNC">
<contactref element="U$1" pad="12"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="INT2">
<contactref element="U$1" pad="9"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="INT1">
<contactref element="U$1" pad="11"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="MST_SDA">
<contactref element="U$1" pad="3"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="MST_SCL">
<contactref element="U$1" pad="2"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="CS">
<contactref element="U$1" pad="8"/>
<contactref element="I2C" pad="2"/>
<contactref element="JP2" pad="6"/>
</signal>
<signal name="SA0_SDO">
<contactref element="U$1" pad="7"/>
<contactref element="SA0" pad="2"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="SDA_SDI">
<contactref element="U$1" pad="6"/>
<contactref element="R2" pad="1"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="N$1">
<contactref element="R3" pad="2"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="SCL_CLK">
<contactref element="JP1" pad="5"/>
<contactref element="U$1" pad="4"/>
<contactref element="R1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
