<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="-0.5" x2="38" y2="-0.5" width="0.2032" layer="20"/>
<wire x1="38" y1="-0.5" x2="38" y2="16.5" width="0" layer="20"/>
<wire x1="38" y1="16.5" x2="0" y2="16.5" width="0" layer="20"/>
<wire x1="0" y1="16.5" x2="0" y2="-0.5" width="0" layer="20"/>
<text>PIO0</text>
<text>PIO1</text>
<text>PIO2</text>
<text>PIO5</text>
<text>3V3</text>
<text>GND</text>
<text>MISO</text>
<text>MOSI</text>
<text>CLK</text>
<text>CS</text>
<text>3V3</text>
<text>GND</text>
<text>SPI/PCM</text>
<text>USBPOW</text>
<text>(C)2013 joost@damad.be</text>
<text>License: CC0</text>
<text>L1</text>
<text>PIOPOW</text>
<text>SPIPOW</text>
<text>v1</text>
</plain>
<libraries>
<library name="01jyd">
<description>more JYD stuff</description>
<packages>
<package name="BT111">
<description>Bluegiga BT111 bluetooth module
&lt;br/&gt;&lt;br/&gt;
Generated by 'madparts'.&lt;br/&gt;
Id: 445c062a047247098327493b7730f02a
</description>
</package>
<package name="SOT-23-6L">
<description>generic SOT-23-6L footprint
&lt;br/&gt;&lt;br/&gt;
Generated by 'madparts'.&lt;br/&gt;
Id: 28bc4baba8cf4350be1102f5bef6c1cf
 parent: 0094a06387e74d2f98a6fe8d01b761ae</description>
</package>
<package name="0603">
<description>Generic 0603 footprint
&lt;br/&gt;&lt;br/&gt;
Generated by 'madparts'.&lt;br/&gt;
Id: 10644a0b9a3a4f2a8a8b0add2ba7ce21
 parent: dc93599ddebd4bf8a02e4beef8a09b8b</description>
</package>
<package name="PIN_1X6_S">
<description>8 pin pinheader
&lt;br/&gt;&lt;br/&gt;
Generated by 'madparts'.&lt;br/&gt;
Id: 0ecb97821889480bbca498d3d59bebd2
 parent: c2bf9acdab414de7891c3f8d5c51767f</description>
</package>
<package name="BUTTON_ALPS_SMD_5.2MM_SKQG">
<description>
&lt;br/&gt;&lt;br/&gt;
Generated by 'madparts'.&lt;br/&gt;
Id: 69749eafd7584cada41b63ad6030d54d
 parent: 7db0a6816f5a4a5581e92cecab7d7e08</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="USB-A-H">
<description>&lt;b&gt;USB Series A Hole Mounted&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SJ_2S">
<description>Small solder jumper with big paste layer so it will short during reflow.</description>
</package>
<package name="SJ_2S-NO">
<description>Small solder jumper with no paste layer so it will open after reflow.</description>
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="CHIP-LED0805">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB R99A&lt;br&gt;
Source: http://www.osram.convergy.de/ ... lb_r99a.pdf</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U2" library="01jyd" package="BT111" value="BT111"/>
<element name="JP1" library="SparkFun-Connectors" package="USB-A-H" value="USB-A-H"/>
<element name="U1" library="01jyd" package="SOT-23-6L" value="">
<attribute name="VALUE"/>
</element>
<element name="R1" library="01jyd" package="0603" value="27">
<attribute name="NAME"/>
</element>
<element name="R2" library="01jyd" package="0603" value="27">
<attribute name="NAME"/>
</element>
<element name="JP3" library="01jyd" package="PIN_1X6_S" value="">
<attribute name="VALUE"/>
</element>
<element name="JP4" library="01jyd" package="PIN_1X6_S" value="">
<attribute name="VALUE"/>
</element>
<element name="R3" library="01jyd" package="0603" value="10k">
<attribute name="NAME"/>
</element>
<element name="B1" library="01jyd" package="BUTTON_ALPS_SMD_5.2MM_SKQG" value="">
<attribute name="VALUE"/>
</element>
<element name="R4" library="01jyd" package="0603" value="10k">
<attribute name="NAME"/>
</element>
<element name="SJ1" library="SparkFun-Passives" package="SJ_2S" value="USBPOW"/>
<element name="SJ2" library="SparkFun-Passives" package="SJ_2S-NO" value="SPIPOW"/>
<element name="SJ3" library="SparkFun-Passives" package="SJ_2S-NO" value="PIOPOW"/>
<element name="SJ4" library="SparkFun-Passives" package="SJ_2S-NO" value="PCMSEL"/>
<element name="R5" library="01jyd" package="0603" value="1k">
<attribute name="NAME"/>
</element>
<element name="LED1" library="led" package="CHIP-LED0805" value="red"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U2" pad="1"/>
<contactref element="U2" pad="21"/>
<contactref element="U2" pad="15"/>
<contactref element="U2" pad="9"/>
<contactref element="JP3" pad="6"/>
<contactref element="JP4" pad="6"/>
<contactref element="B1" pad="4"/>
<contactref element="JP1" pad="GND"/>
<contactref element="U1" pad="2"/>
<contactref element="LED1" pad="C"/>
</signal>
<signal name="VBUS1">
<contactref element="JP1" pad="VBUS"/>
<contactref element="U1" pad="5"/>
<contactref element="SJ1" pad="1"/>
</signal>
<signal name="USB+">
<contactref element="R1" pad="2"/>
<contactref element="U2" pad="3"/>
</signal>
<signal name="USB-">
<contactref element="R2" pad="2"/>
<contactref element="U2" pad="2"/>
</signal>
<signal name="VUSBINT">
<contactref element="U2" pad="17"/>
<contactref element="SJ1" pad="2"/>
</signal>
<signal name="MISO">
<contactref element="JP3" pad="1"/>
<contactref element="U2" pad="12"/>
</signal>
<signal name="MOSI">
<contactref element="U2" pad="8"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="CLK">
<contactref element="U2" pad="7"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="CS">
<contactref element="U2" pad="4"/>
<contactref element="JP3" pad="4"/>
</signal>
<signal name="PIO0">
<contactref element="U2" pad="11"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="PIO1">
<contactref element="U2" pad="13"/>
<contactref element="JP4" pad="2"/>
</signal>
<signal name="PIO2">
<contactref element="U2" pad="6"/>
<contactref element="JP4" pad="3"/>
</signal>
<signal name="PIO5">
<contactref element="U2" pad="5"/>
<contactref element="JP4" pad="4"/>
</signal>
<signal name="+3V3">
<contactref element="U2" pad="10"/>
<contactref element="U2" pad="16"/>
<contactref element="U2" pad="19"/>
<contactref element="R3" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="SJ2" pad="1"/>
<contactref element="SJ3" pad="2"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="JP3" pad="5"/>
<contactref element="SJ2" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="JP4" pad="5"/>
<contactref element="SJ3" pad="1"/>
</signal>
<signal name="SEL">
<contactref element="U2" pad="14"/>
<contactref element="SJ4" pad="2"/>
</signal>
<signal name="SEL2">
<contactref element="R3" pad="2"/>
<contactref element="SJ4" pad="1"/>
</signal>
<signal name="RST">
<contactref element="U2" pad="20"/>
<contactref element="B1" pad="2"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="JP1" pad="D-"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="N$10">
<contactref element="JP1" pad="D+"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="U1" pad="4"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="U1" pad="6"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="R5" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
