<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<text>Buspirate ISP Board for 3.x</text>
<text>3.3/5.0</text>
<text>MOSI</text>
<text>GND</text>
<text>MISO</text>
<text>CLK</text>
<text>RST</text>
<text>VCC</text>
<text>MOSI/TX</text>
<text>GRND</text>
<text>3.3v</text>
<text>5.0v</text>
<text>ADC</text>
<text>VPU</text>
<text>AUX</text>
<text>CLK/SCL</text>
<text>CS/TMS</text>
<text>MISO/RX</text>
<text>GRND</text>
<text>OWD</text>
<text>VCC</text>
<text>SDA</text>
<text>VCC</text>
<text>SLC</text>
<text>GRND</text>
<wire x1="2.032" y1="7.874" x2="2.032" y2="8.128" width="0.4064" layer="20"/>
<text>By Erll</text>
<text>ISP-10</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X5-SHROUDED">
</package>
<package name="1X03">
</package>
<package name="2X3">
</package>
<package name="1X06">
</package>
<package name="1X10">
</package>
<package name="1X04">
</package>
<package name="1X02">
</package>
</packages>
</library>
<library name="Buspirate">
<packages>
<package name="2X5-SHROUDED_LOCK">
</package>
</packages>
</library>
<library name="dp_pcb">
<packages>
<package name="DP6037_V1">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="ISP_10_PIN" library="SparkFun-Connectors" package="2X5-SHROUDED" value="ISP_10"/>
<element name="POWER" library="SparkFun-Connectors" package="1X03" value=""/>
<element name="ISP-6" library="SparkFun-Connectors" package="2X3" value=""/>
<element name="BUSPIRATE" library="Buspirate" package="2X5-SHROUDED_LOCK" value=""/>
<element name="1" library="SparkFun-Connectors" package="1X06" value=""/>
<element name="BUSPIRATE_BREAKOUT" library="SparkFun-Connectors" package="1X10" value=""/>
<element name="I2C" library="SparkFun-Connectors" package="1X04" value=""/>
<element name="1WIRE" library="SparkFun-Connectors" package="1X03" value=""/>
<element name="VCC/GND" library="SparkFun-Connectors" package="1X02" value=""/>
<element name="E$1" library="dp_pcb" package="DP6037_V1" value=""/>
</elements>
<signals>
<signal name="N$2">
<contactref element="ISP_10_PIN" pad="1"/>
<contactref element="ISP-6" pad="4"/>
<contactref element="BUSPIRATE" pad="8"/>
<contactref element="1" pad="1"/>
<contactref element="BUSPIRATE_BREAKOUT" pad="8"/>
<contactref element="1WIRE" pad="2"/>
<contactref element="I2C" pad="4"/>
</signal>
<signal name="N$3">
<contactref element="ISP_10_PIN" pad="5"/>
<contactref element="ISP-6" pad="5"/>
<contactref element="BUSPIRATE" pad="9"/>
<contactref element="1" pad="5"/>
<contactref element="BUSPIRATE_BREAKOUT" pad="9"/>
</signal>
<signal name="N$5">
<contactref element="ISP_10_PIN" pad="7"/>
<contactref element="ISP-6" pad="3"/>
<contactref element="BUSPIRATE" pad="7"/>
<contactref element="1" pad="4"/>
<contactref element="I2C" pad="3"/>
<contactref element="BUSPIRATE_BREAKOUT" pad="7"/>
</signal>
<signal name="N$7">
<contactref element="ISP_10_PIN" pad="9"/>
<contactref element="ISP-6" pad="1"/>
<contactref element="1" pad="3"/>
</signal>
<signal name="N$8">
<contactref element="ISP_10_PIN" pad="2"/>
<contactref element="ISP-6" pad="2"/>
<contactref element="POWER" pad="2"/>
<contactref element="1" pad="6"/>
<contactref element="VCC/GND" pad="1"/>
<contactref element="I2C" pad="2"/>
<contactref element="1WIRE" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="BUSPIRATE" pad="3"/>
<contactref element="POWER" pad="1"/>
<contactref element="BUSPIRATE_BREAKOUT" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="BUSPIRATE" pad="2"/>
<contactref element="POWER" pad="3"/>
<contactref element="BUSPIRATE_BREAKOUT" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="BUSPIRATE" pad="4"/>
<contactref element="BUSPIRATE_BREAKOUT" pad="4"/>
</signal>
<signal name="N$11">
<contactref element="BUSPIRATE" pad="6"/>
<contactref element="BUSPIRATE_BREAKOUT" pad="6"/>
</signal>
<signal name="N$9">
<contactref element="ISP_10_PIN" pad="10"/>
<contactref element="ISP_10_PIN" pad="8"/>
<contactref element="ISP_10_PIN" pad="6"/>
<contactref element="ISP_10_PIN" pad="4"/>
<contactref element="ISP-6" pad="6"/>
<contactref element="1" pad="2"/>
<contactref element="BUSPIRATE" pad="1"/>
<contactref element="VCC/GND" pad="2"/>
<contactref element="1WIRE" pad="1"/>
<contactref element="BUSPIRATE_BREAKOUT" pad="1"/>
<contactref element="I2C" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="BUSPIRATE" pad="5"/>
<contactref element="BUSPIRATE_BREAKOUT" pad="5"/>
</signal>
<signal name="N$12">
<contactref element="BUSPIRATE" pad="10"/>
<contactref element="BUSPIRATE_BREAKOUT" pad="10"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
