<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<text>NEOGEO Controller Board</text>
<text>v1.0</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>6</text>
<text>7</text>
<text>8</text>
<text>9</text>
<text>10</text>
<text>11</text>
<text>12</text>
<text>13</text>
<text>14</text>
<text>15</text>
<text>GND</text>
<text>UP</text>
<text>DOWN</text>
<text>LEFT</text>
<text>RIGHT</text>
<text>A</text>
<text>B</text>
<text>C</text>
<text>D</text>
<text>SELECT</text>
<text>START</text>
<text>+5V</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<wire x1="2" y1="26" x2="0" y2="24" width="0" layer="20" curve="90"/>
<wire x1="0" y1="2" x2="2" y2="0" width="0" layer="20" curve="90"/>
<wire x1="98.5" y1="2" x2="96.5" y2="0" width="0" layer="20" curve="-90"/>
<wire x1="98.5" y1="24" x2="96.5" y2="26" width="0" layer="20" curve="90"/>
<wire x1="98.5" y1="2" x2="98.5" y2="24" width="0" layer="20"/>
<wire x1="96.5" y1="26" x2="2" y2="26" width="0" layer="20"/>
<wire x1="0" y1="24" x2="0" y2="2" width="0" layer="20"/>
<wire x1="2" y1="0" x2="96.5" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED_5MM">
<description>&lt;B&gt;LED 5mm PTH&lt;/B&gt;&lt;p&gt;
5 mm, round
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1inch&lt;/li&gt;
&lt;li&gt;Diameter: 5mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED-IR-THRU&lt;/li&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
</package>
</packages>
</library>
<library name="#mine">
<packages>
<package name="COMBICON_PT_2">
<description>Footprint for a Phoenix Contact Combicon PT series 2 pin terminal block.</description>
</package>
<package name="COMBICON_PT_15">
<description>Footprint for a Phoenix Contact Combicon PT series 15 pin terminal block.</description>
</package>
<package name="COMBICON_PT_5">
<description>Footprint for a Phoenix Contact Combicon PT series 5 pin terminal block.</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="LED" library="SparkFun-LED" package="LED_5MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Passives" package="AXIAL-0.3" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TB_5V" library="#mine" package="COMBICON_PT_2" value="COMBICON_PT_2SIL">
<attribute name="NAME"/>
</element>
<element name="TB_A" library="#mine" package="COMBICON_PT_2" value="COMBICON_PT_2SIL">
<attribute name="NAME"/>
</element>
<element name="TB_B" library="#mine" package="COMBICON_PT_2" value="COMBICON_PT_2SIL">
<attribute name="NAME"/>
</element>
<element name="TB_C" library="#mine" package="COMBICON_PT_2" value="COMBICON_PT_2SIL">
<attribute name="NAME"/>
</element>
<element name="TB_D" library="#mine" package="COMBICON_PT_2" value="COMBICON_PT_2SIL">
<attribute name="NAME"/>
</element>
<element name="TB_DB15" library="#mine" package="COMBICON_PT_15" value="COMBICON_PT_15SIL">
<attribute name="NAME"/>
</element>
<element name="TB_JOYSTICK" library="#mine" package="COMBICON_PT_5" value="COMBICON_PT_5SIL">
<attribute name="NAME"/>
</element>
<element name="TB_SELECT" library="#mine" package="COMBICON_PT_2" value="COMBICON_PT_2SIL">
<attribute name="NAME"/>
</element>
<element name="TB_START" library="#mine" package="COMBICON_PT_2" value="COMBICON_PT_2SIL">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="TB_DB15" pad="1"/>
<contactref element="TB_A" pad="2"/>
<contactref element="TB_B" pad="2"/>
<contactref element="TB_C" pad="2"/>
<contactref element="TB_D" pad="2"/>
<contactref element="TB_START" pad="2"/>
<contactref element="TB_SELECT" pad="2"/>
<contactref element="TB_5V" pad="2"/>
<contactref element="LED" pad="K"/>
<contactref element="TB_JOYSTICK" pad="5"/>
</signal>
<signal name="N$2">
<contactref element="R1" pad="P$2"/>
<contactref element="LED" pad="A"/>
</signal>
<signal name="N$3">
<contactref element="TB_DB15" pad="3"/>
<contactref element="TB_SELECT" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="TB_DB15" pad="4"/>
<contactref element="TB_D" pad="1"/>
<contactref element="TB_DB15" pad="9"/>
</signal>
<signal name="N$5">
<contactref element="TB_DB15" pad="5"/>
<contactref element="TB_B" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="TB_DB15" pad="8"/>
<contactref element="R1" pad="P$1"/>
<contactref element="TB_5V" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="TB_DB15" pad="11"/>
<contactref element="TB_START" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="TB_C" pad="1"/>
<contactref element="TB_DB15" pad="12"/>
</signal>
<signal name="N$9">
<contactref element="TB_DB15" pad="13"/>
<contactref element="TB_A" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="TB_JOYSTICK" pad="4"/>
<contactref element="TB_DB15" pad="14"/>
</signal>
<signal name="N$11">
<contactref element="TB_JOYSTICK" pad="3"/>
<contactref element="TB_DB15" pad="6"/>
</signal>
<signal name="N$12">
<contactref element="TB_JOYSTICK" pad="2"/>
<contactref element="TB_DB15" pad="7"/>
</signal>
<signal name="N$13">
<contactref element="TB_JOYSTICK" pad="1"/>
<contactref element="TB_DB15" pad="15"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
