<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="17.78" y2="0" width="0" layer="20"/>
<wire x1="17.78" y1="0" x2="17.78" y2="14.224" width="0" layer="20"/>
<wire x1="17.78" y1="14.224" x2="0" y2="14.224" width="0" layer="20"/>
<wire x1="0" y1="14.224" x2="0" y2="0" width="0" layer="20"/>
<text>VDD</text>
<text>VDDp</text>
<text>GND</text>
<text>SWa</text>
<text>SWb</text>
<text>Addr</text>
<text>INT</text>
<text>RST</text>
<text>SCL</text>
<text>SDA</text>
<text>1</text>
<text>0</text>
<text>Easy Point</text>
<text>N40P107</text>
<text>AS5013</text>
</plain>
<libraries>
<library name="EasyPoint">
<packages>
<package name="N40P107">
</package>
<package name="AS5013">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
<package name="SJ_3">
</package>
<package name="0402-RES">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X05">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JS2" library="EasyPoint" package="N40P107" value="N40P107">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="EasyPoint" package="AS5013" value="AS5013">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Passives" package="0603-CAP" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Passives" package="0603-CAP" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Passives" package="SJ_3" value="JUMPER-3SMD">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Passives" package="0402-RES" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Passives" package="0402-RES" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Passives" package="0402-RES" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X05" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="SparkFun-Connectors" package="1X05" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="VDD">
<contactref element="U1" pad="12"/>
<contactref element="C2" pad="1"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="VPP">
<contactref element="U1" pad="11"/>
<contactref element="C1" pad="1"/>
<contactref element="JP1" pad="3"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="13"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="JP1" pad="1"/>
<contactref element="JS2" pad="1"/>
<contactref element="JS2" pad="4"/>
<contactref element="JS2" pad="5"/>
<contactref element="JS2" pad="8"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="RESET">
<contactref element="U1" pad="3"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="ADDR">
<contactref element="U1" pad="10"/>
<contactref element="JP1" pad="2"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="SW_B">
<contactref element="JS2" pad="3"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="SDA">
<contactref element="U1" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="JP3" pad="5"/>
</signal>
<signal name="SCL">
<contactref element="R2" pad="1"/>
<contactref element="U1" pad="2"/>
<contactref element="JP3" pad="4"/>
</signal>
<signal name="INT">
<contactref element="U1" pad="4"/>
<contactref element="R3" pad="1"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="SW_A">
<contactref element="JS2" pad="2"/>
<contactref element="JP2" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
