<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.1.3">
<drawing>
<board>
<plain>
<wire x1="0" y1="44.45" x2="0" y2="13.97" width="0" layer="20"/>
<wire x1="0" y1="13.97" x2="1.27" y2="12.7" width="0" layer="20" curve="90"/>
<wire x1="1.27" y1="12.7" x2="67.29" y2="12.7" width="0" layer="20"/>
<wire x1="67.29" y1="12.7" x2="68.56" y2="13.97" width="0" layer="20" curve="90"/>
<wire x1="68.56" y1="13.97" x2="68.56" y2="44.45" width="0" layer="20"/>
<wire x1="68.56" y1="44.45" x2="67.62" y2="45.39" width="0" layer="20" curve="90"/>
<wire x1="67.62" y1="45.39" x2="0.94" y2="45.39" width="0" layer="20"/>
<wire x1="0.94" y1="45.39" x2="0" y2="44.45" width="0" layer="20" curve="90"/>
<text>RS-232 Hard Tap
w/ Probe Points
Phantomic Labs, 2018</text>
<text>(DB-9 Female)</text>
<text>(DB-9 Female)</text>
<text>(DB-9 Male)</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DB9">
<description>&lt;h3&gt;9 Pin Serial Connector - Female PCB Mount Right Angle&lt;/h3&gt;
0.318" style. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:11&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Connectors/DB9-PCB.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;DB9&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="DB9_MALE">
<description>&lt;h3&gt;9 Pin Serial Connector - Male PCB Mount Right Angle&lt;/h3&gt;
0.318" style. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:11&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://www.4uconnector.com/online/object/4udrawing/15944.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;DB9&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X08_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole -8 Pin No Silk&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:8&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_08&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Switches">
<description>&lt;h3&gt;SparkFun Switches, Buttons, Encoders&lt;/h3&gt;
In this library you'll find switches, buttons, joysticks, and anything that moves to create or disrupt an electrical connection.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DIPSWITCH-08">
<description>&lt;h3&gt;8-Position DIP Switch - PTH, 0.1"-Pitch&lt;/h3&gt;
&lt;p&gt;Standard size through-hole DIP switch, 2.54 mm / 0.1" pitch&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.sparkfun.com/datasheets/Components/Switch-DIP8.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Connectors" package="DB9" value="DUT">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08194"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="DB9_MALE" value="PC">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-09904"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="DB9" value="TAP0">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08194"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="SparkFun-Switches" package="DIPSWITCH-08" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="SWCH-12197"/>
<attribute name="SF_SKU" value="COM-08034"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="1X08_NO_SILK" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08438"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="CD_DUT">
<contactref element="J1" pad="1"/>
<contactref element="S1" pad="9"/>
<contactref element="J4" pad="1"/>
</signal>
<signal name="RX_DUT">
<contactref element="J1" pad="2"/>
<contactref element="S1" pad="10"/>
<contactref element="J4" pad="2"/>
</signal>
<signal name="TX_DUT">
<contactref element="J1" pad="3"/>
<contactref element="S1" pad="11"/>
<contactref element="J4" pad="3"/>
</signal>
<signal name="DTR_DUT">
<contactref element="J1" pad="4"/>
<contactref element="S1" pad="12"/>
<contactref element="J4" pad="4"/>
</signal>
<signal name="DST_DUT">
<contactref element="J1" pad="6"/>
<contactref element="S1" pad="13"/>
<contactref element="J4" pad="5"/>
</signal>
<signal name="RTS_DUT">
<contactref element="J1" pad="7"/>
<contactref element="S1" pad="14"/>
<contactref element="J4" pad="6"/>
</signal>
<signal name="CTS_DUT">
<contactref element="J1" pad="8"/>
<contactref element="S1" pad="15"/>
<contactref element="J4" pad="7"/>
</signal>
<signal name="RI_DUT">
<contactref element="J1" pad="9"/>
<contactref element="S1" pad="16"/>
<contactref element="J4" pad="8"/>
</signal>
<signal name="CD_PC">
<contactref element="J2" pad="1"/>
<contactref element="S1" pad="8"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="RX_PC">
<contactref element="J2" pad="2"/>
<contactref element="S1" pad="7"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="TX_PC">
<contactref element="J2" pad="3"/>
<contactref element="S1" pad="6"/>
<contactref element="J3" pad="3"/>
</signal>
<signal name="DTR_PC">
<contactref element="J2" pad="4"/>
<contactref element="S1" pad="5"/>
<contactref element="J3" pad="4"/>
</signal>
<signal name="DST_PC">
<contactref element="J2" pad="6"/>
<contactref element="S1" pad="4"/>
<contactref element="J3" pad="6"/>
</signal>
<signal name="RTS_PC">
<contactref element="J2" pad="7"/>
<contactref element="S1" pad="3"/>
<contactref element="J3" pad="7"/>
</signal>
<signal name="CTS_PC">
<contactref element="J2" pad="8"/>
<contactref element="S1" pad="2"/>
<contactref element="J3" pad="8"/>
</signal>
<signal name="RI_PC">
<contactref element="J2" pad="9"/>
<contactref element="S1" pad="1"/>
<contactref element="J3" pad="9"/>
</signal>
<signal name="GND">
<contactref element="J1" pad="5"/>
<contactref element="J2" pad="5"/>
<contactref element="J3" pad="5"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
