<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="30.48" y2="0" width="0" layer="20"/>
<wire x1="30.48" y1="0" x2="30.48" y2="51.816" width="0" layer="20"/>
<wire x1="30.48" y1="51.816" x2="0" y2="51.816" width="0" layer="20"/>
<wire x1="0" y1="51.816" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="butts">
<packages>
<package name="E5-10,5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 5.08 mm, diameter 10.5 mm</description>
</package>
<package name="RADIAL-PTH-508-BY-8.7DIA">
</package>
<package name="C025-024X044">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 2.4 x 4.4 mm</description>
</package>
<package name="AXIAL-PTH-5.08MM">
</package>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
<package name="SH22,5">
<description>&lt;b&gt;FUSE HOLDER&lt;/b&gt;&lt;p&gt; grid 22,5 mm, OGN0031 8201 Schurter (Buerklin)</description>
</package>
<package name="COW_SMALL">
</package>
<package name="2,8">
<description>&lt;b&gt;MOUNTING HOLE&lt;/b&gt; 2.8 mm with drill center</description>
</package>
</packages>
</library>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="PTC">
</package>
<package name="DIP-08">
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DO41-7.6">
<description>&lt;b&gt;DO41&lt;/b&gt; 7.6mm x 2mm&lt;p&gt;
Source: http://www.diodes.com/datasheets/ds23001.pdf</description>
</package>
</packages>
</library>
<library name="rectifier">
<description>&lt;b&gt;Rectifiers&lt;/b&gt;&lt;p&gt;
General Instrument, Semikron, Diotec, Fagor&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="RB1A">
<description>&lt;b&gt;RECTIFIER&lt;/b&gt;&lt;p&gt;
1 A</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="JST-2-PTH">
</package>
</packages>
</library>
<library name="A_butts">
<packages>
<package name="OSHWLOGO_BOT_0.2_A">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="butts" package="E5-10,5" value="150uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="butts" package="RADIAL-PTH-508-BY-8.7DIA" value="100uH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="butts" package="E5-10,5" value="150uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="F2" library="SparkFun-PowerIC" package="PTC" value="PTC">
<attribute name="VALUE"/>
</element>
<element name="D1" library="diode" package="DO41-7.6" value="1N5819">
<attribute name="VALUE"/>
</element>
<element name="B1" library="rectifier" package="RB1A" value="RECTIFIER-RB1A">
<attribute name="NAME"/>
</element>
<element name="C3" library="butts" package="C025-024X044" value="220pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="SparkFun-PowerIC" package="DIP-08" value="MC34063DIP">
<attribute name="VALUE"/>
</element>
<element name="R3" library="butts" package="AXIAL-PTH-5.08MM" value="0.33R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="butts" package="AXIAL-PTH-5.08MM" value="100R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="butts" package="AXIAL-PTH-5.08MM" value="300R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="INPUT" library="SparkFun-Connectors" package="JST-2-PTH" value="M02JST-PTH-2">
<attribute name="NAME"/>
<attribute name="SKU" value="PRT-09914"/>
</element>
<element name="OUTPUT" library="SparkFun-Connectors" package="JST-2-PTH" value="M02JST-PTH-2">
<attribute name="NAME"/>
<attribute name="SKU" value="PRT-09914"/>
</element>
<element name="F1" library="butts" package="SH22,5" value="5A">
<attribute name="OC_NEWARK" value="96F8317"/>
<attribute name="MPN" value="0031.8201"/>
<attribute name="MF" value="SCHURTER"/>
<attribute name="OC_FARNELL" value="1162740"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="butts" package="AXIAL-PTH-5.08MM" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED1" library="butts" package="LED3MM" value="LED3MM"/>
<element name="U$1" library="butts" package="COW_SMALL" value=""/>
<element name="H1" library="butts" package="2,8" value="MOUNT-HOLE2.8"/>
<element name="H2" library="butts" package="2,8" value="MOUNT-HOLE2.8"/>
<element name="H3" library="butts" package="2,8" value="MOUNT-HOLE2.8"/>
<element name="H4" library="butts" package="2,8" value="MOUNT-HOLE2.8"/>
<element name="U$2" library="A_butts" package="OSHWLOGO_BOT_0.2_A" value=""/>
</elements>
<signals>
<signal name="24VAC+">
<contactref element="B1" pad="AC2"/>
<contactref element="F1" pad="2"/>
</signal>
<signal name="24VAC-">
<contactref element="B1" pad="AC1"/>
<contactref element="INPUT" pad="1"/>
</signal>
<signal name="GND">
<contactref element="B1" pad="-"/>
<contactref element="C1" pad="-"/>
<contactref element="C2" pad="-"/>
<contactref element="C3" pad="2"/>
<contactref element="U2" pad="4"/>
<contactref element="D1" pad="A"/>
<contactref element="R1" pad="P$2"/>
<contactref element="LED1" pad="K"/>
<contactref element="OUTPUT" pad="1"/>
</signal>
<signal name="5V">
<contactref element="L1" pad="P$2"/>
<contactref element="C2" pad="+"/>
<contactref element="R2" pad="P$1"/>
<contactref element="R4" pad="P$1"/>
<contactref element="OUTPUT" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="L1" pad="P$1"/>
<contactref element="D1" pad="C"/>
<contactref element="U2" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="B1" pad="+"/>
<contactref element="F2" pad="P$1"/>
</signal>
<signal name="VIN">
<contactref element="F2" pad="P$2"/>
<contactref element="C1" pad="+"/>
<contactref element="U2" pad="6"/>
<contactref element="R3" pad="P$2"/>
</signal>
<signal name="N$4">
<contactref element="U2" pad="7"/>
<contactref element="U2" pad="8"/>
<contactref element="U2" pad="1"/>
<contactref element="R3" pad="P$1"/>
</signal>
<signal name="N$9">
<contactref element="U2" pad="3"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="R1" pad="P$1"/>
<contactref element="U2" pad="5"/>
<contactref element="R2" pad="P$2"/>
</signal>
<signal name="N$5">
<contactref element="LED1" pad="A"/>
<contactref element="R4" pad="P$2"/>
</signal>
<signal name="N$1">
<contactref element="INPUT" pad="2"/>
<contactref element="F1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
