<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="26.67" y1="1" x2="26.67" y2="10.303" width="0" layer="20"/>
<wire x1="26.67" y1="10.303" x2="25.67" y2="11.303" width="0" layer="20" curve="90"/>
<wire x1="25.67" y1="11.303" x2="1" y2="11.303" width="0" layer="20"/>
<wire x1="1" y1="11.303" x2="0" y2="10.303" width="0" layer="20" curve="90"/>
<wire x1="0" y1="10.303" x2="0" y2="1" width="0" layer="20"/>
<wire x1="0" y1="1" x2="1" y2="0" width="0" layer="20" curve="90"/>
<wire x1="1" y1="0" x2="25.67" y2="0" width="0" layer="20"/>
<wire x1="25.67" y1="0" x2="26.67" y2="1" width="0" layer="20" curve="90"/>
<text>Implant 5.1</text>
<text>C</text>
<text>C</text>
</plain>
<libraries>
<library name="Andy-library">
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="Cerebro-library">
<packages>
<package name="USB_VERT_MICRO_SMD">
</package>
<package name="LASERDIODE_3.8">
</package>
<package name="PHOTO_PACK">
<description>&lt;h3&gt;Plated Through Hole - No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R2" library="Andy-library" package="0805" value="20k">
<attribute name="VALUE"/>
</element>
<element name="U$2" library="Cerebro-library" package="USB_VERT_MICRO_SMD" value="USB_MICRO_SOCKET_VERT"/>
<element name="R1" library="Andy-library" package="0805" value="20k">
<attribute name="VALUE"/>
</element>
<element name="U$4" library="Cerebro-library" package="LASERDIODE_3.8" value="LASERDIODE3.8MM"/>
<element name="U$1" library="Cerebro-library" package="LASERDIODE_3.8" value="LASERDIODE3.8MM"/>
<element name="U$3" library="Cerebro-library" package="PHOTO_PACK" value="AMBIENT-LIGHT-SENSOR"/>
<element name="U$5" library="Cerebro-library" package="PHOTO_PACK" value="AMBIENT-LIGHT-SENSOR"/>
<element name="J1" library="SparkFun-Connectors" package="1X02" value="">
<attribute name="VALUE"/>
</element>
<element name="R3" library="Andy-library" package="0805" value="20k">
<attribute name="VALUE"/>
</element>
<element name="R4" library="Andy-library" package="0805" value="20k">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="L2_CATHODE">
<contactref element="U$2" pad="P5"/>
<contactref element="U$4" pad="3"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="LD_VOLTAGE">
<contactref element="J1" pad="2"/>
<contactref element="U$4" pad="1"/>
<contactref element="U$1" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="HEATSINK">
<contactref element="U$4" pad="2"/>
</signal>
<signal name="3.3VDC">
<contactref element="U$3" pad="COLLECTOR"/>
<contactref element="U$5" pad="COLLECTOR"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="FB1">
<contactref element="U$3" pad="EMITTER"/>
<contactref element="R2" pad="2"/>
<contactref element="U$2" pad="P2"/>
</signal>
<signal name="FB2">
<contactref element="U$5" pad="EMITTER"/>
<contactref element="R1" pad="2"/>
<contactref element="U$2" pad="P4"/>
</signal>
<signal name="GND">
<contactref element="R2" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="U$2" pad="P$1"/>
<contactref element="U$2" pad="P$2"/>
<contactref element="U$2" pad="P$3"/>
</signal>
<signal name="L1_CATHODE">
<contactref element="U$2" pad="P1"/>
<contactref element="U$1" pad="3"/>
<contactref element="R4" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
