<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<text>miniBCS J005904revM</text>
<text>OUTPUT</text>
<text>MM/SEC</text>
<text>1V = 100</text>
<text>9V DC </text>
<text>USB</text>
<text>20240507</text>
<wire x1="0" y1="0" x2="146.05" y2="0" width="0" layer="20"/>
<wire x1="146.05" y1="0" x2="146.05" y2="146.05" width="0" layer="20"/>
<wire x1="146.05" y1="146.05" x2="0" y2="146.05" width="0" layer="20"/>
<wire x1="0" y1="146.05" x2="0" y2="0" width="0" layer="20"/>
<text>GND</text>
<text>GND</text>
<text>+V</text>
<text>DRIVERS</text>
<text>1/5</text>
<text>2/6</text>
<text>3/7</text>
<text>4/8</text>
<text>ENCODER</text>
<text>B</text>
<text>A</text>
<text>IDX</text>
<text>GND</text>
<text>+5V</text>
<text>P2</text>
<text>+V</text>
<text>P3</text>
<text>GND</text>
<text>P4</text>
<text>+V</text>
<text>P5</text>
<text>GND</text>
<text>P6</text>
<text>+V</text>
<text>P7</text>
<text>GND</text>
<text>P8</text>
<text>+V</text>
<text>P9</text>
<text>RS232 1</text>
<text>RS232 2</text>
<text>RS232 3</text>
<text>ENCODER</text>
<text>A</text>
<text>B</text>
<text>IDX</text>
<text>GND</text>
<text>+5V</text>
<text>SOLENOIDS</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>SOLENOID
POWER
5-30VDC</text>
<text>PC USB</text>
<text> USB 
POWER</text>
<text>CAN BUS</text>
<text>TEMPERATURE 1</text>
<text>TEMPERATURE 2</text>
<text>SYNC IN</text>
<text>SYNC OUT</text>
<text>SPEED OUT</text>
<text>ANALOG IN 1</text>
<text>LED BEAM 
BREAK 1</text>
<text>LED BEAM 
BREAK 2</text>
<text>LASER OUT</text>
<text>CAMERA
SYNC OUT</text>
<text>GATE 1 </text>
<text>GATE 2</text>
<text>START</text>
<text>STOP</text>
<text>MiniBCS</text>
<text>H</text>
<text>L</text>
<text>TX2</text>
<text>IO7</text>
<text>RX2</text>
<text>IO8</text>
<text>RS232 1</text>
<text>RS232 2  
PIN 7&amp;8</text>
<text>RS232 3 

</text>
<text>SERIAL 2
ALTERNATES</text>
<text>S</text>
<text>S</text>
<text>MAX11300 </text>
<text>Driver</text>
<text>RS232 Serial</text>
<text>33</text>
<text>34</text>
<text>41/
A17</text>
<text>20/
A6</text>
<text>8</text>
<text>7</text>
<text>G</text>
<text>+</text>
<text>G</text>
<text>+</text>
<text>10</text>
<text>8</text>
<text>G</text>
<text>78L12</text>
<text>79L12</text>
<text>5R0</text>
<text>+/-12V Power</text>
<text>+12VA</text>
<text>-12VA</text>
<text>GND</text>
<text>ISO1H815G</text>
<text>ADM3312/5</text>
<text>TEENSY 4.1</text>
<text>AUX 5V POWER</text>
<text>TOP-TONE
BOT-40/A16</text>
<text>ISL23425</text>
<text>AD9833</text>
<text>ADA4084</text>
<text>M1A</text>
<text>M1B</text>
<text>DRIVER
POWER
11-35V</text>
<text>SJ1</text>
<text>G</text>
<text>+V</text>
<text>8</text>
<text>9</text>
<text>+</text>
<text>G</text>
<text>6</text>
<text>7</text>
<text>+</text>
<text>G</text>
<text>4</text>
<text>5</text>
<text>+</text>
<text>G</text>
<text>2</text>
<text>3</text>
<text>+</text>
<text>G</text>
<text>0</text>
<text>1</text>
<text>+</text>
<text>G</text>
<text>41/
A17</text>
<text>20/
A6</text>
<text>+</text>
<text>G</text>
<text>33</text>
<text>34</text>
<text>+</text>
<text>G</text>
<text>7</text>
<text>8</text>
<text>+</text>
<text>G</text>
<text>MAXIM</text>
<text>MAXIM</text>
<text>MAXIM</text>
<text>MAXIM</text>
<text>MAXIM</text>
<text>AUX IO</text>
<text>+5</text>
<text>G</text>
<text>3V3</text>
<text>G</text>
<text>27</text>
<text>28</text>
<text>G</text>
<text>M19</text>
<text>G</text>
<text>M10</text>
<text>M11</text>
<text>M12</text>
<text>M13</text>
<text>M14</text>
<text>M15</text>
<text>M16</text>
<text>M17</text>
<text>M18</text>
<text>top</text>
<text>23/A10</text>
<text>22/A11</text>
<text>17/A26</text>
<text>16/A25</text>
<text>TOP 9</text>
<text>BOT 10</text>
<text>BOT 8</text>
<text>TOP 7</text>
<text>33</text>
<text>34</text>
<text>MAXIM I/O</text>
<text>PIN 9 &amp; 10</text>
<text>IF BNC: 
INPUT ONLY
5V TOLERANT
TOP PIN 2
BOT PIN 5</text>
<text>-12V</text>
<text>12V</text>
<text>G</text>
<text>3v3</text>
<text>SDA2</text>
<text>SCL2</text>
<text>27</text>
<text>25</text>
<text>24</text>
<text>28</text>
<text>To use qwicc and Ethernet
- cut jumper ECS from 25 and
   solder to 27
- cut jumper ERST from 24 and
 solder to 28</text>
<text>Cable:
PRT-17259</text>
<text>SPI</text>
<text>SPI CS 
Pin 9
Pin 10</text>
</plain>
<libraries>
<library name="SteveS">
<packages>
<package name="0603S">
</package>
<package name="0805S">
</package>
<package name="1206S">
</package>
</packages>
</library>
<library name="STEVES_BU">
<packages>
<package name="AMPMODU-5">
</package>
<package name="JUMPER">
</package>
<package name="PJ-002">
</package>
<package name="PG-DSO-36">
</package>
<package name="NDTD">
</package>
<package name="TSSOP-24">
</package>
<package name="0603S">
</package>
<package name="LOGO_JANELIA_2014_DOC">
</package>
<package name="DUAL-BNC">
</package>
<package name="AMPMODU-4-RA">
</package>
<package name="PHOENIX_1881464">
</package>
<package name="FIDUCIAL_VIA">
</package>
<package name="TSSOP14">
<description>&lt;b&gt;14-Lead Thin Shrink Small Outline Package [TSSOP]&lt;/b&gt;&lt;p&gt;
Source: Analog Devices .. 780914713ADD8704_0.pdf</description>
</package>
<package name="MSOP10">
</package>
<package name="0805S">
</package>
<package name="1894804">
</package>
<package name="ILI9341TFT_HOLES">
</package>
<package name="TFT_LCD_NOHOLES">
</package>
<package name="0432024101">
</package>
<package name="SOT-143">
</package>
<package name="SOT23-6">
</package>
<package name="AMPMODU7-RATH">
</package>
<package name="2X5SHROUDED-RATH">
</package>
<package name="PAD032">
</package>
</packages>
</library>
<library name="MAX11300">
<packages>
<package name="TQFP48">
<description>&lt;b&gt;Thin Quad Flat Pack&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="con-subd">
<description>&lt;b&gt;SUB-D Connectors&lt;/b&gt;&lt;p&gt;
Harting&lt;br&gt;
NorComp&lt;br&gt;
&lt;p&gt;
PREFIX :&lt;br&gt;
H = High density&lt;br&gt;
F = Female&lt;br&gt;
M = Male&lt;p&gt;
NUMBER: Number of pins&lt;p&gt;
SUFFIX :&lt;br&gt;
H = Horizontal&lt;br&gt;
V = Vertical &lt;br&gt;
P = Shield pin on housing&lt;br&gt;
B = No mounting holes&lt;br&gt;
S = Pins individually placeable (Single)&lt;br&gt;
D = Direct mounting &lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="182-009-MALE">
<description>&lt;b&gt;NORCOMP Right Angle D-Sub Connector&lt;/b&gt;, 182 Economy Series (.318" Footprint)&lt;p&gt;
Source: http://www.norcomp.net/ .. 182-yyy-113Ryy1Rev3.pdf</description>
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT89">
<description>&lt;b&gt;SOT98&lt;/b&gt; PK (R-PDSO-G3)&lt;p&gt;
Source: http://focus.ti.com/lit/ds/symlink/ua78l05.pdf</description>
</package>
</packages>
</library>
<library name="jfrc">
<packages>
<package name="SOT89">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SJ_2">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04_LOCK">
</package>
</packages>
</library>
<library name="analog-devices">
<description>&lt;b&gt;Analog Devices Components&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SO8">
<description>&lt;b&gt;8-Lead Small Outline IC&lt;/b&gt; (SO-8)&lt;p&gt;
Source: http://www.analog.com/UploadedFiles/Data_Sheets/703465986AD8611_2_0.pdf</description>
</package>
</packages>
</library>
<library name="IQD-Frequency-Products">
<description>&lt;b&gt;Crystals and Oscillators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by IQD Frequency Products&lt;/author&gt;</description>
<packages>
<package name="5.2X3.4-4-PAD">
<description>&lt;b&gt;IQD Frequency Products SMD Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="rcl">
<description>&lt;b&gt;Resistors, Capacitors, Inductors&lt;/b&gt;&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;r.lbr
&lt;li&gt;cap.lbr 
&lt;li&gt;cap-fe.lbr
&lt;li&gt;captant.lbr
&lt;li&gt;polcap.lbr
&lt;li&gt;ipc-smd.lbr
&lt;/ul&gt;
All SMD packages are defined according to the IPC specifications and  CECC&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
for Electrolyt Capacitors see also :&lt;p&gt;
www.bccomponents.com &lt;p&gt;
www.panasonic.com&lt;p&gt;
www.kemet.com&lt;p&gt;
http://www.secc.co.jp/pdf/os_e/2004/e_os_all.pdf &lt;b&gt;(SANYO)&lt;/b&gt;
&lt;p&gt;
for trimmer refence see : &lt;u&gt;www.electrospec-inc.com/cross_references/trimpotcrossref.asp&lt;/u&gt;&lt;p&gt;

&lt;table border=0 cellspacing=0 cellpadding=0 width="100%" cellpaddding=0&gt;
&lt;tr valign="top"&gt;

&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;TRIM-POT CROSS REFERENCE&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;RECTANGULAR MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BOURNS&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BI&amp;nbsp;TECH&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;DALE-VISHAY&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PHILIPS/MEPCO&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MURATA&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PANASONIC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;SPECTROL&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MILSPEC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;&lt;TD&gt;&amp;nbsp;&lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3 &gt;
      3005P&lt;BR&gt;
      3006P&lt;BR&gt;
      3006W&lt;BR&gt;
      3006Y&lt;BR&gt;
      3009P&lt;BR&gt;
      3009W&lt;BR&gt;
      3009Y&lt;BR&gt;
      3057J&lt;BR&gt;
      3057L&lt;BR&gt;
      3057P&lt;BR&gt;
      3057Y&lt;BR&gt;
      3059J&lt;BR&gt;
      3059L&lt;BR&gt;
      3059P&lt;BR&gt;
      3059Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      89P&lt;BR&gt;
      89W&lt;BR&gt;
      89X&lt;BR&gt;
      89PH&lt;BR&gt;
      76P&lt;BR&gt;
      89XH&lt;BR&gt;
      78SLT&lt;BR&gt;
      78L&amp;nbsp;ALT&lt;BR&gt;
      56P&amp;nbsp;ALT&lt;BR&gt;
      78P&amp;nbsp;ALT&lt;BR&gt;
      T8S&lt;BR&gt;
      78L&lt;BR&gt;
      56P&lt;BR&gt;
      78P&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      T18/784&lt;BR&gt;
      783&lt;BR&gt;
      781&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2199&lt;BR&gt;
      1697/1897&lt;BR&gt;
      1680/1880&lt;BR&gt;
      2187&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      8035EKP/CT20/RJ-20P&lt;BR&gt;
      -&lt;BR&gt;
      RJ-20X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      1211L&lt;BR&gt;
      8012EKQ&amp;nbsp;ALT&lt;BR&gt;
      8012EKR&amp;nbsp;ALT&lt;BR&gt;
      1211P&lt;BR&gt;
      8012EKJ&lt;BR&gt;
      8012EKL&lt;BR&gt;
      8012EKQ&lt;BR&gt;
      8012EKR&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      2101P&lt;BR&gt;
      2101W&lt;BR&gt;
      2101Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2102L&lt;BR&gt;
      2102S&lt;BR&gt;
      2102Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVMCOG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      43P&lt;BR&gt;
      43W&lt;BR&gt;
      43Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      40L&lt;BR&gt;
      40P&lt;BR&gt;
      40Y&lt;BR&gt;
      70Y-T602&lt;BR&gt;
      70L&lt;BR&gt;
      70P&lt;BR&gt;
      70Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SQUARE MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
   &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3250L&lt;BR&gt;
      3250P&lt;BR&gt;
      3250W&lt;BR&gt;
      3250X&lt;BR&gt;
      3252P&lt;BR&gt;
      3252W&lt;BR&gt;
      3252X&lt;BR&gt;
      3260P&lt;BR&gt;
      3260W&lt;BR&gt;
      3260X&lt;BR&gt;
      3262P&lt;BR&gt;
      3262W&lt;BR&gt;
      3262X&lt;BR&gt;
      3266P&lt;BR&gt;
      3266W&lt;BR&gt;
      3266X&lt;BR&gt;
      3290H&lt;BR&gt;
      3290P&lt;BR&gt;
      3290W&lt;BR&gt;
      3292P&lt;BR&gt;
      3292W&lt;BR&gt;
      3292X&lt;BR&gt;
      3296P&lt;BR&gt;
      3296W&lt;BR&gt;
      3296X&lt;BR&gt;
      3296Y&lt;BR&gt;
      3296Z&lt;BR&gt;
      3299P&lt;BR&gt;
      3299W&lt;BR&gt;
      3299X&lt;BR&gt;
      3299Y&lt;BR&gt;
      3299Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64P&amp;nbsp;ALT&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      64X&amp;nbsp;ALT&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66P&lt;BR&gt;
      66W&lt;BR&gt;
      66X&lt;BR&gt;
      67P&lt;BR&gt;
      67W&lt;BR&gt;
      67X&lt;BR&gt;
      67Y&lt;BR&gt;
      67Z&lt;BR&gt;
      68P&lt;BR&gt;
      68W&lt;BR&gt;
      68X&lt;BR&gt;
      67Y&amp;nbsp;ALT&lt;BR&gt;
      67Z&amp;nbsp;ALT&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      5050&lt;BR&gt;
      5091&lt;BR&gt;
      5080&lt;BR&gt;
      5087&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T63YB&lt;BR&gt;
      T63XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      5887&lt;BR&gt;
      5891&lt;BR&gt;
      5880&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T93Z&lt;BR&gt;
      T93YA&lt;BR&gt;
      T93XA&lt;BR&gt;
      T93YB&lt;BR&gt;
      T93XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKW&lt;BR&gt;
      8026EKM&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKB&lt;BR&gt;
      8026EKM&lt;BR&gt;
      1309X&lt;BR&gt;
      1309P&lt;BR&gt;
      1309W&lt;BR&gt;
      8024EKP&lt;BR&gt;
      8024EKW&lt;BR&gt;
      8024EKN&lt;BR&gt;
      RJ-9P/CT9P&lt;BR&gt;
      RJ-9W&lt;BR&gt;
      RJ-9X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3105P/3106P&lt;BR&gt;
      3105W/3106W&lt;BR&gt;
      3105X/3106X&lt;BR&gt;
      3105Y/3106Y&lt;BR&gt;
      3105Z/3105Z&lt;BR&gt;
      3102P&lt;BR&gt;
      3102W&lt;BR&gt;
      3102X&lt;BR&gt;
      3102Y&lt;BR&gt;
      3102Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMCBG&lt;BR&gt;
      EVMCCG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      55-1-X&lt;BR&gt;
      55-4-X&lt;BR&gt;
      55-3-X&lt;BR&gt;
      55-2-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      50-2-X&lt;BR&gt;
      50-4-X&lt;BR&gt;
      50-3-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      64Y&lt;BR&gt;
      64Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3323P&lt;BR&gt;
      3323S&lt;BR&gt;
      3323W&lt;BR&gt;
      3329H&lt;BR&gt;
      3329P&lt;BR&gt;
      3329W&lt;BR&gt;
      3339H&lt;BR&gt;
      3339P&lt;BR&gt;
      3339W&lt;BR&gt;
      3352E&lt;BR&gt;
      3352H&lt;BR&gt;
      3352K&lt;BR&gt;
      3352P&lt;BR&gt;
      3352T&lt;BR&gt;
      3352V&lt;BR&gt;
      3352W&lt;BR&gt;
      3362H&lt;BR&gt;
      3362M&lt;BR&gt;
      3362P&lt;BR&gt;
      3362R&lt;BR&gt;
      3362S&lt;BR&gt;
      3362U&lt;BR&gt;
      3362W&lt;BR&gt;
      3362X&lt;BR&gt;
      3386B&lt;BR&gt;
      3386C&lt;BR&gt;
      3386F&lt;BR&gt;
      3386H&lt;BR&gt;
      3386K&lt;BR&gt;
      3386M&lt;BR&gt;
      3386P&lt;BR&gt;
      3386S&lt;BR&gt;
      3386W&lt;BR&gt;
      3386X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      25P&lt;BR&gt;
      25S&lt;BR&gt;
      25RX&lt;BR&gt;
      82P&lt;BR&gt;
      82M&lt;BR&gt;
      82PA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      91E&lt;BR&gt;
      91X&lt;BR&gt;
      91T&lt;BR&gt;
      91B&lt;BR&gt;
      91A&lt;BR&gt;
      91V&lt;BR&gt;
      91W&lt;BR&gt;
      25W&lt;BR&gt;
      25V&lt;BR&gt;
      25P&lt;BR&gt;
      -&lt;BR&gt;
      25S&lt;BR&gt;
      25U&lt;BR&gt;
      25RX&lt;BR&gt;
      25X&lt;BR&gt;
      72XW&lt;BR&gt;
      72XL&lt;BR&gt;
      72PM&lt;BR&gt;
      72RX&lt;BR&gt;
      -&lt;BR&gt;
      72PX&lt;BR&gt;
      72P&lt;BR&gt;
      72RXW&lt;BR&gt;
      72RXL&lt;BR&gt;
      72X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T7YB&lt;BR&gt;
      T7YA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      TXD&lt;BR&gt;
      TYA&lt;BR&gt;
      TYP&lt;BR&gt;
      -&lt;BR&gt;
      TYD&lt;BR&gt;
      TX&lt;BR&gt;
      -&lt;BR&gt;
      150SX&lt;BR&gt;
      100SX&lt;BR&gt;
      102T&lt;BR&gt;
      101S&lt;BR&gt;
      190T&lt;BR&gt;
      150TX&lt;BR&gt;
      101&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      101SX&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ET6P&lt;BR&gt;
      ET6S&lt;BR&gt;
      ET6X&lt;BR&gt;
      RJ-6W/8014EMW&lt;BR&gt;
      RJ-6P/8014EMP&lt;BR&gt;
      RJ-6X/8014EMX&lt;BR&gt;
      TM7W&lt;BR&gt;
      TM7P&lt;BR&gt;
      TM7X&lt;BR&gt;
      -&lt;BR&gt;
      8017SMS&lt;BR&gt;
      -&lt;BR&gt;
      8017SMB&lt;BR&gt;
      8017SMA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      CT-6W&lt;BR&gt;
      CT-6H&lt;BR&gt;
      CT-6P&lt;BR&gt;
      CT-6R&lt;BR&gt;
      -&lt;BR&gt;
      CT-6V&lt;BR&gt;
      CT-6X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKV&lt;BR&gt;
      -&lt;BR&gt;
      8038EKX&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKP&lt;BR&gt;
      8038EKZ&lt;BR&gt;
      8038EKW&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3321H&lt;BR&gt;
      3321P&lt;BR&gt;
      3321N&lt;BR&gt;
      1102H&lt;BR&gt;
      1102P&lt;BR&gt;
      1102T&lt;BR&gt;
      RVA0911V304A&lt;BR&gt;
      -&lt;BR&gt;
      RVA0911H413A&lt;BR&gt;
      RVG0707V100A&lt;BR&gt;
      RVA0607V(H)306A&lt;BR&gt;
      RVA1214H213A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3104B&lt;BR&gt;
      3104C&lt;BR&gt;
      3104F&lt;BR&gt;
      3104H&lt;BR&gt;
      -&lt;BR&gt;
      3104M&lt;BR&gt;
      3104P&lt;BR&gt;
      3104S&lt;BR&gt;
      3104W&lt;BR&gt;
      3104X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      EVMQ0G&lt;BR&gt;
      EVMQIG&lt;BR&gt;
      EVMQ3G&lt;BR&gt;
      EVMS0G&lt;BR&gt;
      EVMQ0G&lt;BR&gt;
      EVMG0G&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMK4GA00B&lt;BR&gt;
      EVM30GA00B&lt;BR&gt;
      EVMK0GA00B&lt;BR&gt;
      EVM38GA00B&lt;BR&gt;
      EVMB6&lt;BR&gt;
      EVLQ0&lt;BR&gt;
      -&lt;BR&gt;
      EVMMSG&lt;BR&gt;
      EVMMBG&lt;BR&gt;
      EVMMAG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMMCS&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM0&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM3&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      62-3-1&lt;BR&gt;
      62-1-2&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67R&lt;BR&gt;
      -&lt;BR&gt;
      67P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67X&lt;BR&gt;
      63V&lt;BR&gt;
      63S&lt;BR&gt;
      63M&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63H&lt;BR&gt;
      63P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;&amp;nbsp;&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=3&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT color="#0000FF" SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SMD TRIM-POT CROSS REFERENCE&lt;/B&gt;&lt;/FONT&gt;
      &lt;P&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3224G&lt;BR&gt;
      3224J&lt;BR&gt;
      3224W&lt;BR&gt;
      3269P&lt;BR&gt;
      3269W&lt;BR&gt;
      3269X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      44G&lt;BR&gt;
      44J&lt;BR&gt;
      44W&lt;BR&gt;
      84P&lt;BR&gt;
      84W&lt;BR&gt;
      84X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST63Z&lt;BR&gt;
      ST63Y&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST5P&lt;BR&gt;
      ST5W&lt;BR&gt;
      ST5X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3314G&lt;BR&gt;
      3314J&lt;BR&gt;
      3364A/B&lt;BR&gt;
      3364C/D&lt;BR&gt;
      3364W/X&lt;BR&gt;
      3313G&lt;BR&gt;
      3313J&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      23B&lt;BR&gt;
      23A&lt;BR&gt;
      21X&lt;BR&gt;
      21W&lt;BR&gt;
      -&lt;BR&gt;
      22B&lt;BR&gt;
      22A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST5YL/ST53YL&lt;BR&gt;
      ST5YJ/5T53YJ&lt;BR&gt;
      ST-23A&lt;BR&gt;
      ST-22B&lt;BR&gt;
      ST-22&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST-4B&lt;BR&gt;
      ST-4A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST-3B&lt;BR&gt;
      ST-3A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVM-6YS&lt;BR&gt;
      EVM-1E&lt;BR&gt;
      EVM-1G&lt;BR&gt;
      EVM-1D&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      G4B&lt;BR&gt;
      G4A&lt;BR&gt;
      TR04-3S1&lt;BR&gt;
      TRG04-2S1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      DVR-43A&lt;BR&gt;
      CVR-42C&lt;BR&gt;
      CVR-42A/C&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;
&lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;ALT =&amp;nbsp;ALTERNATE&lt;/B&gt;&lt;/FONT&gt;
&lt;P&gt;

&amp;nbsp;
&lt;P&gt;
&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;</description>
<packages>
<package name="PANASONIC_C">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package C&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SMB">
<description>&lt;B&gt;DIODE&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="Wiz820io">
<packages>
<package name="WIZ820IO">
<description>WIZnet, WIZ820io plug in module incl. W5200 chip and MagJack</description>
</package>
</packages>
</library>
<library name="con-3m">
<description>&lt;b&gt;3M Connectors&lt;/b&gt;&lt;p&gt;
PCMCIA-CompactFlash Connectors&lt;p&gt;
Zero Insertion Force Socked&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="PAK100/2500-20">
<description>&lt;b&gt;3M (TM) Pak 100 4-Wall Header&lt;/b&gt; Straight&lt;p&gt;
Source: 3M</description>
</package>
</packages>
</library>
<library name="teensy4.1.dist">
<packages>
<package name="TEENSY4.1">
</package>
</packages>
</library>
<library name="1734035-2">
<packages>
<package name="CONN_1734035-2">
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Aesthetics&lt;/h3&gt;
This library contiains non-functional items such as logos, build/ordering notes, frame blocks, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="QWIIC_8MM">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="JST04_1MM_RA">
<description>&lt;h3&gt;SMD- 4 Pin Right Angle &lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C14" library="SteveS" package="0603S" value="0.1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="SteveS" package="1206S" value="10">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C20" library="SteveS" package="0603S" value="0.1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="SteveS" package="1206S" value="10">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C30" library="SteveS" package="1206S" value="10">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C29" library="SteveS" package="0603S" value="0.1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C19" library="SteveS" package="0603S" value="0.1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="SteveS" package="1206S" value="10">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C27" library="SteveS" package="1206S" value="10">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C28" library="SteveS" package="0603S" value="0.1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RP1" library="SteveS" package="0805S" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RP2" library="SteveS" package="0805S" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J10" library="STEVES_BU" package="AMPMODU-5" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="R13" library="SteveS" package="0805S" value="2K70">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="SteveS" package="0805S" value="2K70">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U10" library="MAX11300" package="TQFP48" value="MAX11300GCM">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="SteveS" package="0805S" value="4R99">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JMP100" library="STEVES_BU" package="JUMPER" value="JUMPER">
<attribute name="VALUE"/>
</element>
<element name="C36" library="SteveS" package="1206S" value="10">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C32" library="SteveS" package="1206S" value="10">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C31" library="SteveS" package="1206S" value="10">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="STEVES_BU" package="PJ-002" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RP5" library="SteveS" package="0805S" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RP8" library="SteveS" package="0805S" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RP9" library="SteveS" package="0805S" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RP10" library="SteveS" package="0805S" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RP6" library="SteveS" package="0805S" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RP7" library="SteveS" package="0805S" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RP3" library="SteveS" package="0805S" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RP4" library="SteveS" package="0805S" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RT3" library="SteveS" package="0805S" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RT4" library="SteveS" package="0805S" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RT8" library="SteveS" package="0805S" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RT7" library="SteveS" package="0805S" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C33" library="SteveS" package="0603S" value="0.1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C37" library="SteveS" package="0603S" value="0.1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C38" library="SteveS" package="0603S" value="0.1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C40" library="SteveS" package="0603S" value="0.1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C39" library="SteveS" package="0603S" value="0.1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C34" library="SteveS" package="0603S" value="0.1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U5" library="STEVES_BU" package="PG-DSO-36" value="ISO1H815G">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PS1" library="STEVES_BU" package="NDTD" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U7" library="STEVES_BU" package="TSSOP-24" value="ADM3312/5">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="C23" library="STEVES_BU" package="0603S" value="0.1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C25" library="STEVES_BU" package="0603S" value="0.1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C24" library="STEVES_BU" package="0603S" value="0.1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C21" library="STEVES_BU" package="0603S" value="0.1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C26" library="STEVES_BU" package="0603S" value="0.1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U6" library="linear" package="SOT89" value="78L12">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U9" library="jfrc" package="SOT89" value="79L12">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C35" library="SteveS" package="1206S" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="STEVES_BU" package="LOGO_JANELIA_2014_DOC" value="JFRC-LOGOLOGO_2014_DOC"/>
<element name="P1" library="con-subd" package="182-009-MALE" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="P2" library="con-subd" package="182-009-MALE" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="P3" library="con-subd" package="182-009-MALE" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="J30" library="STEVES_BU" package="DUAL-BNC" value="">
<attribute name="VALUE"/>
</element>
<element name="J28" library="STEVES_BU" package="DUAL-BNC" value="">
<attribute name="VALUE"/>
</element>
<element name="J29" library="STEVES_BU" package="DUAL-BNC" value="">
<attribute name="VALUE"/>
</element>
<element name="J31" library="STEVES_BU" package="DUAL-BNC" value="">
<attribute name="VALUE"/>
</element>
<element name="J27" library="STEVES_BU" package="DUAL-BNC" value="">
<attribute name="VALUE"/>
</element>
<element name="J35" library="STEVES_BU" package="AMPMODU-4-RA" value="">
<attribute name="VALUE"/>
</element>
<element name="J33" library="STEVES_BU" package="AMPMODU-4-RA" value="">
<attribute name="VALUE"/>
</element>
<element name="J38" library="STEVES_BU" package="PHOENIX_1881464" value="">
<attribute name="VALUE"/>
</element>
<element name="J22" library="STEVES_BU" package="DUAL-BNC" value="">
<attribute name="VALUE"/>
</element>
<element name="J14" library="STEVES_BU" package="DUAL-BNC" value="A0/A1">
<attribute name="VALUE"/>
</element>
<element name="J40" library="STEVES_BU" package="PHOENIX_1881464" value="">
<attribute name="VALUE"/>
</element>
<element name="J32" library="STEVES_BU" package="AMPMODU-4-RA" value="">
<attribute name="VALUE"/>
</element>
<element name="J37" library="STEVES_BU" package="PHOENIX_1881464" value="">
<attribute name="VALUE"/>
</element>
<element name="J34" library="STEVES_BU" package="AMPMODU-4-RA" value="">
<attribute name="VALUE"/>
</element>
<element name="J39" library="STEVES_BU" package="PHOENIX_1881464" value="">
<attribute name="VALUE"/>
</element>
<element name="J36" library="STEVES_BU" package="AMPMODU-4-RA" value="">
<attribute name="VALUE"/>
</element>
<element name="J41" library="STEVES_BU" package="PHOENIX_1881464" value="">
<attribute name="VALUE"/>
</element>
<element name="J23" library="STEVES_BU" package="AMPMODU-4-RA" value="">
<attribute name="VALUE"/>
</element>
<element name="J24" library="STEVES_BU" package="PHOENIX_1881464" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J15" library="STEVES_BU" package="AMPMODU-4-RA" value="">
<attribute name="VALUE"/>
</element>
<element name="J16" library="STEVES_BU" package="PHOENIX_1881464" value="">
<attribute name="VALUE"/>
</element>
<element name="RT6" library="SteveS" package="0805S" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RT5" library="SteveS" package="0805S" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J19" library="STEVES_BU" package="DUAL-BNC" value="">
<attribute name="VALUE"/>
</element>
<element name="J18" library="STEVES_BU" package="AMPMODU-4-RA" value="">
<attribute name="VALUE"/>
</element>
<element name="SJ1" library="jumper" package="SJ_2" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ2" library="jumper" package="SJ_2" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RT1" library="SteveS" package="0805S" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RT2" library="SteveS" package="0805S" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J13" library="STEVES_BU" package="DUAL-BNC" value="">
<attribute name="VALUE"/>
</element>
<element name="J12" library="STEVES_BU" package="AMPMODU-4-RA" value="">
<attribute name="VALUE"/>
</element>
<element name="J4" library="STEVES_BU" package="DUAL-BNC" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SteveS" package="0805S" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SteveS" package="0805S" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="SteveS" package="0805S" value="0.1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FID1" library="STEVES_BU" package="FIDUCIAL_VIA" value="FIDUCIAL_VIA"/>
<element name="FID2" library="STEVES_BU" package="FIDUCIAL_VIA" value="FIDUCIAL_VIA"/>
<element name="FID3" library="STEVES_BU" package="FIDUCIAL_VIA" value="FIDUCIAL_VIA"/>
<element name="FID4" library="STEVES_BU" package="FIDUCIAL_VIA" value="FIDUCIAL_VIA"/>
<element name="JP1" library="SparkFun" package="1X04_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="STEVES_BU" package="TSSOP14" value="ISL23425">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U4" library="STEVES_BU" package="MSOP10" value="AD9833">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="analog-devices" package="SO8" value="ADA4084">
<attribute name="OC_NEWARK" value="59K4556"/>
<attribute name="OC_FARNELL" value="1263975"/>
<attribute name="MPN" value="AD712KRZ"/>
<attribute name="MF" value="ALTERA CORPORATION"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="STEVES_BU" package="0805S" value="1250">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="STEVES_BU" package="0805S" value="4K99">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="STEVES_BU" package="0805S" value="4K99">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="STEVES_BU" package="0603S" value="0.1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="STEVES_BU" package="0603S" value="0.1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="STEVES_BU" package="0603S" value="0.1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="STEVES_BU" package="0603S" value="0.1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X1" library="IQD-Frequency-Products" package="5.2X3.4-4-PAD" value="OSC-OE-CFPS-9">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="STEVES_BU" package="0603S" value="0.1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="rcl" package="PANASONIC_C" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="rcl" package="PANASONIC_C" value="">
<attribute name="VALUE"/>
</element>
<element name="C15" library="STEVES_BU" package="0603S" value="0.1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="STEVES_BU" package="0805S" value="1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="STEVES_BU" package="0603S" value="0.1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="STEVES_BU" package="1894804" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J6" library="STEVES_BU" package="1894804" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J7" library="STEVES_BU" package="1894804" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J8" library="STEVES_BU" package="1894804" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="OUT" library="jumper" package="SJ_2" value="SJ1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="diode" package="SMB" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="diode" package="SMB" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R17" library="SteveS" package="0805S" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L" library="STEVES_BU" package="ILI9341TFT_HOLES" value="ILI9341TFT_FP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="SteveS" package="0805S" value="10K0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="SteveS" package="0805S" value="10K0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LCD1" library="STEVES_BU" package="TFT_LCD_NOHOLES" value="TFT_LCDTFT_NOHOLES">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J21" library="STEVES_BU" package="0432024101" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J17" library="STEVES_BU" package="0432024101" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J9" library="STEVES_BU" package="0432024101" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J44" library="STEVES_BU" package="0432024101" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J45" library="STEVES_BU" package="0432024101" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J43" library="STEVES_BU" package="0432024101" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J42" library="STEVES_BU" package="0432024101" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J46" library="STEVES_BU" package="0432024101" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="SteveS" package="0805S" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="SteveS" package="0805S" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R25" library="SteveS" package="0805S" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R24" library="SteveS" package="0805S" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R22" library="SteveS" package="0805S" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="SteveS" package="0805S" value="118">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="SteveS" package="0805S" value="118">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="SteveS" package="0805S" value="118">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="Wiz820io" package="WIZ820IO" value="WIZ850io ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U11" library="STEVES_BU" package="SOT-143" value="CAT811">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R26" library="SteveS" package="0805S" value="4K99">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R27" library="SteveS" package="0805S" value="4K99">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ERST" library="jumper" package="SJ_2" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C41" library="SteveS" package="0603S" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ECS" library="jumper" package="SJ_2" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R28" library="SteveS" package="0805S" value="4R99">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RP11" library="SteveS" package="0805S" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RP12" library="SteveS" package="0805S" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RP13" library="SteveS" package="0805S" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RP14" library="SteveS" package="0805S" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RP15" library="SteveS" package="0805S" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RP16" library="SteveS" package="0805S" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RP17" library="SteveS" package="0805S" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RP18" library="SteveS" package="0805S" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RP19" library="SteveS" package="0805S" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RP20" library="SteveS" package="0805S" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="con-3m" package="PAK100/2500-20" value="2520-">
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RP22" library="SteveS" package="0805S" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RP23" library="SteveS" package="0805S" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="M2" library="teensy4.1.dist" package="TEENSY4.1" value="TEENSY4.1"/>
<element name="U2" library="STEVES_BU" package="SOT23-6" value="2G17">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="U8" library="STEVES_BU" package="SOT23-6" value="2G17">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="J20" library="STEVES_BU" package="DUAL-BNC" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="1734035-2" package="CONN_1734035-2" value="1734035-2">
<attribute name="MANUFACTURER" value="TE Connectivity"/>
<attribute name="PARTREV" value="F"/>
<attribute name="STANDARD" value="Manufacturer recommendations"/>
</element>
<element name="LOGO1" library="SparkFun-Aesthetics" package="QWIIC_8MM" value="QWIIC_LOGO_8MM"/>
<element name="J11" library="SparkFun-Connectors" package="JST04_1MM_RA" value="QWIIC_RIGHT_ANGLE">
<attribute name="PROD_ID" value="CONN-13694"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SteveS" package="0805S" value="4K99">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SteveS" package="0805S" value="4K99">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="STEVES_BU" package="AMPMODU7-RATH" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J26" library="STEVES_BU" package="2X5SHROUDED-RATH" value="">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="25MHZ" library="STEVES_BU" package="PAD032" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="AGND">
<contactref element="C30" pad="1"/>
<contactref element="C20" pad="2"/>
<contactref element="C29" pad="1"/>
<contactref element="C17" pad="2"/>
<contactref element="C19" pad="2"/>
<contactref element="C18" pad="2"/>
<contactref element="C28" pad="1"/>
<contactref element="C27" pad="1"/>
<contactref element="R13" pad="1"/>
<contactref element="R8" pad="2"/>
<contactref element="U10" pad="P$1"/>
<contactref element="U10" pad="38"/>
<contactref element="U10" pad="18"/>
<contactref element="U10" pad="17"/>
<contactref element="JMP100" pad="1"/>
<contactref element="C31" pad="2"/>
<contactref element="C32" pad="2"/>
<contactref element="C36" pad="2"/>
<contactref element="C40" pad="2"/>
<contactref element="C39" pad="2"/>
<contactref element="C38" pad="2"/>
<contactref element="C34" pad="2"/>
<contactref element="PS1" pad="16"/>
<contactref element="PS1" pad="9"/>
<contactref element="U6" pad="2"/>
<contactref element="U6" pad="2@1"/>
<contactref element="U9" pad="1"/>
<contactref element="C35" pad="2"/>
<contactref element="C37" pad="2"/>
<contactref element="J28" pad="P$4"/>
<contactref element="J28" pad="P$3"/>
<contactref element="J29" pad="P$4"/>
<contactref element="J29" pad="P$3"/>
<contactref element="J31" pad="P$4"/>
<contactref element="J31" pad="P$3"/>
<contactref element="J27" pad="P$4"/>
<contactref element="J27" pad="P$3"/>
<contactref element="J30" pad="P$4"/>
<contactref element="J30" pad="P$3"/>
<contactref element="J33" pad="4"/>
<contactref element="J38" pad="4"/>
<contactref element="J35" pad="4"/>
<contactref element="J40" pad="4"/>
<contactref element="J37" pad="4"/>
<contactref element="J32" pad="4"/>
<contactref element="J34" pad="4"/>
<contactref element="J39" pad="4"/>
<contactref element="J41" pad="4"/>
<contactref element="J36" pad="4"/>
<contactref element="C16" pad="2"/>
<contactref element="J4" pad="P$4"/>
<contactref element="J4" pad="P$3"/>
<contactref element="U4" pad="9"/>
<contactref element="C10" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="C15" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="U1" pad="4"/>
<contactref element="U3" pad="8"/>
<contactref element="J43" pad="3"/>
<contactref element="J42" pad="3"/>
<contactref element="J46" pad="3"/>
<contactref element="J44" pad="3"/>
<contactref element="J45" pad="3"/>
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="5"/>
<contactref element="JP2" pad="3"/>
</signal>
<signal name="DGND">
<contactref element="C12" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="U10" pad="2"/>
<contactref element="JMP100" pad="2"/>
<contactref element="J10" pad="5"/>
<contactref element="C33" pad="2"/>
<contactref element="U5" pad="4"/>
<contactref element="U5" pad="5"/>
<contactref element="PS1" pad="3"/>
<contactref element="PS1" pad="2"/>
<contactref element="U7" pad="5"/>
<contactref element="U7" pad="23"/>
<contactref element="U7" pad="19"/>
<contactref element="C25" pad="2"/>
<contactref element="P2" pad="5"/>
<contactref element="P3" pad="5"/>
<contactref element="P1" pad="5"/>
<contactref element="J22" pad="P$4"/>
<contactref element="J22" pad="P$3"/>
<contactref element="J14" pad="P$4"/>
<contactref element="J14" pad="P$3"/>
<contactref element="J15" pad="4"/>
<contactref element="J16" pad="4"/>
<contactref element="J24" pad="4"/>
<contactref element="J23" pad="4"/>
<contactref element="J19" pad="P$4"/>
<contactref element="J19" pad="P$3"/>
<contactref element="J18" pad="4"/>
<contactref element="J13" pad="P$4"/>
<contactref element="J13" pad="P$3"/>
<contactref element="J12" pad="4"/>
<contactref element="JP1" pad="4"/>
<contactref element="JP1" pad="3"/>
<contactref element="JP1" pad="2"/>
<contactref element="JP1" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="U3" pad="7"/>
<contactref element="U3" pad="1"/>
<contactref element="C11" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="U4" pad="4"/>
<contactref element="X1" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="U5" pad="15"/>
<contactref element="LCD1" pad="2"/>
<contactref element="J21" pad="3"/>
<contactref element="J17" pad="3"/>
<contactref element="J9" pad="3"/>
<contactref element="IC1" pad="J1.1"/>
<contactref element="IC1" pad="J1.2"/>
<contactref element="IC1" pad="J2.1"/>
<contactref element="U11" pad="1"/>
<contactref element="IC1" pad="J2.4"/>
<contactref element="C41" pad="1"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP2" pad="10"/>
<contactref element="JP2" pad="20"/>
<contactref element="M2" pad="GND"/>
<contactref element="M2" pad="GND1"/>
<contactref element="M2" pad="AGND"/>
<contactref element="U2" pad="2"/>
<contactref element="U8" pad="2"/>
<contactref element="M2" pad="GND2"/>
<contactref element="J20" pad="P$3"/>
<contactref element="J20" pad="P$4"/>
<contactref element="U8" pad="1"/>
<contactref element="J2" pad="5"/>
<contactref element="J11" pad="1"/>
<contactref element="J3" pad="1"/>
<contactref element="J26" pad="7"/>
<contactref element="J26" pad="5"/>
<contactref element="J26" pad="3"/>
<contactref element="J26" pad="1"/>
</signal>
<signal name="-15V">
<contactref element="C29" pad="2"/>
<contactref element="C30" pad="2"/>
<contactref element="R13" pad="2"/>
<contactref element="PS1" pad="11"/>
<contactref element="U9" pad="2"/>
<contactref element="U9" pad="2@1"/>
</signal>
<signal name="-12VA">
<contactref element="C28" pad="2"/>
<contactref element="C27" pad="2"/>
<contactref element="U10" pad="24"/>
<contactref element="U10" pad="29"/>
<contactref element="U10" pad="34"/>
<contactref element="U10" pad="41"/>
<contactref element="U10" pad="44"/>
<contactref element="U10" pad="48"/>
<contactref element="C34" pad="1"/>
<contactref element="C38" pad="1"/>
<contactref element="U9" pad="3"/>
<contactref element="JP2" pad="6"/>
</signal>
<signal name="+12VA">
<contactref element="C19" pad="1"/>
<contactref element="C18" pad="1"/>
<contactref element="U10" pad="26"/>
<contactref element="U10" pad="39"/>
<contactref element="C40" pad="1"/>
<contactref element="C39" pad="1"/>
<contactref element="U6" pad="1"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="EN_B">
<contactref element="J10" pad="1"/>
<contactref element="U2" pad="3"/>
<contactref element="J20" pad="P$1"/>
</signal>
<signal name="EA">
<contactref element="RP1" pad="1"/>
<contactref element="J28" pad="P$2"/>
<contactref element="J33" pad="2"/>
<contactref element="J38" pad="2"/>
<contactref element="J43" pad="1"/>
</signal>
<signal name="EB">
<contactref element="RP2" pad="1"/>
<contactref element="J28" pad="P$1"/>
<contactref element="J33" pad="3"/>
<contactref element="J38" pad="3"/>
<contactref element="J43" pad="4"/>
</signal>
<signal name="IDX">
<contactref element="J10" pad="4"/>
<contactref element="U8" pad="3"/>
</signal>
<signal name="COPI">
<contactref element="U10" pad="4"/>
<contactref element="U4" pad="6"/>
<contactref element="U3" pad="5"/>
<contactref element="LCD1" pad="6"/>
<contactref element="LCD1" pad="12"/>
<contactref element="IC1" pad="J1.3"/>
<contactref element="M2" pad="11/MOSI"/>
<contactref element="J3" pad="3"/>
<contactref element="J26" pad="4"/>
</signal>
<signal name="CIPO">
<contactref element="U10" pad="7"/>
<contactref element="U3" pad="3"/>
<contactref element="LCD1" pad="9"/>
<contactref element="LCD1" pad="13"/>
<contactref element="IC1" pad="J2.6"/>
<contactref element="M2" pad="12/MISO"/>
<contactref element="J3" pad="4"/>
<contactref element="J26" pad="6"/>
</signal>
<signal name="SCLK">
<contactref element="U10" pad="5"/>
<contactref element="U4" pad="7"/>
<contactref element="U3" pad="4"/>
<contactref element="LCD1" pad="7"/>
<contactref element="LCD1" pad="10"/>
<contactref element="IC1" pad="J1.4"/>
<contactref element="M2" pad="13/SCK"/>
<contactref element="J3" pad="2"/>
<contactref element="J26" pad="2"/>
</signal>
<signal name="+3V3D">
<contactref element="U10" pad="3"/>
<contactref element="C33" pad="1"/>
<contactref element="U5" pad="3"/>
<contactref element="U5" pad="2"/>
<contactref element="U7" pad="3"/>
<contactref element="C23" pad="2"/>
<contactref element="R16" pad="1"/>
<contactref element="R20" pad="1"/>
<contactref element="IC1" pad="J2.2"/>
<contactref element="IC1" pad="J2.3"/>
<contactref element="U11" pad="4"/>
<contactref element="R27" pad="1"/>
<contactref element="R26" pad="1"/>
<contactref element="C41" pad="2"/>
<contactref element="C10" pad="1"/>
<contactref element="U4" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="X1" pad="4"/>
<contactref element="C4" pad="1"/>
<contactref element="U3" pad="14"/>
<contactref element="C8" pad="2"/>
<contactref element="C11" pad="1"/>
<contactref element="U3" pad="2"/>
<contactref element="R23" pad="2"/>
<contactref element="R28" pad="2"/>
<contactref element="J33" pad="1"/>
<contactref element="J38" pad="1"/>
<contactref element="R21" pad="2"/>
<contactref element="J34" pad="1"/>
<contactref element="J39" pad="1"/>
<contactref element="R22" pad="2"/>
<contactref element="J41" pad="1"/>
<contactref element="J36" pad="1"/>
<contactref element="R24" pad="2"/>
<contactref element="J37" pad="1"/>
<contactref element="J32" pad="1"/>
<contactref element="R25" pad="2"/>
<contactref element="J24" pad="1"/>
<contactref element="J23" pad="1"/>
<contactref element="J18" pad="1"/>
<contactref element="J12" pad="1"/>
<contactref element="R12" pad="2"/>
<contactref element="J15" pad="1"/>
<contactref element="J16" pad="1"/>
<contactref element="M2" pad="3V3"/>
<contactref element="M2" pad="3V3_LO"/>
<contactref element="R19" pad="1"/>
<contactref element="R15" pad="1"/>
<contactref element="U8" pad="5"/>
<contactref element="U2" pad="5"/>
<contactref element="M2" pad="V33"/>
<contactref element="JP2" pad="4"/>
<contactref element="J11" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="J3" pad="7"/>
<contactref element="J26" pad="9"/>
</signal>
<signal name="+5VA">
<contactref element="R14" pad="1"/>
<contactref element="U10" pad="15"/>
<contactref element="U10" pad="16"/>
<contactref element="C37" pad="1"/>
<contactref element="C35" pad="1"/>
</signal>
<signal name="DAC_REF">
<contactref element="U10" pad="12"/>
<contactref element="C36" pad="1"/>
</signal>
<signal name="EXT_REF">
<contactref element="U10" pad="11"/>
<contactref element="C32" pad="1"/>
</signal>
<signal name="INT_REF">
<contactref element="U10" pad="10"/>
<contactref element="C31" pad="1"/>
</signal>
<signal name="!MAXCNVT">
<contactref element="U10" pad="9"/>
<contactref element="M2" pad="30"/>
</signal>
<signal name="P0">
<contactref element="RP1" pad="2"/>
<contactref element="U10" pad="19"/>
</signal>
<signal name="P1">
<contactref element="U10" pad="20"/>
<contactref element="RP2" pad="2"/>
</signal>
<signal name="+5VD">
<contactref element="D2" pad="C"/>
<contactref element="D1" pad="A"/>
<contactref element="R17" pad="1"/>
<contactref element="LCD1" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="C14" pad="1"/>
<contactref element="R14" pad="2"/>
<contactref element="PS1" pad="22"/>
<contactref element="PS1" pad="23"/>
<contactref element="J10" pad="2"/>
<contactref element="JP2" pad="2"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="P4">
<contactref element="U10" pad="27"/>
<contactref element="RP9" pad="2"/>
</signal>
<signal name="P6">
<contactref element="U10" pad="30"/>
<contactref element="RP6" pad="2"/>
</signal>
<signal name="EN_A">
<contactref element="J10" pad="3"/>
<contactref element="U2" pad="1"/>
<contactref element="J20" pad="P$2"/>
</signal>
<signal name="RX1">
<contactref element="U7" pad="10"/>
<contactref element="M2" pad="0/RX"/>
</signal>
<signal name="TX1">
<contactref element="U7" pad="7"/>
<contactref element="M2" pad="1/TX"/>
</signal>
<signal name="P8">
<contactref element="U10" pad="32"/>
<contactref element="RP3" pad="2"/>
</signal>
<signal name="EA1">
<contactref element="RP5" pad="1"/>
<contactref element="J29" pad="P$2"/>
<contactref element="J39" pad="2"/>
<contactref element="J34" pad="2"/>
<contactref element="J44" pad="1"/>
</signal>
<signal name="EB1">
<contactref element="RP8" pad="1"/>
<contactref element="J29" pad="P$1"/>
<contactref element="J39" pad="3"/>
<contactref element="J34" pad="3"/>
<contactref element="J44" pad="4"/>
</signal>
<signal name="P3">
<contactref element="RP8" pad="2"/>
<contactref element="U10" pad="25"/>
</signal>
<signal name="EA2">
<contactref element="RP9" pad="1"/>
<contactref element="J30" pad="P$2"/>
<contactref element="J35" pad="2"/>
<contactref element="J40" pad="2"/>
<contactref element="J42" pad="1"/>
</signal>
<signal name="EB2">
<contactref element="RP10" pad="1"/>
<contactref element="J35" pad="3"/>
<contactref element="J40" pad="3"/>
<contactref element="J30" pad="P$1"/>
<contactref element="J42" pad="4"/>
</signal>
<signal name="P5">
<contactref element="RP10" pad="2"/>
<contactref element="U10" pad="28"/>
</signal>
<signal name="EA3">
<contactref element="RP6" pad="1"/>
<contactref element="J31" pad="P$2"/>
<contactref element="J41" pad="2"/>
<contactref element="J36" pad="2"/>
<contactref element="J45" pad="1"/>
</signal>
<signal name="EB3">
<contactref element="RP7" pad="1"/>
<contactref element="J31" pad="P$1"/>
<contactref element="J41" pad="3"/>
<contactref element="J36" pad="3"/>
<contactref element="J45" pad="4"/>
</signal>
<signal name="P7">
<contactref element="RP7" pad="2"/>
<contactref element="U10" pad="31"/>
</signal>
<signal name="TX2">
<contactref element="U7" pad="9"/>
<contactref element="SJ2" pad="1"/>
<contactref element="SJ2" pad="2"/>
<contactref element="M2" pad="8"/>
</signal>
<signal name="EA4">
<contactref element="RP3" pad="1"/>
<contactref element="J37" pad="2"/>
<contactref element="J32" pad="2"/>
<contactref element="J46" pad="1"/>
<contactref element="J27" pad="P$2"/>
</signal>
<signal name="EB4">
<contactref element="RP4" pad="1"/>
<contactref element="J37" pad="3"/>
<contactref element="J32" pad="3"/>
<contactref element="J27" pad="P$1"/>
<contactref element="J46" pad="4"/>
</signal>
<signal name="P9">
<contactref element="RP4" pad="2"/>
<contactref element="U10" pad="33"/>
</signal>
<signal name="EA6">
<contactref element="RT8" pad="1"/>
<contactref element="J22" pad="P$2"/>
<contactref element="J24" pad="2"/>
<contactref element="J23" pad="2"/>
<contactref element="J21" pad="1"/>
</signal>
<signal name="!CS_DDS">
<contactref element="U4" pad="8"/>
<contactref element="M2" pad="19/A5/SCL"/>
</signal>
<signal name="VBB">
<contactref element="J1" pad="1B"/>
<contactref element="J1" pad="1A"/>
<contactref element="U5" pad="P$1"/>
</signal>
<signal name="DRV0">
<contactref element="U5" pad="36"/>
<contactref element="U5" pad="35"/>
<contactref element="J5" pad="3"/>
</signal>
<signal name="DRV1">
<contactref element="U5" pad="34"/>
<contactref element="U5" pad="33"/>
<contactref element="J6" pad="3"/>
</signal>
<signal name="DRV2">
<contactref element="U5" pad="32"/>
<contactref element="U5" pad="31"/>
<contactref element="J7" pad="3"/>
</signal>
<signal name="SOL1">
<contactref element="U5" pad="6"/>
<contactref element="M2" pad="23/A9"/>
</signal>
<signal name="SOL2">
<contactref element="U5" pad="7"/>
<contactref element="M2" pad="22/A8"/>
</signal>
<signal name="SOL3">
<contactref element="U5" pad="8"/>
<contactref element="M2" pad="17/A3"/>
</signal>
<signal name="SOL4">
<contactref element="U5" pad="9"/>
<contactref element="M2" pad="16/A2"/>
</signal>
<signal name="N$16">
<contactref element="U7" pad="18"/>
<contactref element="P1" pad="3"/>
</signal>
<signal name="N$28">
<contactref element="U7" pad="15"/>
<contactref element="P1" pad="2"/>
</signal>
<signal name="N$44">
<contactref element="U7" pad="16"/>
<contactref element="P3" pad="3"/>
</signal>
<signal name="RX3_232">
<contactref element="U7" pad="13"/>
<contactref element="P3" pad="2"/>
</signal>
<signal name="N$46">
</signal>
<signal name="N$47">
</signal>
<signal name="N$48">
</signal>
<signal name="H2">
</signal>
<signal name="N$9">
<contactref element="U7" pad="14"/>
<contactref element="P2" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="U7" pad="1"/>
<contactref element="C23" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="U7" pad="21"/>
<contactref element="C25" pad="1"/>
</signal>
<signal name="N$21">
<contactref element="U7" pad="24"/>
<contactref element="C26" pad="2"/>
</signal>
<signal name="N$23">
<contactref element="U7" pad="22"/>
<contactref element="C26" pad="1"/>
</signal>
<signal name="N$25">
<contactref element="U7" pad="4"/>
<contactref element="C21" pad="1"/>
</signal>
<signal name="N$26">
<contactref element="C21" pad="2"/>
<contactref element="U7" pad="2"/>
</signal>
<signal name="N$27">
<contactref element="U7" pad="20"/>
<contactref element="C24" pad="1"/>
</signal>
<signal name="N$31">
<contactref element="C24" pad="2"/>
<contactref element="U7" pad="6"/>
</signal>
<signal name="P2">
<contactref element="U10" pad="21"/>
<contactref element="RP5" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="P2" pad="3"/>
<contactref element="U7" pad="17"/>
</signal>
<signal name="TFT_DC">
<contactref element="LCD1" pad="5"/>
<contactref element="M2" pad="21/A7"/>
</signal>
<signal name="EA5">
<contactref element="J16" pad="2"/>
<contactref element="RT3" pad="1"/>
<contactref element="J14" pad="P$2"/>
<contactref element="J15" pad="2"/>
<contactref element="J17" pad="1"/>
</signal>
<signal name="EB5">
<contactref element="J16" pad="3"/>
<contactref element="RT4" pad="1"/>
<contactref element="J15" pad="3"/>
<contactref element="J17" pad="4"/>
<contactref element="J14" pad="P$1"/>
</signal>
<signal name="EA9">
<contactref element="RT6" pad="1"/>
<contactref element="J19" pad="P$2"/>
<contactref element="J18" pad="2"/>
</signal>
<signal name="EA10">
<contactref element="RT5" pad="1"/>
<contactref element="J19" pad="P$1"/>
<contactref element="J18" pad="3"/>
</signal>
<signal name="PIN7">
<contactref element="SJ1" pad="3"/>
<contactref element="RT1" pad="2"/>
</signal>
<signal name="PIN8">
<contactref element="SJ2" pad="3"/>
<contactref element="RT2" pad="2"/>
</signal>
<signal name="EA7">
<contactref element="RT1" pad="1"/>
<contactref element="J13" pad="P$2"/>
<contactref element="J12" pad="2"/>
<contactref element="J9" pad="1"/>
</signal>
<signal name="EB8">
<contactref element="RT2" pad="1"/>
<contactref element="J13" pad="P$1"/>
<contactref element="J12" pad="3"/>
<contactref element="J9" pad="4"/>
</signal>
<signal name="PIN9">
<contactref element="M2" pad="9"/>
<contactref element="RT6" pad="2"/>
<contactref element="J3" pad="5"/>
<contactref element="J26" pad="8"/>
</signal>
<signal name="PIN10">
<contactref element="M2" pad="10/CS"/>
<contactref element="RT5" pad="2"/>
<contactref element="J3" pad="6"/>
<contactref element="J26" pad="10"/>
</signal>
<signal name="VIN">
<contactref element="D2" pad="A"/>
<contactref element="D1" pad="C"/>
<contactref element="M2" pad="VIN"/>
</signal>
<signal name="!TFT_CS">
<contactref element="LCD1" pad="3"/>
<contactref element="M2" pad="36"/>
</signal>
<signal name="A16">
<contactref element="R1" pad="1"/>
<contactref element="M2" pad="40"/>
</signal>
<signal name="ETH_INT">
<contactref element="IC1" pad="J1.6"/>
<contactref element="M2" pad="26"/>
</signal>
<signal name="PIN27/ALT_ECS">
<contactref element="RP23" pad="1"/>
<contactref element="M2" pad="27"/>
<contactref element="ECS" pad="1"/>
<contactref element="R27" pad="2"/>
</signal>
<signal name="PIN28/ALT_ERST">
<contactref element="RP22" pad="1"/>
<contactref element="M2" pad="28"/>
<contactref element="ERST" pad="1"/>
<contactref element="R26" pad="2"/>
</signal>
<signal name="A17">
<contactref element="M2" pad="41"/>
<contactref element="RT7" pad="2"/>
</signal>
<signal name="!MAX_CS">
<contactref element="U10" pad="6"/>
<contactref element="M2" pad="6"/>
</signal>
<signal name="PWR_P4-5">
<contactref element="J40" pad="1"/>
<contactref element="J35" pad="1"/>
</signal>
<signal name="!MAXINT">
<contactref element="U10" pad="8"/>
<contactref element="M2" pad="29"/>
</signal>
<signal name="DAC0_OUT">
<contactref element="R1" pad="2"/>
<contactref element="J4" pad="P$1"/>
</signal>
<signal name="DDS_OUT">
<contactref element="R5" pad="2"/>
<contactref element="C16" pad="1"/>
<contactref element="J4" pad="P$2"/>
</signal>
<signal name="!CS_POT">
<contactref element="U3" pad="6"/>
<contactref element="M2" pad="31/A12"/>
</signal>
<signal name="N$13">
<contactref element="U4" pad="5"/>
<contactref element="X1" pad="3"/>
<contactref element="25MHZ" pad="P$1"/>
</signal>
<signal name="N$20">
<contactref element="U4" pad="3"/>
<contactref element="C7" pad="1"/>
</signal>
<signal name="N$22">
<contactref element="U4" pad="1"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="N$34">
<contactref element="R4" pad="1"/>
<contactref element="C13" pad="+"/>
</signal>
<signal name="N$36">
<contactref element="R4" pad="2"/>
<contactref element="U1" pad="2"/>
<contactref element="U3" pad="13"/>
</signal>
<signal name="N$37">
<contactref element="U1" pad="7"/>
</signal>
<signal name="N$38">
<contactref element="U3" pad="11"/>
<contactref element="U3" pad="12"/>
<contactref element="U1" pad="1"/>
<contactref element="C9" pad="+"/>
</signal>
<signal name="DDS">
<contactref element="C13" pad="-"/>
<contactref element="U4" pad="10"/>
<contactref element="OUT" pad="1"/>
</signal>
<signal name="DRV4">
<contactref element="U5" pad="28"/>
<contactref element="U5" pad="27"/>
<contactref element="J5" pad="1"/>
</signal>
<signal name="DRV5">
<contactref element="U5" pad="26"/>
<contactref element="U5" pad="25"/>
<contactref element="J6" pad="1"/>
</signal>
<signal name="DRV3">
<contactref element="J8" pad="3"/>
<contactref element="U5" pad="30"/>
<contactref element="U5" pad="29"/>
</signal>
<signal name="DRV7">
<contactref element="U5" pad="22"/>
<contactref element="U5" pad="21"/>
<contactref element="J8" pad="1"/>
</signal>
<signal name="GNDBB">
<contactref element="J1" pad="2"/>
<contactref element="U5" pad="19"/>
<contactref element="J7" pad="4"/>
<contactref element="J7" pad="2"/>
<contactref element="J6" pad="4"/>
<contactref element="J6" pad="2"/>
<contactref element="J5" pad="2"/>
<contactref element="J5" pad="4"/>
<contactref element="J8" pad="2"/>
<contactref element="J8" pad="4"/>
</signal>
<signal name="DRV6">
<contactref element="U5" pad="24"/>
<contactref element="U5" pad="23"/>
<contactref element="J7" pad="1"/>
</signal>
<signal name="SOL5">
<contactref element="U5" pad="10"/>
<contactref element="M2" pad="18/A4/SDA"/>
</signal>
<signal name="SOL7">
<contactref element="U5" pad="12"/>
<contactref element="M2" pad="3"/>
</signal>
<signal name="SOL6">
<contactref element="U5" pad="11"/>
<contactref element="M2" pad="39"/>
</signal>
<signal name="SOL8">
<contactref element="U5" pad="13"/>
<contactref element="M2" pad="4"/>
</signal>
<signal name="SJ1">
<contactref element="C9" pad="-"/>
<contactref element="OUT" pad="3"/>
<contactref element="R5" pad="1"/>
<contactref element="OUT" pad="2"/>
</signal>
<signal name="+15V">
<contactref element="C20" pad="1"/>
<contactref element="C17" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="PS1" pad="14"/>
<contactref element="U6" pad="3"/>
</signal>
<signal name="TFT_LED">
<contactref element="R17" pad="2"/>
<contactref element="LCD1" pad="8"/>
</signal>
<signal name="EB6">
<contactref element="RT7" pad="1"/>
<contactref element="J22" pad="P$1"/>
<contactref element="J24" pad="3"/>
<contactref element="J23" pad="3"/>
<contactref element="J21" pad="4"/>
</signal>
<signal name="N$24">
<contactref element="J43" pad="2"/>
<contactref element="R21" pad="1"/>
</signal>
<signal name="N$29">
<contactref element="J42" pad="2"/>
<contactref element="R23" pad="1"/>
</signal>
<signal name="N$33">
<contactref element="J46" pad="2"/>
<contactref element="R25" pad="1"/>
</signal>
<signal name="N$35">
<contactref element="J45" pad="2"/>
<contactref element="R24" pad="1"/>
</signal>
<signal name="N$41">
<contactref element="J44" pad="2"/>
<contactref element="R22" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="R19" pad="2"/>
<contactref element="J21" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="R15" pad="2"/>
<contactref element="J17" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="J9" pad="2"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="PIN33">
<contactref element="M2" pad="33"/>
<contactref element="RT3" pad="2"/>
</signal>
<signal name="ERST">
<contactref element="U11" pad="2"/>
<contactref element="IC1" pad="J2.5"/>
</signal>
<signal name="+3V3ADDS">
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="8"/>
<contactref element="R28" pad="1"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="P10">
<contactref element="U10" pad="35"/>
<contactref element="RP20" pad="1"/>
</signal>
<signal name="P11">
<contactref element="U10" pad="36"/>
<contactref element="RP19" pad="1"/>
</signal>
<signal name="P12">
<contactref element="U10" pad="37"/>
<contactref element="RP18" pad="1"/>
</signal>
<signal name="P13">
<contactref element="U10" pad="40"/>
<contactref element="RP17" pad="1"/>
</signal>
<signal name="P14">
<contactref element="U10" pad="42"/>
<contactref element="RP16" pad="1"/>
</signal>
<signal name="P15">
<contactref element="U10" pad="43"/>
<contactref element="RP15" pad="1"/>
</signal>
<signal name="P16">
<contactref element="U10" pad="45"/>
<contactref element="RP14" pad="1"/>
</signal>
<signal name="P17">
<contactref element="U10" pad="46"/>
<contactref element="RP13" pad="1"/>
</signal>
<signal name="P18">
<contactref element="U10" pad="47"/>
<contactref element="RP12" pad="1"/>
</signal>
<signal name="P19">
<contactref element="U10" pad="1"/>
<contactref element="RP11" pad="1"/>
</signal>
<signal name="ETH_RST/SCL2">
<contactref element="M2" pad="24"/>
<contactref element="J11" pad="4"/>
<contactref element="R2" pad="2"/>
<contactref element="U11" pad="3"/>
<contactref element="ERST" pad="3"/>
<contactref element="ERST" pad="2"/>
</signal>
<signal name="ETH_CS/SDA2">
<contactref element="IC1" pad="J1.5"/>
<contactref element="ECS" pad="2"/>
<contactref element="ECS" pad="3"/>
<contactref element="M2" pad="25"/>
<contactref element="J11" pad="3"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$53">
<contactref element="RP20" pad="2"/>
<contactref element="JP2" pad="19"/>
</signal>
<signal name="N$54">
<contactref element="JP2" pad="18"/>
<contactref element="RP19" pad="2"/>
</signal>
<signal name="N$55">
<contactref element="RP18" pad="2"/>
<contactref element="JP2" pad="17"/>
</signal>
<signal name="N$56">
<contactref element="JP2" pad="16"/>
<contactref element="RP17" pad="2"/>
</signal>
<signal name="N$57">
<contactref element="RP16" pad="2"/>
<contactref element="JP2" pad="15"/>
</signal>
<signal name="N$42">
<contactref element="RP15" pad="2"/>
<contactref element="JP2" pad="14"/>
</signal>
<signal name="N$51">
<contactref element="JP2" pad="13"/>
<contactref element="RP14" pad="2"/>
</signal>
<signal name="N$58">
<contactref element="RP13" pad="2"/>
<contactref element="JP2" pad="12"/>
</signal>
<signal name="N$59">
<contactref element="RP12" pad="2"/>
<contactref element="JP2" pad="11"/>
</signal>
<signal name="N$60">
<contactref element="RP11" pad="2"/>
<contactref element="JP2" pad="9"/>
</signal>
<signal name="N$62">
<contactref element="RP22" pad="2"/>
<contactref element="JP2" pad="7"/>
</signal>
<signal name="A6/20">
<contactref element="M2" pad="20/A6"/>
<contactref element="RT8" pad="2"/>
</signal>
<signal name="+1V65A">
<contactref element="R6" pad="2"/>
<contactref element="C15" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="RX2">
<contactref element="M2" pad="7"/>
<contactref element="U7" pad="12"/>
<contactref element="SJ1" pad="1"/>
<contactref element="SJ1" pad="2"/>
</signal>
<signal name="!TCHINT">
<contactref element="LCD1" pad="14"/>
<contactref element="M2" pad="32"/>
</signal>
<signal name="!TFTRST">
<contactref element="LCD1" pad="4"/>
<contactref element="M2" pad="37"/>
<contactref element="R20" pad="2"/>
</signal>
<signal name="!CS_TCH">
<contactref element="LCD1" pad="11"/>
<contactref element="M2" pad="38"/>
<contactref element="R16" pad="2"/>
</signal>
<signal name="IDX3V3">
<contactref element="M2" pad="35"/>
<contactref element="U8" pad="4"/>
</signal>
<signal name="ENCA3V3">
<contactref element="M2" pad="2"/>
<contactref element="U2" pad="6"/>
</signal>
<signal name="ENCB3V3">
<contactref element="M2" pad="5"/>
<contactref element="U2" pad="4"/>
</signal>
<signal name="RX3">
<contactref element="M2" pad="15/A1"/>
<contactref element="U7" pad="11"/>
</signal>
<signal name="TX3">
<contactref element="M2" pad="14/A0"/>
<contactref element="U7" pad="8"/>
</signal>
<signal name="PIN34">
<contactref element="M2" pad="34"/>
<contactref element="RT4" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="RP23" pad="2"/>
<contactref element="JP2" pad="8"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
