<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="25.5804" y2="0" width="0" layer="20"/>
<wire x1="25.5804" y1="0" x2="25.5804" y2="15" width="0" layer="20"/>
<wire x1="25.5804" y1="15" x2="0" y2="15" width="0" layer="20"/>
<wire x1="0" y1="15" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="EXASTIFY">
<packages>
<package name="TE-FPC-12">
</package>
<package name="SOT-5">
</package>
<package name="B3U-3000P">
</package>
<package name="ISP">
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
<package name="0603-CAP">
</package>
<package name="0603-RES">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="EXASTIFY" package="TE-FPC-12" value="FRC"/>
<element name="U1" library="SparkFun-DigitalIC" package="TQFP32-08" value="ATMEGA328P">
<attribute name="PROD_ID" value="IC-09069"/>
</element>
<element name="U$2" library="EXASTIFY" package="SOT-5" value="TPS782XXDDC"/>
<element name="C1" library="SparkFun-Passives" package="0805" value="BATT"/>
<element name="C2" library="SparkFun-Passives" package="0603-CAP" value="1uf"/>
<element name="C3" library="SparkFun-Passives" package="0603-CAP" value="1uf"/>
<element name="U$3" library="EXASTIFY" package="B3U-3000P" value="B3U-3000P"/>
<element name="R1" library="SparkFun-Passives" package="0603-RES" value=""/>
<element name="U$4" library="EXASTIFY" package="ISP" value="ISP"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U$1" pad="P$12"/>
<contactref element="U$1" pad="P$1"/>
<contactref element="U$1" pad="P$9"/>
<contactref element="U$2" pad="P$2"/>
<contactref element="C1" pad="2"/>
<contactref element="U$2" pad="P$4"/>
<contactref element="C3" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="U1" pad="21"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="5"/>
<contactref element="U$3" pad="P$2"/>
<contactref element="U$4" pad="P$1"/>
</signal>
<signal name="3.3V">
<contactref element="U$1" pad="P$10"/>
<contactref element="U$1" pad="P$11"/>
<contactref element="U$1" pad="P$8"/>
<contactref element="U$2" pad="P$5"/>
<contactref element="C2" pad="1"/>
<contactref element="U1" pad="18"/>
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="20"/>
<contactref element="R1" pad="2"/>
<contactref element="U$4" pad="P$3"/>
</signal>
<signal name="N$2">
<contactref element="U$1" pad="P$2"/>
<contactref element="U$1" pad="P$3"/>
<contactref element="U1" pad="27"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="P$4"/>
<contactref element="U1" pad="28"/>
</signal>
<signal name="N$1">
<contactref element="U$2" pad="P$1"/>
<contactref element="C1" pad="1"/>
<contactref element="U$2" pad="P$3"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="RST">
<contactref element="R1" pad="1"/>
<contactref element="U1" pad="29"/>
<contactref element="U$3" pad="P$1"/>
<contactref element="U$4" pad="P$6"/>
</signal>
<signal name="N$4">
<contactref element="U1" pad="15"/>
<contactref element="U$4" pad="P$2"/>
</signal>
<signal name="N$5">
<contactref element="U1" pad="16"/>
<contactref element="U$4" pad="P$4"/>
</signal>
<signal name="N$6">
<contactref element="U1" pad="17"/>
<contactref element="U$4" pad="P$5"/>
</signal>
<signal name="N$7">
<contactref element="U$1" pad="P$5"/>
<contactref element="U1" pad="26"/>
</signal>
<signal name="N$8">
<contactref element="U$1" pad="P$6"/>
<contactref element="U1" pad="25"/>
</signal>
<signal name="N$9">
<contactref element="U$1" pad="P$7"/>
<contactref element="U1" pad="24"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
