<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="60.706" y1="49.657" x2="0" y2="49.657" width="0" layer="20"/>
<wire x1="0" y1="49.657" x2="0" y2="-49.657" width="0" layer="20"/>
<text>Fast Out</text>
<text>Slow Out</text>
<text>Offset Adjust-Slow</text>
<text>Offset Adjust-Fast</text>
<text>1. Adjust board size to be smaller</text>
<text>2. Changed OP400 - U3's footprint to match the 16SOIC</text>
<text>3. Reroute traces to not be underneath (top layer) most of the chips</text>
<text>4. Changed Ground plane isolate to be 0.016</text>
<text>5. Replaced regulators</text>
<text>J000331H</text>
<text>2.2"</text>
<text>6. Adjust board size for enclosure</text>
<text>7. Mirrored Pot pins to be an accurate footprint</text>
<wire x1="60.706" y1="49.657" x2="60.706" y2="-49.657" width="0" layer="20"/>
<wire x1="0" y1="-49.657" x2="60.706" y2="-49.657" width="0" layer="20"/>
<text>8. Made fast path more of a short direct line to avoid any noise issues</text>
<text>9. Switched regulators to be smd components</text>
<text>10. Delete tant cap marking for regular ceramic caps</text>
<text>11. Changed font to be uniform and vector style</text>
<text>20161220</text>
<text>FIXED
ADJ</text>
<text>ADJ
FIXED</text>
<text>DUAL PMT AMP</text>
<hole x="1.27" y="0" drill="0.635"/>
<hole x="2.54" y="0" drill="0.635"/>
<hole x="6.35" y="0" drill="0.635"/>
<hole x="7.62" y="0" drill="0.635"/>
<hole x="11.43" y="0" drill="0.635"/>
<hole x="12.7" y="0" drill="0.635"/>
<hole x="13.97" y="0" drill="0.635"/>
<hole x="15.24" y="0" drill="0.635"/>
<hole x="16.51" y="0" drill="0.635"/>
<hole x="17.78" y="0" drill="0.635"/>
<hole x="19.05" y="0" drill="0.635"/>
<hole x="20.32" y="0" drill="0.635"/>
<hole x="21.59" y="0" drill="0.635"/>
<hole x="22.86" y="0" drill="0.635"/>
<hole x="24.13" y="0" drill="0.635"/>
<hole x="25.4" y="0" drill="0.635"/>
<hole x="26.67" y="0" drill="0.635"/>
<hole x="27.94" y="0" drill="0.635"/>
<hole x="29.21" y="0" drill="0.635"/>
<hole x="30.48" y="0" drill="0.635"/>
<hole x="31.75" y="0" drill="0.635"/>
<hole x="33.02" y="0" drill="0.635"/>
<hole x="34.29" y="0" drill="0.635"/>
<hole x="35.56" y="0" drill="0.635"/>
<hole x="36.83" y="0" drill="0.635"/>
<hole x="38.1" y="0" drill="0.635"/>
<hole x="39.37" y="0" drill="0.635"/>
<hole x="40.64" y="0" drill="0.635"/>
<hole x="41.91" y="0" drill="0.635"/>
<hole x="43.18" y="0" drill="0.635"/>
<hole x="44.45" y="0" drill="0.635"/>
<hole x="45.72" y="0" drill="0.635"/>
<hole x="46.99" y="0" drill="0.635"/>
<hole x="48.26" y="0" drill="0.635"/>
<hole x="49.53" y="0" drill="0.635"/>
<hole x="50.8" y="0" drill="0.635"/>
<hole x="52.07" y="0" drill="0.635"/>
<hole x="53.34" y="0" drill="0.635"/>
<hole x="54.61" y="0" drill="0.635"/>
<hole x="55.88" y="0" drill="0.635"/>
<hole x="57.15" y="0" drill="0.635"/>
<hole x="58.42" y="0" drill="0.635"/>
<hole x="59.69" y="0" drill="0.635"/>
<text>Fast Out</text>
<text>Slow Out</text>
<text>Offset Adjust-Slow</text>
<text>Offset Adjust-Fast</text>
<text>J000331H</text>
<text>20161220</text>
<text>FIXED
ADJ</text>
<text>ADJ
FIXED</text>
<text>DUAL PMT AMP</text>
<text>1. Adjust board size to be smaller</text>
<text>2. Changed OP400 - U3's footprint to match the 16SOIC</text>
<text>3. Reroute traces to not be underneath (top layer) most of the chips</text>
<text>4. Changed Ground plane isolate to be 0.016</text>
<text>5. Replaced regulators</text>
<text>6. Adjust board size for enclosure</text>
<text>7. Mirrored Pot pins to be an accurate footprint</text>
<text>8. Made fast path more of a short direct line to avoid any noise issues</text>
<text>9. Switched regulators to be smd components</text>
<text>10. Delete tant cap marking for regular ceramic caps</text>
<text>11. Changed font to be uniform and vector style</text>
</plain>
<libraries>
<library name="resistor">
<packages>
<package name="R1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="con-coax">
<packages>
<package name="AMP_227161">
<description>&lt;b&gt;JACK,  RIGHT ANGLE, 50 OHM, PCB, BNC&lt;/b&gt;&lt;p&gt;
Source: amp_227161.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun">
<packages>
<package name="SJ_3">
</package>
<package name="1X01">
</package>
<package name="1X02_LOCK">
</package>
</packages>
</library>
<library name="STEVES_BU">
<packages>
<package name="2512LONG">
</package>
<package name="LOGO_JANELIA_2014">
</package>
<package name="PJ-002">
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SO16L">
<description>&lt;b&gt;Small Outline Package 16&lt;/b&gt; large</description>
</package>
</packages>
</library>
<library name="jfrc">
<packages>
<package name="SOT89">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="analog-devices">
<description>&lt;b&gt;Analog Devices Components&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SO8">
<description>&lt;b&gt;8-Lead Small Outline IC&lt;/b&gt; (SO-8)&lt;p&gt;
Source: http://www.analog.com/UploadedFiles/Data_Sheets/703465986AD8611_2_0.pdf</description>
</package>
</packages>
</library>
<library name="rcl">
<description>&lt;b&gt;Resistors, Capacitors, Inductors&lt;/b&gt;&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;r.lbr
&lt;li&gt;cap.lbr 
&lt;li&gt;cap-fe.lbr
&lt;li&gt;captant.lbr
&lt;li&gt;polcap.lbr
&lt;li&gt;ipc-smd.lbr
&lt;/ul&gt;
All SMD packages are defined according to the IPC specifications and  CECC&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
for Electrolyt Capacitors see also :&lt;p&gt;
www.bccomponents.com &lt;p&gt;
www.panasonic.com&lt;p&gt;
www.kemet.com&lt;p&gt;
http://www.secc.co.jp/pdf/os_e/2004/e_os_all.pdf &lt;b&gt;(SANYO)&lt;/b&gt;
&lt;p&gt;
for trimmer refence see : &lt;u&gt;www.electrospec-inc.com/cross_references/trimpotcrossref.asp&lt;/u&gt;&lt;p&gt;

&lt;table border=0 cellspacing=0 cellpadding=0 width="100%" cellpaddding=0&gt;
&lt;tr valign="top"&gt;

&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;TRIM-POT CROSS REFERENCE&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;RECTANGULAR MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BOURNS&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BI&amp;nbsp;TECH&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;DALE-VISHAY&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PHILIPS/MEPCO&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MURATA&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PANASONIC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;SPECTROL&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MILSPEC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;&lt;TD&gt;&amp;nbsp;&lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3 &gt;
      3005P&lt;BR&gt;
      3006P&lt;BR&gt;
      3006W&lt;BR&gt;
      3006Y&lt;BR&gt;
      3009P&lt;BR&gt;
      3009W&lt;BR&gt;
      3009Y&lt;BR&gt;
      3057J&lt;BR&gt;
      3057L&lt;BR&gt;
      3057P&lt;BR&gt;
      3057Y&lt;BR&gt;
      3059J&lt;BR&gt;
      3059L&lt;BR&gt;
      3059P&lt;BR&gt;
      3059Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      89P&lt;BR&gt;
      89W&lt;BR&gt;
      89X&lt;BR&gt;
      89PH&lt;BR&gt;
      76P&lt;BR&gt;
      89XH&lt;BR&gt;
      78SLT&lt;BR&gt;
      78L&amp;nbsp;ALT&lt;BR&gt;
      56P&amp;nbsp;ALT&lt;BR&gt;
      78P&amp;nbsp;ALT&lt;BR&gt;
      T8S&lt;BR&gt;
      78L&lt;BR&gt;
      56P&lt;BR&gt;
      78P&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      T18/784&lt;BR&gt;
      783&lt;BR&gt;
      781&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2199&lt;BR&gt;
      1697/1897&lt;BR&gt;
      1680/1880&lt;BR&gt;
      2187&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      8035EKP/CT20/RJ-20P&lt;BR&gt;
      -&lt;BR&gt;
      RJ-20X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      1211L&lt;BR&gt;
      8012EKQ&amp;nbsp;ALT&lt;BR&gt;
      8012EKR&amp;nbsp;ALT&lt;BR&gt;
      1211P&lt;BR&gt;
      8012EKJ&lt;BR&gt;
      8012EKL&lt;BR&gt;
      8012EKQ&lt;BR&gt;
      8012EKR&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      2101P&lt;BR&gt;
      2101W&lt;BR&gt;
      2101Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2102L&lt;BR&gt;
      2102S&lt;BR&gt;
      2102Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVMCOG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      43P&lt;BR&gt;
      43W&lt;BR&gt;
      43Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      40L&lt;BR&gt;
      40P&lt;BR&gt;
      40Y&lt;BR&gt;
      70Y-T602&lt;BR&gt;
      70L&lt;BR&gt;
      70P&lt;BR&gt;
      70Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SQUARE MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
   &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3250L&lt;BR&gt;
      3250P&lt;BR&gt;
      3250W&lt;BR&gt;
      3250X&lt;BR&gt;
      3252P&lt;BR&gt;
      3252W&lt;BR&gt;
      3252X&lt;BR&gt;
      3260P&lt;BR&gt;
      3260W&lt;BR&gt;
      3260X&lt;BR&gt;
      3262P&lt;BR&gt;
      3262W&lt;BR&gt;
      3262X&lt;BR&gt;
      3266P&lt;BR&gt;
      3266W&lt;BR&gt;
      3266X&lt;BR&gt;
      3290H&lt;BR&gt;
      3290P&lt;BR&gt;
      3290W&lt;BR&gt;
      3292P&lt;BR&gt;
      3292W&lt;BR&gt;
      3292X&lt;BR&gt;
      3296P&lt;BR&gt;
      3296W&lt;BR&gt;
      3296X&lt;BR&gt;
      3296Y&lt;BR&gt;
      3296Z&lt;BR&gt;
      3299P&lt;BR&gt;
      3299W&lt;BR&gt;
      3299X&lt;BR&gt;
      3299Y&lt;BR&gt;
      3299Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64P&amp;nbsp;ALT&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      64X&amp;nbsp;ALT&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66P&lt;BR&gt;
      66W&lt;BR&gt;
      66X&lt;BR&gt;
      67P&lt;BR&gt;
      67W&lt;BR&gt;
      67X&lt;BR&gt;
      67Y&lt;BR&gt;
      67Z&lt;BR&gt;
      68P&lt;BR&gt;
      68W&lt;BR&gt;
      68X&lt;BR&gt;
      67Y&amp;nbsp;ALT&lt;BR&gt;
      67Z&amp;nbsp;ALT&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      5050&lt;BR&gt;
      5091&lt;BR&gt;
      5080&lt;BR&gt;
      5087&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T63YB&lt;BR&gt;
      T63XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      5887&lt;BR&gt;
      5891&lt;BR&gt;
      5880&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T93Z&lt;BR&gt;
      T93YA&lt;BR&gt;
      T93XA&lt;BR&gt;
      T93YB&lt;BR&gt;
      T93XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKW&lt;BR&gt;
      8026EKM&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKB&lt;BR&gt;
      8026EKM&lt;BR&gt;
      1309X&lt;BR&gt;
      1309P&lt;BR&gt;
      1309W&lt;BR&gt;
      8024EKP&lt;BR&gt;
      8024EKW&lt;BR&gt;
      8024EKN&lt;BR&gt;
      RJ-9P/CT9P&lt;BR&gt;
      RJ-9W&lt;BR&gt;
      RJ-9X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3105P/3106P&lt;BR&gt;
      3105W/3106W&lt;BR&gt;
      3105X/3106X&lt;BR&gt;
      3105Y/3106Y&lt;BR&gt;
      3105Z/3105Z&lt;BR&gt;
      3102P&lt;BR&gt;
      3102W&lt;BR&gt;
      3102X&lt;BR&gt;
      3102Y&lt;BR&gt;
      3102Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMCBG&lt;BR&gt;
      EVMCCG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      55-1-X&lt;BR&gt;
      55-4-X&lt;BR&gt;
      55-3-X&lt;BR&gt;
      55-2-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      50-2-X&lt;BR&gt;
      50-4-X&lt;BR&gt;
      50-3-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      64Y&lt;BR&gt;
      64Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3323P&lt;BR&gt;
      3323S&lt;BR&gt;
      3323W&lt;BR&gt;
      3329H&lt;BR&gt;
      3329P&lt;BR&gt;
      3329W&lt;BR&gt;
      3339H&lt;BR&gt;
      3339P&lt;BR&gt;
      3339W&lt;BR&gt;
      3352E&lt;BR&gt;
      3352H&lt;BR&gt;
      3352K&lt;BR&gt;
      3352P&lt;BR&gt;
      3352T&lt;BR&gt;
      3352V&lt;BR&gt;
      3352W&lt;BR&gt;
      3362H&lt;BR&gt;
      3362M&lt;BR&gt;
      3362P&lt;BR&gt;
      3362R&lt;BR&gt;
      3362S&lt;BR&gt;
      3362U&lt;BR&gt;
      3362W&lt;BR&gt;
      3362X&lt;BR&gt;
      3386B&lt;BR&gt;
      3386C&lt;BR&gt;
      3386F&lt;BR&gt;
      3386H&lt;BR&gt;
      3386K&lt;BR&gt;
      3386M&lt;BR&gt;
      3386P&lt;BR&gt;
      3386S&lt;BR&gt;
      3386W&lt;BR&gt;
      3386X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      25P&lt;BR&gt;
      25S&lt;BR&gt;
      25RX&lt;BR&gt;
      82P&lt;BR&gt;
      82M&lt;BR&gt;
      82PA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      91E&lt;BR&gt;
      91X&lt;BR&gt;
      91T&lt;BR&gt;
      91B&lt;BR&gt;
      91A&lt;BR&gt;
      91V&lt;BR&gt;
      91W&lt;BR&gt;
      25W&lt;BR&gt;
      25V&lt;BR&gt;
      25P&lt;BR&gt;
      -&lt;BR&gt;
      25S&lt;BR&gt;
      25U&lt;BR&gt;
      25RX&lt;BR&gt;
      25X&lt;BR&gt;
      72XW&lt;BR&gt;
      72XL&lt;BR&gt;
      72PM&lt;BR&gt;
      72RX&lt;BR&gt;
      -&lt;BR&gt;
      72PX&lt;BR&gt;
      72P&lt;BR&gt;
      72RXW&lt;BR&gt;
      72RXL&lt;BR&gt;
      72X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T7YB&lt;BR&gt;
      T7YA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      TXD&lt;BR&gt;
      TYA&lt;BR&gt;
      TYP&lt;BR&gt;
      -&lt;BR&gt;
      TYD&lt;BR&gt;
      TX&lt;BR&gt;
      -&lt;BR&gt;
      150SX&lt;BR&gt;
      100SX&lt;BR&gt;
      102T&lt;BR&gt;
      101S&lt;BR&gt;
      190T&lt;BR&gt;
      150TX&lt;BR&gt;
      101&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      101SX&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ET6P&lt;BR&gt;
      ET6S&lt;BR&gt;
      ET6X&lt;BR&gt;
      RJ-6W/8014EMW&lt;BR&gt;
      RJ-6P/8014EMP&lt;BR&gt;
      RJ-6X/8014EMX&lt;BR&gt;
      TM7W&lt;BR&gt;
      TM7P&lt;BR&gt;
      TM7X&lt;BR&gt;
      -&lt;BR&gt;
      8017SMS&lt;BR&gt;
      -&lt;BR&gt;
      8017SMB&lt;BR&gt;
      8017SMA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      CT-6W&lt;BR&gt;
      CT-6H&lt;BR&gt;
      CT-6P&lt;BR&gt;
      CT-6R&lt;BR&gt;
      -&lt;BR&gt;
      CT-6V&lt;BR&gt;
      CT-6X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKV&lt;BR&gt;
      -&lt;BR&gt;
      8038EKX&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKP&lt;BR&gt;
      8038EKZ&lt;BR&gt;
      8038EKW&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3321H&lt;BR&gt;
      3321P&lt;BR&gt;
      3321N&lt;BR&gt;
      1102H&lt;BR&gt;
      1102P&lt;BR&gt;
      1102T&lt;BR&gt;
      RVA0911V304A&lt;BR&gt;
      -&lt;BR&gt;
      RVA0911H413A&lt;BR&gt;
      RVG0707V100A&lt;BR&gt;
      RVA0607V(H)306A&lt;BR&gt;
      RVA1214H213A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3104B&lt;BR&gt;
      3104C&lt;BR&gt;
      3104F&lt;BR&gt;
      3104H&lt;BR&gt;
      -&lt;BR&gt;
      3104M&lt;BR&gt;
      3104P&lt;BR&gt;
      3104S&lt;BR&gt;
      3104W&lt;BR&gt;
      3104X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      EVMQ0G&lt;BR&gt;
      EVMQIG&lt;BR&gt;
      EVMQ3G&lt;BR&gt;
      EVMS0G&lt;BR&gt;
      EVMQ0G&lt;BR&gt;
      EVMG0G&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMK4GA00B&lt;BR&gt;
      EVM30GA00B&lt;BR&gt;
      EVMK0GA00B&lt;BR&gt;
      EVM38GA00B&lt;BR&gt;
      EVMB6&lt;BR&gt;
      EVLQ0&lt;BR&gt;
      -&lt;BR&gt;
      EVMMSG&lt;BR&gt;
      EVMMBG&lt;BR&gt;
      EVMMAG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMMCS&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM0&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM3&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      62-3-1&lt;BR&gt;
      62-1-2&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67R&lt;BR&gt;
      -&lt;BR&gt;
      67P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67X&lt;BR&gt;
      63V&lt;BR&gt;
      63S&lt;BR&gt;
      63M&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63H&lt;BR&gt;
      63P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;&amp;nbsp;&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=3&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT color="#0000FF" SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SMD TRIM-POT CROSS REFERENCE&lt;/B&gt;&lt;/FONT&gt;
      &lt;P&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3224G&lt;BR&gt;
      3224J&lt;BR&gt;
      3224W&lt;BR&gt;
      3269P&lt;BR&gt;
      3269W&lt;BR&gt;
      3269X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      44G&lt;BR&gt;
      44J&lt;BR&gt;
      44W&lt;BR&gt;
      84P&lt;BR&gt;
      84W&lt;BR&gt;
      84X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST63Z&lt;BR&gt;
      ST63Y&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST5P&lt;BR&gt;
      ST5W&lt;BR&gt;
      ST5X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3314G&lt;BR&gt;
      3314J&lt;BR&gt;
      3364A/B&lt;BR&gt;
      3364C/D&lt;BR&gt;
      3364W/X&lt;BR&gt;
      3313G&lt;BR&gt;
      3313J&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      23B&lt;BR&gt;
      23A&lt;BR&gt;
      21X&lt;BR&gt;
      21W&lt;BR&gt;
      -&lt;BR&gt;
      22B&lt;BR&gt;
      22A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST5YL/ST53YL&lt;BR&gt;
      ST5YJ/5T53YJ&lt;BR&gt;
      ST-23A&lt;BR&gt;
      ST-22B&lt;BR&gt;
      ST-22&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST-4B&lt;BR&gt;
      ST-4A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST-3B&lt;BR&gt;
      ST-3A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVM-6YS&lt;BR&gt;
      EVM-1E&lt;BR&gt;
      EVM-1G&lt;BR&gt;
      EVM-1D&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      G4B&lt;BR&gt;
      G4A&lt;BR&gt;
      TR04-3S1&lt;BR&gt;
      TRG04-2S1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      DVR-43A&lt;BR&gt;
      CVR-42C&lt;BR&gt;
      CVR-42A/C&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;
&lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;ALT =&amp;nbsp;ALTERNATE&lt;/B&gt;&lt;/FONT&gt;
&lt;P&gt;

&amp;nbsp;
&lt;P&gt;
&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;</description>
<packages>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="RTRIM3006P">
<description>&lt;b&gt;Trimm resistor&lt;/b&gt; BOURNS&lt;p&gt;</description>
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DO214BA">
<description>&lt;b&gt;DIODE&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R1" library="rcl" package="R0805" value="75">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RF1" library="resistor" package="R1206" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RIN1" library="rcl" package="R0805" value="0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CF1A" library="rcl" package="C1206" value="1p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CF1B" library="rcl" package="C1206" value="1p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="rcl" package="R0805" value="37.4k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="rcl" package="C0805" value="3.3n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="rcl" package="R0805" value="3.74k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="con-coax" package="AMP_227161" value="1-227161-0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MF" value="TE"/>
<attribute name="MPN" value="5413879-1"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="33B3200"/>
</element>
<element name="J2" library="con-coax" package="AMP_227161" value="1-227161-0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MF" value="TE"/>
<attribute name="MPN" value="5413879-1"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="33B3200"/>
</element>
<element name="C1" library="rcl" package="C1206" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="rcl" package="C1206" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="con-coax" package="AMP_227161" value="1-227161-0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MF" value="TE"/>
<attribute name="MPN" value="5413879-1"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="33B3200"/>
</element>
<element name="R100" library="rcl" package="R0805" value="0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R101" library="rcl" package="R0805" value="DNP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="rcl" package="RTRIM3006P" value="100k">
<attribute name="NAME"/>
<attribute name="MPN" value="3006P-1-104LF"/>
<attribute name="MF" value="BOURNS"/>
</element>
<element name="R7" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="rcl" package="R0805" value="3.74k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="STEVES_BU" package="2512LONG" value="49.9">
<attribute name="NAME"/>
</element>
<element name="C12" library="rcl" package="C0603" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="rcl" package="C0603" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="rcl" package="C0603" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="rcl" package="C0603" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="rcl" package="C0603" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="rcl" package="C0603" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="linear" package="SO16L" value="OP400">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="rcl" package="C0603" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="rcl" package="C0603" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FST1" library="SparkFun" package="SJ_3" value="">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="SLW1" library="SparkFun" package="SJ_3" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="rcl" package="C1206" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="rcl" package="C1206" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="V+" library="SparkFun" package="1X01" value="M01PTH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="V-" library="SparkFun" package="1X01" value="M01PTH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="OUT1" library="SparkFun" package="1X01" value="M01PTH">
<attribute name="VALUE"/>
</element>
<element name="U$1" library="STEVES_BU" package="LOGO_JANELIA_2014" value="JFRC-LOGOLOGO_JANELIA_2014"/>
<element name="U3" library="jfrc" package="SOT89" value="MC79L05ACHX">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="jfrc" package="SOT89" value="MC78L05ACHX">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="rcl" package="R0805" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="rcl" package="R0805" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C100" library="rcl" package="C0805" value="DNP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U4" library="analog-devices" package="SO8" value="OPA656">
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1838867"/>
<attribute name="MF" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U5" library="analog-devices" package="SO8" value="OPA656">
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1838867"/>
<attribute name="MF" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="STEVES_BU" package="PJ-002" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="STEVES_BU" package="PJ-002" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun" package="1X02_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="rcl" package="C0805" value="68n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="rcl" package="R0805" value="75">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RF2" library="resistor" package="R1206" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RIN2" library="rcl" package="R0805" value="0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CF2A" library="rcl" package="C1206" value="1p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CF2B" library="rcl" package="C1206" value="1p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R26" library="rcl" package="R0805" value="37.4k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C27" library="rcl" package="C0805" value="3.3n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R24" library="rcl" package="R0805" value="3.74k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J6" library="con-coax" package="AMP_227161" value="1-227161-0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MF" value="TE"/>
<attribute name="MPN" value="5413879-1"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="33B3200"/>
</element>
<element name="J7" library="con-coax" package="AMP_227161" value="1-227161-0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MF" value="TE"/>
<attribute name="MPN" value="5413879-1"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="33B3200"/>
</element>
<element name="C21" library="rcl" package="C1206" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C23" library="rcl" package="C1206" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J8" library="con-coax" package="AMP_227161" value="1-227161-0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MF" value="TE"/>
<attribute name="MPN" value="5413879-1"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="33B3200"/>
</element>
<element name="R200" library="rcl" package="R0805" value="0">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R201" library="rcl" package="R0805" value="DNP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R33" library="rcl" package="RTRIM3006P" value="100k">
<attribute name="NAME"/>
<attribute name="MPN" value="3006P-1-104LF"/>
<attribute name="MF" value="BOURNS"/>
</element>
<element name="R27" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R25" library="rcl" package="R0805" value="3.74k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R28" library="rcl" package="R0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="STEVES_BU" package="2512LONG" value="49.9">
<attribute name="NAME"/>
</element>
<element name="C32" library="rcl" package="C0603" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C33" library="rcl" package="C0603" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C30" library="rcl" package="C0603" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C31" library="rcl" package="C0603" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C29" library="rcl" package="C0603" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C28" library="rcl" package="C0603" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U6" library="linear" package="SO16L" value="OP400">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C35" library="rcl" package="C0603" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C34" library="rcl" package="C0603" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FST2" library="SparkFun" package="SJ_3" value="">
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="SLW2" library="SparkFun" package="SJ_3" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="VALUE"/>
</element>
<element name="C24" library="rcl" package="C1206" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="rcl" package="C1206" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="V2+" library="SparkFun" package="1X01" value="M01PTH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="V2-" library="SparkFun" package="1X01" value="M01PTH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="OUT2" library="SparkFun" package="1X01" value="M01PTH">
<attribute name="VALUE"/>
</element>
<element name="U$2" library="STEVES_BU" package="LOGO_JANELIA_2014" value="JFRC-LOGOLOGO_JANELIA_2014"/>
<element name="U7" library="jfrc" package="SOT89" value="MC79L05ACHX">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U8" library="jfrc" package="SOT89" value="MC78L05ACHX">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R31" library="rcl" package="R0805" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R30" library="rcl" package="R0805" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C200" library="rcl" package="C0805" value="DNP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U9" library="analog-devices" package="SO8" value="OPA656">
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1838867"/>
<attribute name="MF" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U10" library="analog-devices" package="SO8" value="OPA656">
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="1838867"/>
<attribute name="MF" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J9" library="STEVES_BU" package="PJ-002" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J10" library="STEVES_BU" package="PJ-002" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun" package="1X02_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C26" library="rcl" package="C0805" value="68n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="rcl" package="C0805" value="4.7n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="rcl" package="R0805" value="715">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="rcl" package="R0805" value="715">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C25" library="rcl" package="C0805" value="4.7n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R29" library="rcl" package="R0805" value="715">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R22" library="rcl" package="R0805" value="715">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="rcl" package="RTRIM3006P" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MPN" value="3006P-1-104LF"/>
<attribute name="MF" value="BOURNS"/>
</element>
<element name="R32" library="rcl" package="RTRIM3006P" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="MPN" value="3006P-1-104LF"/>
<attribute name="MF" value="BOURNS"/>
</element>
<element name="D1" library="diode" package="DO214BA" value="LSM115J"/>
<element name="D2" library="diode" package="DO214BA" value="LSM115J"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="RIN1" pad="2"/>
<contactref element="RF1" pad="1"/>
<contactref element="CF1A" pad="1"/>
<contactref element="CF1B" pad="1"/>
<contactref element="U4" pad="2"/>
</signal>
<signal name="GND">
<contactref element="J5" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="J4" pad="2"/>
<contactref element="J2" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C15" pad="1"/>
<contactref element="C14" pad="1"/>
<contactref element="FST1" pad="3"/>
<contactref element="C4" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C100" pad="2"/>
<contactref element="J3" pad="2"/>
<contactref element="J1" pad="1A"/>
<contactref element="J1" pad="1B"/>
<contactref element="JP1" pad="2"/>
<contactref element="U1" pad="2"/>
<contactref element="U1" pad="2@1"/>
<contactref element="U3" pad="1"/>
<contactref element="U2" pad="3"/>
<contactref element="C6" pad="2"/>
<contactref element="R101" pad="1"/>
<contactref element="J6" pad="2"/>
<contactref element="C21" pad="1"/>
<contactref element="C23" pad="2"/>
<contactref element="J8" pad="2"/>
<contactref element="J7" pad="2"/>
<contactref element="C32" pad="2"/>
<contactref element="C33" pad="2"/>
<contactref element="C30" pad="2"/>
<contactref element="C31" pad="2"/>
<contactref element="C29" pad="2"/>
<contactref element="C28" pad="2"/>
<contactref element="C35" pad="1"/>
<contactref element="C34" pad="1"/>
<contactref element="FST2" pad="3"/>
<contactref element="SLW2" pad="3"/>
<contactref element="C24" pad="2"/>
<contactref element="C22" pad="2"/>
<contactref element="C200" pad="2"/>
<contactref element="J9" pad="2"/>
<contactref element="J10" pad="1A"/>
<contactref element="J10" pad="1B"/>
<contactref element="JP2" pad="2"/>
<contactref element="U8" pad="2"/>
<contactref element="U8" pad="2@1"/>
<contactref element="U7" pad="1"/>
<contactref element="U6" pad="3"/>
<contactref element="C26" pad="2"/>
<contactref element="R201" pad="1"/>
<contactref element="C5" pad="2"/>
<contactref element="SLW1" pad="3"/>
<contactref element="R9" pad="1"/>
<contactref element="SLW1" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="FST1" pad="2"/>
<contactref element="C25" pad="2"/>
<contactref element="SLW2" pad="2"/>
<contactref element="R29" pad="1"/>
<contactref element="FST2" pad="2"/>
<contactref element="R22" pad="1"/>
<contactref element="D2" pad="A"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="N$8">
<contactref element="J5" pad="1"/>
<contactref element="RIN1" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="R1" pad="2"/>
<contactref element="C100" pad="1"/>
<contactref element="U5" pad="3"/>
</signal>
<signal name="N$10">
<contactref element="R100" pad="1"/>
<contactref element="R101" pad="2"/>
<contactref element="U5" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="C8" pad="1"/>
<contactref element="U2" pad="5"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="C7" pad="1"/>
<contactref element="U2" pad="2"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="C9" pad="1"/>
<contactref element="U2" pad="14"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="R6" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="R7" pad="1"/>
<contactref element="U2" pad="1"/>
</signal>
<signal name="FO1">
<contactref element="R3" pad="2"/>
<contactref element="J4" pad="1"/>
</signal>
<signal name="VIN-">
<contactref element="C1" pad="2"/>
<contactref element="J1" pad="2"/>
<contactref element="U3" pad="2"/>
<contactref element="U3" pad="2@1"/>
<contactref element="C21" pad="2"/>
<contactref element="J10" pad="2"/>
<contactref element="U7" pad="2"/>
<contactref element="U7" pad="2@1"/>
</signal>
<signal name="VIN+">
<contactref element="C3" pad="1"/>
<contactref element="J3" pad="1A"/>
<contactref element="J3" pad="1B"/>
<contactref element="U1" pad="3"/>
<contactref element="C23" pad="1"/>
<contactref element="J9" pad="1A"/>
<contactref element="J9" pad="1B"/>
<contactref element="U8" pad="3"/>
</signal>
<signal name="FAST1">
<contactref element="R3" pad="1"/>
<contactref element="R100" pad="2"/>
<contactref element="U5" pad="6"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="U2" pad="15"/>
<contactref element="U2" pad="16"/>
<contactref element="SLW1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="R8" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="U2" pad="11"/>
</signal>
<signal name="V+">
<contactref element="C4" pad="1"/>
<contactref element="V+" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="U4" pad="7"/>
<contactref element="U2" pad="4"/>
<contactref element="C15" pad="2"/>
<contactref element="C13" pad="1"/>
<contactref element="U5" pad="7"/>
<contactref element="R11" pad="2"/>
<contactref element="U1" pad="1"/>
<contactref element="R12" pad="1"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="V-">
<contactref element="C2" pad="1"/>
<contactref element="V-" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="U4" pad="4"/>
<contactref element="C12" pad="1"/>
<contactref element="U5" pad="4"/>
<contactref element="U2" pad="13"/>
<contactref element="C14" pad="2"/>
<contactref element="U3" pad="3"/>
<contactref element="R10" pad="1"/>
<contactref element="R12" pad="3"/>
</signal>
<signal name="FASTOUT1">
</signal>
<signal name="SLOWOUT1">
<contactref element="OUT1" pad="1"/>
<contactref element="U2" pad="10"/>
<contactref element="R8" pad="1"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="U4OUT1">
<contactref element="CF1B" pad="2"/>
<contactref element="CF1A" pad="2"/>
<contactref element="RF1" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="U4" pad="6"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$28">
<contactref element="R4" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="U2" pad="6"/>
<contactref element="U2" pad="7"/>
<contactref element="FST1" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="RIN2" pad="2"/>
<contactref element="RF2" pad="1"/>
<contactref element="CF2A" pad="1"/>
<contactref element="CF2B" pad="1"/>
<contactref element="U9" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="J6" pad="1"/>
<contactref element="RIN2" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="R21" pad="2"/>
<contactref element="C200" pad="1"/>
<contactref element="U10" pad="3"/>
</signal>
<signal name="N$15">
<contactref element="R200" pad="1"/>
<contactref element="R201" pad="2"/>
<contactref element="U10" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="C28" pad="1"/>
<contactref element="U6" pad="5"/>
<contactref element="R32" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="C27" pad="1"/>
<contactref element="U6" pad="2"/>
<contactref element="R25" pad="2"/>
</signal>
<signal name="N$20">
<contactref element="C29" pad="1"/>
<contactref element="U6" pad="14"/>
<contactref element="R33" pad="2"/>
</signal>
<signal name="N$21">
<contactref element="R26" pad="2"/>
<contactref element="C27" pad="2"/>
<contactref element="R27" pad="1"/>
<contactref element="U6" pad="1"/>
</signal>
<signal name="FO2">
<contactref element="R23" pad="2"/>
<contactref element="J8" pad="1"/>
</signal>
<signal name="N$22">
<contactref element="U6" pad="15"/>
<contactref element="U6" pad="16"/>
<contactref element="SLW2" pad="1"/>
</signal>
<signal name="N$23">
<contactref element="R28" pad="2"/>
<contactref element="R27" pad="2"/>
<contactref element="U6" pad="11"/>
</signal>
<signal name="FASTOUT2">
</signal>
<signal name="U9OUT1">
<contactref element="CF2B" pad="2"/>
<contactref element="CF2A" pad="2"/>
<contactref element="RF2" pad="2"/>
<contactref element="R21" pad="1"/>
<contactref element="U9" pad="6"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="N$26">
<contactref element="R24" pad="2"/>
<contactref element="R26" pad="1"/>
<contactref element="C26" pad="1"/>
<contactref element="R25" pad="1"/>
<contactref element="C25" pad="1"/>
</signal>
<signal name="N$27">
<contactref element="U6" pad="6"/>
<contactref element="U6" pad="7"/>
<contactref element="FST2" pad="1"/>
</signal>
<signal name="SLOWOUT2">
<contactref element="OUT2" pad="1"/>
<contactref element="U6" pad="10"/>
<contactref element="R28" pad="1"/>
<contactref element="J7" pad="1"/>
</signal>
<signal name="FAST2">
<contactref element="R23" pad="1"/>
<contactref element="R200" pad="2"/>
<contactref element="U10" pad="6"/>
<contactref element="R24" pad="1"/>
</signal>
<signal name="V2+">
<contactref element="C24" pad="1"/>
<contactref element="U8" pad="1"/>
<contactref element="V2+" pad="1"/>
<contactref element="C30" pad="1"/>
<contactref element="U9" pad="7"/>
<contactref element="U6" pad="4"/>
<contactref element="C35" pad="2"/>
<contactref element="C33" pad="1"/>
<contactref element="U10" pad="7"/>
<contactref element="R31" pad="2"/>
<contactref element="R32" pad="1"/>
<contactref element="D2" pad="C"/>
</signal>
<signal name="V2-">
<contactref element="C22" pad="1"/>
<contactref element="U7" pad="3"/>
<contactref element="R30" pad="1"/>
<contactref element="V2-" pad="1"/>
<contactref element="C31" pad="1"/>
<contactref element="U9" pad="4"/>
<contactref element="C32" pad="1"/>
<contactref element="U10" pad="4"/>
<contactref element="U6" pad="13"/>
<contactref element="C34" pad="2"/>
<contactref element="R32" pad="3"/>
</signal>
<signal name="N$29">
<contactref element="U2" pad="12"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="N$30">
<contactref element="U4" pad="3"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$31">
</signal>
<signal name="N$32">
</signal>
<signal name="N$33">
<contactref element="U6" pad="12"/>
<contactref element="R29" pad="2"/>
</signal>
<signal name="N$34">
<contactref element="U9" pad="3"/>
<contactref element="R22" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="R11" pad="1"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="R13" pad="3"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="N$24">
<contactref element="R31" pad="1"/>
<contactref element="R33" pad="1"/>
</signal>
<signal name="N$25">
<contactref element="R33" pad="3"/>
<contactref element="R30" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
