<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0.8128" y1="0" x2="27.94" y2="0" width="0" layer="20"/>
<wire x1="28.7528" y1="0.8128" x2="28.7528" y2="19.939" width="0" layer="20"/>
<wire x1="0" y1="19.939" x2="0" y2="10.3886" width="0" layer="46"/>
<text>BricksTer
8884bt</text>
<text>rev. 3</text>
<text>github.com/BTbricks</text>
<wire x1="0" y1="0.8128" x2="0.8128" y2="0" width="0" layer="20" curve="90"/>
<wire x1="27.94" y1="0" x2="28.7528" y2="0.8128" width="0" layer="20" curve="90"/>
<wire x1="0" y1="19.939" x2="0.8128" y2="20.7518" width="0" layer="46" curve="-90"/>
<wire x1="28.7528" y1="19.939" x2="27.94" y2="20.7518" width="0" layer="20" curve="90"/>
<wire x1="27.94" y1="20.7518" x2="0.8128" y2="20.7518" width="0" layer="46"/>
<text>github.com/BTbricks</text>
<text>rev. 3</text>
<wire x1="0" y1="0.8128" x2="0" y2="10.3886" width="0" layer="20"/>
</plain>
<libraries>
<library name="brickster">
<description>&lt;b&gt;BricksTer 8884bt Components&lt;/b&gt;&lt;br/&gt;
&lt;br /&gt;
More information: &lt;a href="https://github.com/codefox421/brickster"&gt;https://github.com/codefox421/brickster&lt;/a&gt;&lt;br /&gt;
&lt;br /&gt;
&lt;i&gt;Created by: Nick Iaconis&lt;/i&gt;</description>
<packages>
<package name="SOT223">
</package>
<package name="1206">
</package>
<package name="SO8">
</package>
<package name="0402">
</package>
<package name="CHIP-LTST">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X3-NS">
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-M">
</package>
<package name="OSHW-LOGO-M-MASK">
</package>
</packages>
</library>
<library name="bt_avr">
<description>&lt;b&gt;AVR Microcontrollers&lt;/b&gt;
&lt;p&gt;Created by Michael Shimniok &lt;a href="http://www.bot-thoughts.com/"&gt;www.bot-thoughts.com&lt;/a&gt;&lt;/b&gt;</description>
<packages>
<package name="14SOICN">
</package>
</packages>
</library>
<library name="codefox421-parts">
<description>&lt;b&gt;Codefox421's Useful Parts Library&lt;/b&gt;
&lt;p&gt;https://github.com/codefox421&lt;/p&gt;
&lt;author&gt;codefox421&lt;/author&gt;</description>
<packages>
<package name="VCT24">
</package>
<package name="HM-05/06/07">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="NCP1117ST33T3G" library="brickster" package="SOT223" value="IC_RT9164A">
<attribute name="NAME"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="2X3-NS" value="AVR_SPI_PRG_6NS"/>
<element name="LOGO1" library="SparkFun-Aesthetics" package="OSHW-LOGO-M" value="OSHW-LOGOM"/>
<element name="C2" library="brickster" package="1206" value="100µF">
<attribute name="VALUE"/>
</element>
<element name="Q1" library="brickster" package="SO8" value="DMHC3025LSD-13">
<attribute name="VALUE"/>
</element>
<element name="U5" library="bt_avr" package="14SOICN" value="ATtiny841">
<attribute name="VALUE"/>
</element>
<element name="U6" library="codefox421-parts" package="VCT24" value="LV8402GP-TE-L-H"/>
<element name="C3" library="brickster" package="0402" value="10nF">
<attribute name="VALUE"/>
</element>
<element name="C4" library="brickster" package="0402" value="0.1µF">
<attribute name="VALUE"/>
</element>
<element name="U2" library="codefox421-parts" package="HM-05/06/07" value="HM-06"/>
<element name="R1" library="brickster" package="0402" value="10k">
<attribute name="PARTNO" value="ERJ-3GEYJ103V"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="brickster" package="0402" value="3.3k">
<attribute name="PARTNO" value="ERJ-3GEYJ103V"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="brickster" package="0402" value="3.3k">
<attribute name="PARTNO" value="ERJ-3GEYJ103V"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="brickster" package="CHIP-LTST" value="LTST-C195TBKFKT">
<attribute name="VALUE"/>
</element>
<element name="C1" library="brickster" package="0402" value="0.1µF">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="J1" pad="6"/>
<contactref element="NCP1117ST33T3G" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="U6" pad="3"/>
<contactref element="U6" pad="4"/>
<contactref element="C4" pad="2"/>
<contactref element="U6" pad="18"/>
<contactref element="Q1" pad="P$3"/>
<contactref element="U5" pad="14"/>
<contactref element="U2" pad="12"/>
<contactref element="D1" pad="3"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="ATTX/BTRX">
<contactref element="U5" pad="12"/>
<contactref element="U2" pad="4"/>
</signal>
<signal name="A01">
<contactref element="U6" pad="1"/>
</signal>
<signal name="A02">
<contactref element="U6" pad="2"/>
</signal>
<signal name="B02">
<contactref element="U6" pad="6"/>
</signal>
<signal name="B01">
<contactref element="U6" pad="5"/>
</signal>
<signal name="AIN2">
<contactref element="U6" pad="14"/>
<contactref element="U5" pad="7"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="AIN1">
<contactref element="U6" pad="15"/>
<contactref element="U5" pad="6"/>
</signal>
<signal name="BIN1">
<contactref element="U6" pad="11"/>
<contactref element="U5" pad="9"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="BIN2">
<contactref element="U6" pad="10"/>
<contactref element="U5" pad="10"/>
</signal>
<signal name="!RESET">
<contactref element="J1" pad="5"/>
<contactref element="U5" pad="4"/>
<contactref element="U6" pad="16"/>
<contactref element="U6" pad="12"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="ATRX/BTTX">
<contactref element="U5" pad="11"/>
<contactref element="U2" pad="2"/>
</signal>
<signal name="3.3V">
<contactref element="NCP1117ST33T3G" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="J1" pad="2"/>
<contactref element="NCP1117ST33T3G" pad="4"/>
<contactref element="U6" pad="13"/>
<contactref element="U5" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="U2" pad="9"/>
</signal>
<signal name="VIN">
<contactref element="NCP1117ST33T3G" pad="3"/>
<contactref element="U6" pad="22"/>
<contactref element="U6" pad="23"/>
<contactref element="U6" pad="9"/>
<contactref element="U6" pad="8"/>
<contactref element="Q1" pad="P$7"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="PF_C1">
<contactref element="Q1" pad="P$4"/>
<contactref element="Q1" pad="P$5"/>
<contactref element="Q1" pad="P$2"/>
</signal>
<signal name="PF_C2">
<contactref element="Q1" pad="P$8"/>
<contactref element="Q1" pad="P$1"/>
<contactref element="Q1" pad="P$6"/>
</signal>
<signal name="N$15">
<contactref element="U6" pad="20"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="C3" pad="2"/>
<contactref element="U6" pad="19"/>
</signal>
<signal name="N$11">
<contactref element="U6" pad="21"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="U5" pad="13"/>
</signal>
<signal name="N$16">
<contactref element="U5" pad="8"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="LED">
<contactref element="R2" pad="2"/>
<contactref element="U2" pad="15"/>
<contactref element="U5" pad="3"/>
<contactref element="D1" pad="4"/>
</signal>
<signal name="N$3">
<contactref element="U2" pad="1"/>
<contactref element="U2" pad="3"/>
</signal>
<signal name="KEY">
<contactref element="U2" pad="16"/>
<contactref element="U5" pad="2"/>
</signal>
<signal name="!BTRST">
<contactref element="U2" pad="11"/>
<contactref element="U5" pad="5"/>
</signal>
<signal name="N$1">
<contactref element="R3" pad="1"/>
<contactref element="D1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="D1" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
