<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.4.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="37.77" y2="0" width="0" layer="20"/>
<wire x1="37.77" y1="0" x2="37.77" y2="12.69" width="0" layer="20"/>
<wire x1="37.77" y1="12.69" x2="0" y2="12.69" width="0" layer="20"/>
<wire x1="0" y1="12.69" x2="0" y2="0" width="0" layer="20"/>
<text>1</text>
<text>1</text>
<text>MPXH6400A</text>
<text>MPXH6400A</text>
<text>Todds board</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="MOLEX-1X2">
<description>&lt;h3&gt;Molex 2-Pin Plated Through-Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/2pin_molex_set_19iv10.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="con-lstb">
<description>&lt;b&gt;Pin Headers&lt;/b&gt;&lt;p&gt;
Naming:&lt;p&gt;
MA = male&lt;p&gt;
# contacts - # rows&lt;p&gt;
W = angled&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MA06-1">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X01">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="mpxh6400">
<description>&lt;h1&gt;Freescale MPXH6400&lt;/h1&gt;
MEMS pressure sensor
&lt;p&gt;Entered by &lt;a href="mailto:larwe@larwe.com"&gt;larwe@larwe.com&lt;/a&gt;&lt;/p&gt;</description>
<packages>
<package name="SSOP8">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Connectors" package="MOLEX-1X2" value="Cap C1">
<attribute name="SF_ID" value="PRT-09918"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0603" value="10M">
<attribute name="PROD_ID" value="RES-08283"/>
</element>
<element name="SV1" library="con-lstb" package="MA06-1" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="TOJS5" library="pinhead" package="1X01" value=""/>
<element name="U1" library="mpxh6400" package="SSOP8" value="MPXH6400AC6T1"/>
<element name="U2" library="mpxh6400" package="SSOP8" value="MPXH6400AC6T1"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="U2" pad="4"/>
<contactref element="SV1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="U2" pad="3"/>
<contactref element="SV1" pad="2"/>
<contactref element="J1" pad="2"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="4"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="R1" pad="2"/>
<contactref element="J1" pad="1"/>
<contactref element="TOJS5" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="U2" pad="2"/>
<contactref element="SV1" pad="3"/>
<contactref element="U1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
