<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="330.2" y2="0" width="0" layer="20"/>
<wire x1="330.2" y1="0" x2="330.2" y2="76.2" width="0" layer="20"/>
<wire x1="330.2" y1="76.2" x2="0" y2="76.2" width="0" layer="20"/>
<wire x1="0" y1="76.2" x2="0" y2="0" width="0" layer="20"/>
<text>+5V</text>
<text>GND</text>
<text>Temp Controller
v1.0   BJR</text>
<text>DAC VREF</text>
<text>VSET1</text>
<text>GND</text>
<hole x="6.35" y="69.85" drill="3.175"/>
<hole x="323.85" y="69.85" drill="3.175"/>
<hole x="254.635" y="64.77" drill="3.175"/>
<hole x="187.325" y="64.77" drill="3.175"/>
<hole x="120.015" y="64.77" drill="3.175"/>
<text>VSET2</text>
<text>VSET3</text>
<text>VSET4</text>
<text>P</text>
<text>1V</text>
<text>I</text>
<text>2.5V</text>
<text>P</text>
<text>1V</text>
<text>I</text>
<text>P</text>
<text>1V</text>
<text>I</text>
<text>P</text>
<text>1V</text>
<text>I</text>
<text>Cool Disable</text>
<text>Cool Disable</text>
<text>Cool Disable</text>
<text>Cool Disable</text>
<text>Heat Disable</text>
<text>Heat Disable</text>
<text>Heat Disable</text>
<text>Heat Disable</text>
<text>Ext Vref</text>
<text>Temp</text>
<text>Temp</text>
<text>Temp</text>
<text>Temp</text>
<text>Voltage</text>
<text>Voltage</text>
<text>Voltage</text>
<text>Voltage</text>
<text>VSET Protection Circuit</text>
<text>VSET Protection Circuit</text>
<text>VSET Protection Circuit</text>
<text>VSET Protection Circuit</text>
<text>Max V</text>
<text>Max V</text>
<text>Max V</text>
<text>Max V</text>
<text>Min V</text>
<text>Min V</text>
<text>Min V</text>
<text>Min V</text>
<text>Int Vref</text>
</plain>
<libraries>
<library name="rlc-jqi">
<packages>
<package name="0603">
<description>0603 SMT Package</description>
</package>
<package name="0805">
<description>0805 SMT Package</description>
</package>
</packages>
</library>
<library name="mcu-accessories">
<packages>
<package name="TEENSY_3.1+4">
</package>
<package name="ML08">
</package>
</packages>
</library>
<library name="jqi_passives">
<description>Library originally designed by Joshua Bienfang NIST.
Pad's sizes are slightly smaller than Eagle's default producing an artwork that is more compact.

Symbols are also compact, but still fit on a standard .1'' grid. 
Additional passive components (RLC and trimpots) can be added.</description>
<packages>
<package name="R_0603">
</package>
</packages>
</library>
<library name="Lin-Temp-Controller">
<packages>
<package name="MSOP10">
<description>&lt;b&gt;MSOP10&lt;/b&gt; MSE Package 10-Lead Plastic MSOP (Reference LTC DWG # 05-08-1664)&lt;p&gt;
Auto generated by &lt;i&gt;make-symbol-device-package-bsdl.ulp Rev. 43&lt;/i&gt;&lt;br&gt;
Source: &lt;a href="http://cds.linear.com/docs/Datasheet/3592fc.pdf"&gt; Data sheet &lt;/a&gt;</description>
</package>
<package name="1206TESTPAD">
</package>
<package name="1X02_SCRWTRM">
<description>&lt;b&gt;1x02 Screw Terminal Block&lt;/b&gt; 
&lt;p&gt; wire horizontal wrt board 
&lt;p&gt;Digikey: ED2635-ND
&lt;p&gt; MFN PN: OSTTE020161</description>
</package>
<package name="SOT-23">
</package>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package 8&lt;/b&gt;&lt;br&gt;
NS Package M08A</description>
</package>
<package name="64WPOT">
</package>
<package name="E-SWITCH-100-M7">
</package>
<package name="HLMP--F0010">
<description>Subminiature right angle indicator from Avago Technologies
&lt;p&gt;Digikey PN: 516-1417-ND</description>
</package>
<package name="TSSOP16">
<description>&lt;b&gt;16-Lead Thin Shrink Small Outline Package&lt;/b&gt; [TSSOP] (RU-16)&lt;p&gt;
Source: 8x ADG1408_1409.pdf</description>
</package>
</packages>
</library>
<library name="rcl">
<description>&lt;b&gt;Resistors, Capacitors, Inductors&lt;/b&gt;&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;r.lbr
&lt;li&gt;cap.lbr 
&lt;li&gt;cap-fe.lbr
&lt;li&gt;captant.lbr
&lt;li&gt;polcap.lbr
&lt;li&gt;ipc-smd.lbr
&lt;/ul&gt;
All SMD packages are defined according to the IPC specifications and  CECC&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
for Electrolyt Capacitors see also :&lt;p&gt;
www.bccomponents.com &lt;p&gt;
www.panasonic.com&lt;p&gt;
www.kemet.com&lt;p&gt;
http://www.secc.co.jp/pdf/os_e/2004/e_os_all.pdf &lt;b&gt;(SANYO)&lt;/b&gt;
&lt;p&gt;
for trimmer refence see : &lt;u&gt;www.electrospec-inc.com/cross_references/trimpotcrossref.asp&lt;/u&gt;&lt;p&gt;

&lt;table border=0 cellspacing=0 cellpadding=0 width="100%" cellpaddding=0&gt;
&lt;tr valign="top"&gt;

&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;TRIM-POT CROSS REFERENCE&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;RECTANGULAR MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BOURNS&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BI&amp;nbsp;TECH&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;DALE-VISHAY&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PHILIPS/MEPCO&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MURATA&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PANASONIC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;SPECTROL&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MILSPEC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;&lt;TD&gt;&amp;nbsp;&lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3 &gt;
      3005P&lt;BR&gt;
      3006P&lt;BR&gt;
      3006W&lt;BR&gt;
      3006Y&lt;BR&gt;
      3009P&lt;BR&gt;
      3009W&lt;BR&gt;
      3009Y&lt;BR&gt;
      3057J&lt;BR&gt;
      3057L&lt;BR&gt;
      3057P&lt;BR&gt;
      3057Y&lt;BR&gt;
      3059J&lt;BR&gt;
      3059L&lt;BR&gt;
      3059P&lt;BR&gt;
      3059Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      89P&lt;BR&gt;
      89W&lt;BR&gt;
      89X&lt;BR&gt;
      89PH&lt;BR&gt;
      76P&lt;BR&gt;
      89XH&lt;BR&gt;
      78SLT&lt;BR&gt;
      78L&amp;nbsp;ALT&lt;BR&gt;
      56P&amp;nbsp;ALT&lt;BR&gt;
      78P&amp;nbsp;ALT&lt;BR&gt;
      T8S&lt;BR&gt;
      78L&lt;BR&gt;
      56P&lt;BR&gt;
      78P&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      T18/784&lt;BR&gt;
      783&lt;BR&gt;
      781&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2199&lt;BR&gt;
      1697/1897&lt;BR&gt;
      1680/1880&lt;BR&gt;
      2187&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      8035EKP/CT20/RJ-20P&lt;BR&gt;
      -&lt;BR&gt;
      RJ-20X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      1211L&lt;BR&gt;
      8012EKQ&amp;nbsp;ALT&lt;BR&gt;
      8012EKR&amp;nbsp;ALT&lt;BR&gt;
      1211P&lt;BR&gt;
      8012EKJ&lt;BR&gt;
      8012EKL&lt;BR&gt;
      8012EKQ&lt;BR&gt;
      8012EKR&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      2101P&lt;BR&gt;
      2101W&lt;BR&gt;
      2101Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2102L&lt;BR&gt;
      2102S&lt;BR&gt;
      2102Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVMCOG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      43P&lt;BR&gt;
      43W&lt;BR&gt;
      43Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      40L&lt;BR&gt;
      40P&lt;BR&gt;
      40Y&lt;BR&gt;
      70Y-T602&lt;BR&gt;
      70L&lt;BR&gt;
      70P&lt;BR&gt;
      70Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SQUARE MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
   &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3250L&lt;BR&gt;
      3250P&lt;BR&gt;
      3250W&lt;BR&gt;
      3250X&lt;BR&gt;
      3252P&lt;BR&gt;
      3252W&lt;BR&gt;
      3252X&lt;BR&gt;
      3260P&lt;BR&gt;
      3260W&lt;BR&gt;
      3260X&lt;BR&gt;
      3262P&lt;BR&gt;
      3262W&lt;BR&gt;
      3262X&lt;BR&gt;
      3266P&lt;BR&gt;
      3266W&lt;BR&gt;
      3266X&lt;BR&gt;
      3290H&lt;BR&gt;
      3290P&lt;BR&gt;
      3290W&lt;BR&gt;
      3292P&lt;BR&gt;
      3292W&lt;BR&gt;
      3292X&lt;BR&gt;
      3296P&lt;BR&gt;
      3296W&lt;BR&gt;
      3296X&lt;BR&gt;
      3296Y&lt;BR&gt;
      3296Z&lt;BR&gt;
      3299P&lt;BR&gt;
      3299W&lt;BR&gt;
      3299X&lt;BR&gt;
      3299Y&lt;BR&gt;
      3299Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64P&amp;nbsp;ALT&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      64X&amp;nbsp;ALT&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66P&lt;BR&gt;
      66W&lt;BR&gt;
      66X&lt;BR&gt;
      67P&lt;BR&gt;
      67W&lt;BR&gt;
      67X&lt;BR&gt;
      67Y&lt;BR&gt;
      67Z&lt;BR&gt;
      68P&lt;BR&gt;
      68W&lt;BR&gt;
      68X&lt;BR&gt;
      67Y&amp;nbsp;ALT&lt;BR&gt;
      67Z&amp;nbsp;ALT&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      5050&lt;BR&gt;
      5091&lt;BR&gt;
      5080&lt;BR&gt;
      5087&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T63YB&lt;BR&gt;
      T63XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      5887&lt;BR&gt;
      5891&lt;BR&gt;
      5880&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T93Z&lt;BR&gt;
      T93YA&lt;BR&gt;
      T93XA&lt;BR&gt;
      T93YB&lt;BR&gt;
      T93XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKW&lt;BR&gt;
      8026EKM&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKB&lt;BR&gt;
      8026EKM&lt;BR&gt;
      1309X&lt;BR&gt;
      1309P&lt;BR&gt;
      1309W&lt;BR&gt;
      8024EKP&lt;BR&gt;
      8024EKW&lt;BR&gt;
      8024EKN&lt;BR&gt;
      RJ-9P/CT9P&lt;BR&gt;
      RJ-9W&lt;BR&gt;
      RJ-9X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3105P/3106P&lt;BR&gt;
      3105W/3106W&lt;BR&gt;
      3105X/3106X&lt;BR&gt;
      3105Y/3106Y&lt;BR&gt;
      3105Z/3105Z&lt;BR&gt;
      3102P&lt;BR&gt;
      3102W&lt;BR&gt;
      3102X&lt;BR&gt;
      3102Y&lt;BR&gt;
      3102Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMCBG&lt;BR&gt;
      EVMCCG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      55-1-X&lt;BR&gt;
      55-4-X&lt;BR&gt;
      55-3-X&lt;BR&gt;
      55-2-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      50-2-X&lt;BR&gt;
      50-4-X&lt;BR&gt;
      50-3-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      64Y&lt;BR&gt;
      64Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3323P&lt;BR&gt;
      3323S&lt;BR&gt;
      3323W&lt;BR&gt;
      3329H&lt;BR&gt;
      3329P&lt;BR&gt;
      3329W&lt;BR&gt;
      3339H&lt;BR&gt;
      3339P&lt;BR&gt;
      3339W&lt;BR&gt;
      3352E&lt;BR&gt;
      3352H&lt;BR&gt;
      3352K&lt;BR&gt;
      3352P&lt;BR&gt;
      3352T&lt;BR&gt;
      3352V&lt;BR&gt;
      3352W&lt;BR&gt;
      3362H&lt;BR&gt;
      3362M&lt;BR&gt;
      3362P&lt;BR&gt;
      3362R&lt;BR&gt;
      3362S&lt;BR&gt;
      3362U&lt;BR&gt;
      3362W&lt;BR&gt;
      3362X&lt;BR&gt;
      3386B&lt;BR&gt;
      3386C&lt;BR&gt;
      3386F&lt;BR&gt;
      3386H&lt;BR&gt;
      3386K&lt;BR&gt;
      3386M&lt;BR&gt;
      3386P&lt;BR&gt;
      3386S&lt;BR&gt;
      3386W&lt;BR&gt;
      3386X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      25P&lt;BR&gt;
      25S&lt;BR&gt;
      25RX&lt;BR&gt;
      82P&lt;BR&gt;
      82M&lt;BR&gt;
      82PA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      91E&lt;BR&gt;
      91X&lt;BR&gt;
      91T&lt;BR&gt;
      91B&lt;BR&gt;
      91A&lt;BR&gt;
      91V&lt;BR&gt;
      91W&lt;BR&gt;
      25W&lt;BR&gt;
      25V&lt;BR&gt;
      25P&lt;BR&gt;
      -&lt;BR&gt;
      25S&lt;BR&gt;
      25U&lt;BR&gt;
      25RX&lt;BR&gt;
      25X&lt;BR&gt;
      72XW&lt;BR&gt;
      72XL&lt;BR&gt;
      72PM&lt;BR&gt;
      72RX&lt;BR&gt;
      -&lt;BR&gt;
      72PX&lt;BR&gt;
      72P&lt;BR&gt;
      72RXW&lt;BR&gt;
      72RXL&lt;BR&gt;
      72X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T7YB&lt;BR&gt;
      T7YA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      TXD&lt;BR&gt;
      TYA&lt;BR&gt;
      TYP&lt;BR&gt;
      -&lt;BR&gt;
      TYD&lt;BR&gt;
      TX&lt;BR&gt;
      -&lt;BR&gt;
      150SX&lt;BR&gt;
      100SX&lt;BR&gt;
      102T&lt;BR&gt;
      101S&lt;BR&gt;
      190T&lt;BR&gt;
      150TX&lt;BR&gt;
      101&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      101SX&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ET6P&lt;BR&gt;
      ET6S&lt;BR&gt;
      ET6X&lt;BR&gt;
      RJ-6W/8014EMW&lt;BR&gt;
      RJ-6P/8014EMP&lt;BR&gt;
      RJ-6X/8014EMX&lt;BR&gt;
      TM7W&lt;BR&gt;
      TM7P&lt;BR&gt;
      TM7X&lt;BR&gt;
      -&lt;BR&gt;
      8017SMS&lt;BR&gt;
      -&lt;BR&gt;
      8017SMB&lt;BR&gt;
      8017SMA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      CT-6W&lt;BR&gt;
      CT-6H&lt;BR&gt;
      CT-6P&lt;BR&gt;
      CT-6R&lt;BR&gt;
      -&lt;BR&gt;
      CT-6V&lt;BR&gt;
      CT-6X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKV&lt;BR&gt;
      -&lt;BR&gt;
      8038EKX&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKP&lt;BR&gt;
      8038EKZ&lt;BR&gt;
      8038EKW&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3321H&lt;BR&gt;
      3321P&lt;BR&gt;
      3321N&lt;BR&gt;
      1102H&lt;BR&gt;
      1102P&lt;BR&gt;
      1102T&lt;BR&gt;
      RVA0911V304A&lt;BR&gt;
      -&lt;BR&gt;
      RVA0911H413A&lt;BR&gt;
      RVG0707V100A&lt;BR&gt;
      RVA0607V(H)306A&lt;BR&gt;
      RVA1214H213A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3104B&lt;BR&gt;
      3104C&lt;BR&gt;
      3104F&lt;BR&gt;
      3104H&lt;BR&gt;
      -&lt;BR&gt;
      3104M&lt;BR&gt;
      3104P&lt;BR&gt;
      3104S&lt;BR&gt;
      3104W&lt;BR&gt;
      3104X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      EVMQ0G&lt;BR&gt;
      EVMQIG&lt;BR&gt;
      EVMQ3G&lt;BR&gt;
      EVMS0G&lt;BR&gt;
      EVMQ0G&lt;BR&gt;
      EVMG0G&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMK4GA00B&lt;BR&gt;
      EVM30GA00B&lt;BR&gt;
      EVMK0GA00B&lt;BR&gt;
      EVM38GA00B&lt;BR&gt;
      EVMB6&lt;BR&gt;
      EVLQ0&lt;BR&gt;
      -&lt;BR&gt;
      EVMMSG&lt;BR&gt;
      EVMMBG&lt;BR&gt;
      EVMMAG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMMCS&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM0&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM3&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      62-3-1&lt;BR&gt;
      62-1-2&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67R&lt;BR&gt;
      -&lt;BR&gt;
      67P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67X&lt;BR&gt;
      63V&lt;BR&gt;
      63S&lt;BR&gt;
      63M&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63H&lt;BR&gt;
      63P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;&amp;nbsp;&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=3&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT color="#0000FF" SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SMD TRIM-POT CROSS REFERENCE&lt;/B&gt;&lt;/FONT&gt;
      &lt;P&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3224G&lt;BR&gt;
      3224J&lt;BR&gt;
      3224W&lt;BR&gt;
      3269P&lt;BR&gt;
      3269W&lt;BR&gt;
      3269X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      44G&lt;BR&gt;
      44J&lt;BR&gt;
      44W&lt;BR&gt;
      84P&lt;BR&gt;
      84W&lt;BR&gt;
      84X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST63Z&lt;BR&gt;
      ST63Y&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST5P&lt;BR&gt;
      ST5W&lt;BR&gt;
      ST5X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3314G&lt;BR&gt;
      3314J&lt;BR&gt;
      3364A/B&lt;BR&gt;
      3364C/D&lt;BR&gt;
      3364W/X&lt;BR&gt;
      3313G&lt;BR&gt;
      3313J&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      23B&lt;BR&gt;
      23A&lt;BR&gt;
      21X&lt;BR&gt;
      21W&lt;BR&gt;
      -&lt;BR&gt;
      22B&lt;BR&gt;
      22A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST5YL/ST53YL&lt;BR&gt;
      ST5YJ/5T53YJ&lt;BR&gt;
      ST-23A&lt;BR&gt;
      ST-22B&lt;BR&gt;
      ST-22&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST-4B&lt;BR&gt;
      ST-4A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST-3B&lt;BR&gt;
      ST-3A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVM-6YS&lt;BR&gt;
      EVM-1E&lt;BR&gt;
      EVM-1G&lt;BR&gt;
      EVM-1D&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      G4B&lt;BR&gt;
      G4A&lt;BR&gt;
      TR04-3S1&lt;BR&gt;
      TRG04-2S1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      DVR-43A&lt;BR&gt;
      CVR-42C&lt;BR&gt;
      CVR-42A/C&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;
&lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;ALT =&amp;nbsp;ALTERNATE&lt;/B&gt;&lt;/FONT&gt;
&lt;P&gt;

&amp;nbsp;
&lt;P&gt;
&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;</description>
<packages>
<package name="PANASONIC_F">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package F&lt;/b&gt;</description>
</package>
<package name="CT7343">
<description>&lt;b&gt;TANTALUM CAPACITOR&lt;/b&gt;</description>
</package>
<package name="C0805K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0805 reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 2012</description>
</package>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2X06/90">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="connector-jqi">
<packages>
<package name="BNC90">
<description>Right angle BNC. AMP_227161.</description>
</package>
<package name="PEC092320FS">
<description>PC Pin layout for Bourns rotary encoder PEC09-2320F-S0015.</description>
</package>
</packages>
</library>
<library name="JQI_Logo">
<description>Connectors &amp; Components for PTS &amp; PulseBlaster related boards</description>
<packages>
<package name="JQI_LOGO_NEGATIVE-SILKSCREEN">
<description>JQI Logo, Silkscreen background with lettering showing stop mask</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="rlc-jqi" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="rlc-jqi" package="0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="mcu-accessories" package="TEENSY_3.1+4" value="TEENSY_3.1+4">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L2" library="rlc-jqi" package="0805" value="Ferrite 1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="jqi_passives" package="R_0603" value="10k 1%">
<attribute name="NAME"/>
</element>
<element name="R21" library="jqi_passives" package="R_0603" value="10k 1%">
<attribute name="NAME"/>
</element>
<element name="R22" library="jqi_passives" package="R_0603" value="10k 1%">
<attribute name="NAME"/>
</element>
<element name="R23" library="jqi_passives" package="R_0603" value="10k 1%">
<attribute name="NAME"/>
</element>
<element name="R24" library="jqi_passives" package="R_0603" value="10k 1%">
<attribute name="NAME"/>
</element>
<element name="R25" library="jqi_passives" package="R_0603" value="10k 1%">
<attribute name="NAME"/>
</element>
<element name="R26" library="jqi_passives" package="R_0603" value="10k 1%">
<attribute name="NAME"/>
</element>
<element name="R27" library="jqi_passives" package="R_0603" value="10k 1%">
<attribute name="NAME"/>
</element>
<element name="C9" library="rlc-jqi" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="rlc-jqi" package="0603" value="1000pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="rlc-jqi" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="rlc-jqi" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="rlc-jqi" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="rlc-jqi" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="rlc-jqi" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="rlc-jqi" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="rlc-jqi" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L3" library="rlc-jqi" package="0805" value="Ferrite 1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC3" library="Lin-Temp-Controller" package="MSOP10" value="AD5624R">
<attribute name="DIGIKEY" value="AD5624RBRMZ-3-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C27" library="rlc-jqi" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C30" library="rlc-jqi" package="0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="rlc-jqi" package="0805" value="Ferrite 1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP1" library="Lin-Temp-Controller" package="1206TESTPAD" value="TESTPT">
<attribute name="NAME"/>
</element>
<element name="CP1" library="rcl" package="PANASONIC_F" value="220uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CP3" library="rcl" package="CT7343" value="47uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CP2" library="rcl" package="C0805K" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP4" library="Lin-Temp-Controller" package="1X02_SCRWTRM" value="">
<attribute name="MFR_PN" value="OSTTE020161"/>
<attribute name="DIGIKEY" value="ED2635-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L4" library="rlc-jqi" package="0805" value="Ferrite 1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="pinhead" package="2X06/90" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="rlc-jqi" package="0603" value="4.3k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="rlc-jqi" package="0603" value="1.5k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP5" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="rlc-jqi" package="0603" value="4.3k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="rlc-jqi" package="0603" value="1.5k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T1" library="Lin-Temp-Controller" package="SOT-23" value="MMBT3904">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY" value="MMBT3904-FDICT-ND"/>
</element>
<element name="T2" library="Lin-Temp-Controller" package="SOT-23" value="MMBT3904">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY" value="MMBT3904-FDICT-ND"/>
</element>
<element name="IC1" library="Lin-Temp-Controller" package="SO08" value="LM393D">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY" value="296-1015-5-ND"/>
</element>
<element name="R6" library="Lin-Temp-Controller" package="64WPOT" value="10k">
<attribute name="DIGIKEY" value="987-1061-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="Lin-Temp-Controller" package="64WPOT" value="10k">
<attribute name="DIGIKEY" value="987-1061-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="rlc-jqi" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="rlc-jqi" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="rlc-jqi" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="rlc-jqi" package="0603" value="33k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="rlc-jqi" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="rlc-jqi" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP2" library="Lin-Temp-Controller" package="1206TESTPAD" value="TESTPT">
<attribute name="NAME"/>
</element>
<element name="TP3" library="Lin-Temp-Controller" package="1206TESTPAD" value="TESTPT">
<attribute name="NAME"/>
</element>
<element name="S1" library="Lin-Temp-Controller" package="E-SWITCH-100-M7" value="">
<attribute name="MFR_PN" value="100DP1T2B4M7QE"/>
<attribute name="DIGIKEY" value="100DP1T2B4M7QE-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="Lin-Temp-Controller" package="HLMP--F0010" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY" value="516-1417-ND"/>
</element>
<element name="R5" library="rlc-jqi" package="0603" value="330">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC4" library="Lin-Temp-Controller" package="TSSOP16" value="AD5262">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY" value="AD5262BRUZ200-ND"/>
</element>
<element name="C12" library="rlc-jqi" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="rlc-jqi" package="0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP4" library="Lin-Temp-Controller" package="1206TESTPAD" value="TESTPT">
<attribute name="NAME"/>
</element>
<element name="TP5" library="Lin-Temp-Controller" package="1206TESTPAD" value="TESTPT">
<attribute name="NAME"/>
</element>
<element name="TP6" library="Lin-Temp-Controller" package="1206TESTPAD" value="TESTPT">
<attribute name="NAME"/>
</element>
<element name="X1" library="connector-jqi" package="BNC90" value="BNC-H">
<attribute name="DIGIKEY" value="A32260-ND"/>
<attribute name="NAME"/>
</element>
<element name="X2" library="connector-jqi" package="BNC90" value="BNC-H">
<attribute name="DIGIKEY" value="A32260-ND"/>
<attribute name="NAME"/>
</element>
<element name="IC6" library="Lin-Temp-Controller" package="SOT-23" value="">
<attribute name="DIGIKEY" value="TS6001BIG325TCT-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="rlc-jqi" package="0603" value="1000pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="rlc-jqi" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP7" library="Lin-Temp-Controller" package="1206TESTPAD" value="TESTPT">
<attribute name="NAME"/>
</element>
<element name="R14" library="rlc-jqi" package="0603" value="1.0k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="rlc-jqi" package="0603" value="1.0k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="rlc-jqi" package="0603" value="1.0k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP8" library="Lin-Temp-Controller" package="1206TESTPAD" value="TESTPT">
<attribute name="NAME"/>
</element>
<element name="ENC1" library="connector-jqi" package="PEC092320FS" value="PEC09"/>
<element name="R19" library="rlc-jqi" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R28" library="jqi_passives" package="R_0603" value="10k">
<attribute name="NAME"/>
</element>
<element name="R29" library="rlc-jqi" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="rcl" package="C0603" value="10nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="rcl" package="C0603" value="10nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R30" library="rlc-jqi" package="0603" value="50">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R31" library="rlc-jqi" package="0603" value="50">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ENC2" library="connector-jqi" package="PEC092320FS" value="PEC09"/>
<element name="R32" library="rlc-jqi" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R33" library="jqi_passives" package="R_0603" value="10k">
<attribute name="NAME"/>
</element>
<element name="R34" library="rlc-jqi" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="rcl" package="C0603" value="10nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C19" library="rcl" package="C0603" value="10nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R35" library="rlc-jqi" package="0603" value="50">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R36" library="rlc-jqi" package="0603" value="50">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="pinhead" package="2X06/90" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R37" library="rlc-jqi" package="0603" value="4.3k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R38" library="rlc-jqi" package="0603" value="1.5k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP6" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP7" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R39" library="rlc-jqi" package="0603" value="4.3k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R40" library="rlc-jqi" package="0603" value="1.5k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T3" library="Lin-Temp-Controller" package="SOT-23" value="MMBT3904">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY" value="MMBT3904-FDICT-ND"/>
</element>
<element name="T4" library="Lin-Temp-Controller" package="SOT-23" value="MMBT3904">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY" value="MMBT3904-FDICT-ND"/>
</element>
<element name="IC2" library="Lin-Temp-Controller" package="SO08" value="LM393D">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY" value="296-1015-5-ND"/>
</element>
<element name="R41" library="Lin-Temp-Controller" package="64WPOT" value="10k">
<attribute name="DIGIKEY" value="987-1061-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R42" library="Lin-Temp-Controller" package="64WPOT" value="10k">
<attribute name="DIGIKEY" value="987-1061-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R43" library="rlc-jqi" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R44" library="rlc-jqi" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R45" library="rlc-jqi" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R46" library="rlc-jqi" package="0603" value="33k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R47" library="rlc-jqi" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R48" library="rlc-jqi" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP9" library="Lin-Temp-Controller" package="1206TESTPAD" value="TESTPT">
<attribute name="NAME"/>
</element>
<element name="TP10" library="Lin-Temp-Controller" package="1206TESTPAD" value="TESTPT">
<attribute name="NAME"/>
</element>
<element name="S2" library="Lin-Temp-Controller" package="E-SWITCH-100-M7" value="">
<attribute name="MFR_PN" value="100DP1T2B4M7QE"/>
<attribute name="DIGIKEY" value="100DP1T2B4M7QE-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="Lin-Temp-Controller" package="HLMP--F0010" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY" value="516-1417-ND"/>
</element>
<element name="R49" library="rlc-jqi" package="0603" value="330">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC5" library="Lin-Temp-Controller" package="TSSOP16" value="AD5262">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY" value="AD5262BRUZ200-ND"/>
</element>
<element name="C20" library="rlc-jqi" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C21" library="rlc-jqi" package="0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP11" library="Lin-Temp-Controller" package="1206TESTPAD" value="TESTPT">
<attribute name="NAME"/>
</element>
<element name="TP12" library="Lin-Temp-Controller" package="1206TESTPAD" value="TESTPT">
<attribute name="NAME"/>
</element>
<element name="TP13" library="Lin-Temp-Controller" package="1206TESTPAD" value="TESTPT">
<attribute name="NAME"/>
</element>
<element name="X3" library="connector-jqi" package="BNC90" value="BNC-H">
<attribute name="DIGIKEY" value="A32260-ND"/>
<attribute name="NAME"/>
</element>
<element name="X4" library="connector-jqi" package="BNC90" value="BNC-H">
<attribute name="DIGIKEY" value="A32260-ND"/>
<attribute name="NAME"/>
</element>
<element name="R52" library="rlc-jqi" package="0603" value="1.0k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R53" library="rlc-jqi" package="0603" value="1.0k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R54" library="rlc-jqi" package="0603" value="1.0k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP14" library="Lin-Temp-Controller" package="1206TESTPAD" value="TESTPT">
<attribute name="NAME"/>
</element>
<element name="JP8" library="pinhead" package="2X06/90" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R55" library="rlc-jqi" package="0603" value="4.3k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R56" library="rlc-jqi" package="0603" value="1.5k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP9" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP10" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R57" library="rlc-jqi" package="0603" value="4.3k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R58" library="rlc-jqi" package="0603" value="1.5k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T5" library="Lin-Temp-Controller" package="SOT-23" value="MMBT3904">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY" value="MMBT3904-FDICT-ND"/>
</element>
<element name="T6" library="Lin-Temp-Controller" package="SOT-23" value="MMBT3904">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY" value="MMBT3904-FDICT-ND"/>
</element>
<element name="IC7" library="Lin-Temp-Controller" package="SO08" value="LM393D">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY" value="296-1015-5-ND"/>
</element>
<element name="R59" library="Lin-Temp-Controller" package="64WPOT" value="10k">
<attribute name="DIGIKEY" value="987-1061-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R60" library="Lin-Temp-Controller" package="64WPOT" value="10k">
<attribute name="DIGIKEY" value="987-1061-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R61" library="rlc-jqi" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R62" library="rlc-jqi" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R63" library="rlc-jqi" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R64" library="rlc-jqi" package="0603" value="33k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R65" library="rlc-jqi" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R66" library="rlc-jqi" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP15" library="Lin-Temp-Controller" package="1206TESTPAD" value="TESTPT">
<attribute name="NAME"/>
</element>
<element name="TP16" library="Lin-Temp-Controller" package="1206TESTPAD" value="TESTPT">
<attribute name="NAME"/>
</element>
<element name="S3" library="Lin-Temp-Controller" package="E-SWITCH-100-M7" value="">
<attribute name="MFR_PN" value="100DP1T2B4M7QE"/>
<attribute name="DIGIKEY" value="100DP1T2B4M7QE-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="Lin-Temp-Controller" package="HLMP--F0010" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY" value="516-1417-ND"/>
</element>
<element name="R67" library="rlc-jqi" package="0603" value="330">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC8" library="Lin-Temp-Controller" package="TSSOP16" value="AD5262">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY" value="AD5262BRUZ200-ND"/>
</element>
<element name="C22" library="rlc-jqi" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C23" library="rlc-jqi" package="0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP17" library="Lin-Temp-Controller" package="1206TESTPAD" value="TESTPT">
<attribute name="NAME"/>
</element>
<element name="TP18" library="Lin-Temp-Controller" package="1206TESTPAD" value="TESTPT">
<attribute name="NAME"/>
</element>
<element name="TP19" library="Lin-Temp-Controller" package="1206TESTPAD" value="TESTPT">
<attribute name="NAME"/>
</element>
<element name="X5" library="connector-jqi" package="BNC90" value="BNC-H">
<attribute name="DIGIKEY" value="A32260-ND"/>
<attribute name="NAME"/>
</element>
<element name="X6" library="connector-jqi" package="BNC90" value="BNC-H">
<attribute name="DIGIKEY" value="A32260-ND"/>
<attribute name="NAME"/>
</element>
<element name="R70" library="rlc-jqi" package="0603" value="1.0k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R71" library="rlc-jqi" package="0603" value="1.0k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R72" library="rlc-jqi" package="0603" value="1.0k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP20" library="Lin-Temp-Controller" package="1206TESTPAD" value="TESTPT">
<attribute name="NAME"/>
</element>
<element name="JP11" library="pinhead" package="2X06/90" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R73" library="rlc-jqi" package="0603" value="4.3k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R74" library="rlc-jqi" package="0603" value="1.5k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP12" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP13" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R75" library="rlc-jqi" package="0603" value="4.3k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R76" library="rlc-jqi" package="0603" value="1.5k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T7" library="Lin-Temp-Controller" package="SOT-23" value="MMBT3904">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY" value="MMBT3904-FDICT-ND"/>
</element>
<element name="T8" library="Lin-Temp-Controller" package="SOT-23" value="MMBT3904">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY" value="MMBT3904-FDICT-ND"/>
</element>
<element name="IC9" library="Lin-Temp-Controller" package="SO08" value="LM393D">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY" value="296-1015-5-ND"/>
</element>
<element name="R77" library="Lin-Temp-Controller" package="64WPOT" value="10k">
<attribute name="DIGIKEY" value="987-1061-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R78" library="Lin-Temp-Controller" package="64WPOT" value="10k">
<attribute name="DIGIKEY" value="987-1061-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R79" library="rlc-jqi" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R80" library="rlc-jqi" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R81" library="rlc-jqi" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R82" library="rlc-jqi" package="0603" value="33k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R83" library="rlc-jqi" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R84" library="rlc-jqi" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP21" library="Lin-Temp-Controller" package="1206TESTPAD" value="TESTPT">
<attribute name="NAME"/>
</element>
<element name="TP22" library="Lin-Temp-Controller" package="1206TESTPAD" value="TESTPT">
<attribute name="NAME"/>
</element>
<element name="S4" library="Lin-Temp-Controller" package="E-SWITCH-100-M7" value="">
<attribute name="MFR_PN" value="100DP1T2B4M7QE"/>
<attribute name="DIGIKEY" value="100DP1T2B4M7QE-ND"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="Lin-Temp-Controller" package="HLMP--F0010" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY" value="516-1417-ND"/>
</element>
<element name="R85" library="rlc-jqi" package="0603" value="330">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC10" library="Lin-Temp-Controller" package="TSSOP16" value="AD5262">
<attribute name="NAME"/>
<attribute name="VALUE"/>
<attribute name="DIGIKEY" value="AD5262BRUZ200-ND"/>
</element>
<element name="C24" library="rlc-jqi" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C25" library="rlc-jqi" package="0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP23" library="Lin-Temp-Controller" package="1206TESTPAD" value="TESTPT">
<attribute name="NAME"/>
</element>
<element name="TP24" library="Lin-Temp-Controller" package="1206TESTPAD" value="TESTPT">
<attribute name="NAME"/>
</element>
<element name="TP25" library="Lin-Temp-Controller" package="1206TESTPAD" value="TESTPT">
<attribute name="NAME"/>
</element>
<element name="X7" library="connector-jqi" package="BNC90" value="BNC-H">
<attribute name="DIGIKEY" value="A32260-ND"/>
<attribute name="NAME"/>
</element>
<element name="X8" library="connector-jqi" package="BNC90" value="BNC-H">
<attribute name="DIGIKEY" value="A32260-ND"/>
<attribute name="NAME"/>
</element>
<element name="R88" library="rlc-jqi" package="0603" value="1.0k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R89" library="rlc-jqi" package="0603" value="1.0k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R90" library="rlc-jqi" package="0603" value="1.0k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP26" library="Lin-Temp-Controller" package="1206TESTPAD" value="TESTPT">
<attribute name="NAME"/>
</element>
<element name="U$2" library="JQI_Logo" package="JQI_LOGO_NEGATIVE-SILKSCREEN" value=""/>
<element name="TP27" library="Lin-Temp-Controller" package="1206TESTPAD" value="TESTPT">
<attribute name="NAME"/>
</element>
<element name="LCD_HEADER" library="mcu-accessories" package="ML08" value=""/>
<element name="C26" library="rlc-jqi" package="0603" value="1000pF"/>
<element name="JP14" library="pinhead" package="2X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="VBAT">
<contactref element="U$1" pad="VBAT"/>
</signal>
<signal name="VUSB">
<contactref element="U$1" pad="VUSB"/>
</signal>
<signal name="AGND">
<contactref element="U$1" pad="AGND"/>
<contactref element="R21" pad="P$1"/>
<contactref element="C3" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="R27" pad="P$1"/>
<contactref element="C9" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="R25" pad="P$1"/>
<contactref element="C6" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="R23" pad="P$1"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="L3" pad="1"/>
<contactref element="IC3" pad="3"/>
<contactref element="C27" pad="1"/>
<contactref element="C30" pad="1"/>
<contactref element="IC6" pad="3"/>
<contactref element="C15" pad="1"/>
<contactref element="C14" pad="1"/>
<contactref element="CP1" pad="-"/>
<contactref element="CP2" pad="2"/>
<contactref element="CP3" pad="-"/>
<contactref element="JP4" pad="1"/>
<contactref element="X1" pad="2"/>
<contactref element="X2" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="JP3" pad="2"/>
<contactref element="JP5" pad="2"/>
<contactref element="T1" pad="2"/>
<contactref element="T2" pad="2"/>
<contactref element="S1" pad="P$5"/>
<contactref element="S1" pad="P$2"/>
<contactref element="R6" pad="P$3"/>
<contactref element="R6" pad="P$2"/>
<contactref element="R7" pad="P$3"/>
<contactref element="R7" pad="P$2"/>
<contactref element="IC1" pad="4"/>
<contactref element="C12" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="IC4" pad="11"/>
<contactref element="X3" pad="2"/>
<contactref element="X4" pad="2"/>
<contactref element="R37" pad="1"/>
<contactref element="R39" pad="1"/>
<contactref element="JP6" pad="2"/>
<contactref element="JP7" pad="2"/>
<contactref element="T3" pad="2"/>
<contactref element="T4" pad="2"/>
<contactref element="S2" pad="P$5"/>
<contactref element="S2" pad="P$2"/>
<contactref element="R41" pad="P$3"/>
<contactref element="R41" pad="P$2"/>
<contactref element="R42" pad="P$3"/>
<contactref element="R42" pad="P$2"/>
<contactref element="IC2" pad="4"/>
<contactref element="C20" pad="1"/>
<contactref element="C21" pad="1"/>
<contactref element="IC5" pad="11"/>
<contactref element="X5" pad="2"/>
<contactref element="X6" pad="2"/>
<contactref element="R55" pad="1"/>
<contactref element="R57" pad="1"/>
<contactref element="JP9" pad="2"/>
<contactref element="JP10" pad="2"/>
<contactref element="T5" pad="2"/>
<contactref element="T6" pad="2"/>
<contactref element="S3" pad="P$5"/>
<contactref element="S3" pad="P$2"/>
<contactref element="R59" pad="P$3"/>
<contactref element="R59" pad="P$2"/>
<contactref element="R60" pad="P$3"/>
<contactref element="R60" pad="P$2"/>
<contactref element="IC7" pad="4"/>
<contactref element="C22" pad="1"/>
<contactref element="C23" pad="1"/>
<contactref element="IC8" pad="11"/>
<contactref element="X7" pad="2"/>
<contactref element="X8" pad="2"/>
<contactref element="R73" pad="1"/>
<contactref element="R75" pad="1"/>
<contactref element="JP12" pad="2"/>
<contactref element="JP13" pad="2"/>
<contactref element="T7" pad="2"/>
<contactref element="T8" pad="2"/>
<contactref element="S4" pad="P$5"/>
<contactref element="S4" pad="P$2"/>
<contactref element="R77" pad="P$3"/>
<contactref element="R77" pad="P$2"/>
<contactref element="R78" pad="P$3"/>
<contactref element="R78" pad="P$2"/>
<contactref element="IC9" pad="4"/>
<contactref element="C24" pad="1"/>
<contactref element="C25" pad="1"/>
<contactref element="IC10" pad="11"/>
<contactref element="JP1" pad="12"/>
<contactref element="JP2" pad="12"/>
<contactref element="JP8" pad="12"/>
<contactref element="JP11" pad="12"/>
<contactref element="TP27" pad="P$1"/>
<contactref element="C26" pad="2"/>
</signal>
<signal name="VDD">
<contactref element="L2" pad="2"/>
<contactref element="L1" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="IC6" pad="1"/>
<contactref element="R19" pad="2"/>
<contactref element="R28" pad="P$2"/>
<contactref element="R29" pad="2"/>
<contactref element="R32" pad="2"/>
<contactref element="R33" pad="P$2"/>
<contactref element="R34" pad="2"/>
<contactref element="CP3" pad="+"/>
<contactref element="L4" pad="1"/>
<contactref element="R8" pad="2"/>
<contactref element="IC1" pad="8"/>
<contactref element="R9" pad="2"/>
<contactref element="R11" pad="2"/>
<contactref element="R12" pad="2"/>
<contactref element="D1" pad="A"/>
<contactref element="C12" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="IC4" pad="5"/>
<contactref element="IC4" pad="13"/>
<contactref element="IC4" pad="6"/>
<contactref element="IC4" pad="10"/>
<contactref element="R43" pad="2"/>
<contactref element="IC2" pad="8"/>
<contactref element="R44" pad="2"/>
<contactref element="R46" pad="2"/>
<contactref element="R47" pad="2"/>
<contactref element="D2" pad="A"/>
<contactref element="C20" pad="2"/>
<contactref element="C21" pad="2"/>
<contactref element="IC5" pad="5"/>
<contactref element="IC5" pad="13"/>
<contactref element="IC5" pad="6"/>
<contactref element="IC5" pad="10"/>
<contactref element="R61" pad="2"/>
<contactref element="IC7" pad="8"/>
<contactref element="R62" pad="2"/>
<contactref element="R64" pad="2"/>
<contactref element="R65" pad="2"/>
<contactref element="D3" pad="A"/>
<contactref element="C22" pad="2"/>
<contactref element="C23" pad="2"/>
<contactref element="IC8" pad="5"/>
<contactref element="IC8" pad="13"/>
<contactref element="IC8" pad="6"/>
<contactref element="IC8" pad="10"/>
<contactref element="R79" pad="2"/>
<contactref element="IC9" pad="8"/>
<contactref element="R80" pad="2"/>
<contactref element="R82" pad="2"/>
<contactref element="R83" pad="2"/>
<contactref element="D4" pad="A"/>
<contactref element="C24" pad="2"/>
<contactref element="C25" pad="2"/>
<contactref element="IC10" pad="5"/>
<contactref element="IC10" pad="13"/>
<contactref element="IC10" pad="6"/>
<contactref element="IC10" pad="10"/>
<contactref element="JP1" pad="11"/>
<contactref element="JP1" pad="2"/>
<contactref element="JP2" pad="2"/>
<contactref element="JP2" pad="11"/>
<contactref element="JP8" pad="2"/>
<contactref element="JP8" pad="11"/>
<contactref element="JP11" pad="11"/>
<contactref element="JP11" pad="2"/>
</signal>
<signal name="MOSI">
<contactref element="U$1" pad="11"/>
<contactref element="LCD_HEADER" pad="3"/>
</signal>
<signal name="SCK">
<contactref element="U$1" pad="13"/>
<contactref element="LCD_HEADER" pad="5"/>
</signal>
<signal name="CS_DAC">
<contactref element="IC3" pad="6"/>
<contactref element="U$1" pad="6"/>
</signal>
<signal name="CS_LCD">
<contactref element="U$1" pad="12"/>
<contactref element="LCD_HEADER" pad="6"/>
</signal>
<signal name="RS_LCD">
<contactref element="U$1" pad="10"/>
<contactref element="LCD_HEADER" pad="7"/>
</signal>
<signal name="RST_LCD">
<contactref element="U$1" pad="9"/>
<contactref element="LCD_HEADER" pad="8"/>
</signal>
<signal name="ACT_T3">
<contactref element="R71" pad="2"/>
<contactref element="U$1" pad="21/A7"/>
<contactref element="C5" pad="2"/>
</signal>
<signal name="ACT_T4">
<contactref element="R89" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="U$1" pad="19/A5"/>
</signal>
<signal name="VMON4">
<contactref element="R20" pad="P$2"/>
<contactref element="R90" pad="1"/>
<contactref element="JP11" pad="7"/>
</signal>
<signal name="ENC_B1">
<contactref element="R19" pad="1"/>
<contactref element="ENC1" pad="B"/>
<contactref element="C16" pad="2"/>
<contactref element="U$1" pad="7"/>
</signal>
<signal name="ENC_A2">
<contactref element="R33" pad="P$1"/>
<contactref element="ENC2" pad="A"/>
<contactref element="C19" pad="2"/>
<contactref element="U$1" pad="14/A0"/>
</signal>
<signal name="ENC_B2">
<contactref element="R32" pad="1"/>
<contactref element="ENC2" pad="B"/>
<contactref element="C18" pad="2"/>
<contactref element="U$1" pad="16/A2"/>
</signal>
<signal name="ENC_SW1">
<contactref element="ENC1" pad="E"/>
<contactref element="R29" pad="1"/>
<contactref element="U$1" pad="8"/>
</signal>
<signal name="ENC_A1">
<contactref element="R28" pad="P$1"/>
<contactref element="ENC1" pad="A"/>
<contactref element="C17" pad="2"/>
<contactref element="U$1" pad="17/A3"/>
</signal>
<signal name="N$25">
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="U$1" pad="VIN"/>
<contactref element="L2" pad="1"/>
</signal>
<signal name="DGND">
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="U$1" pad="GND"/>
<contactref element="U$1" pad="GND1"/>
<contactref element="L3" pad="2"/>
<contactref element="R31" pad="1"/>
<contactref element="C17" pad="1"/>
<contactref element="R30" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="R36" pad="1"/>
<contactref element="C19" pad="1"/>
<contactref element="R35" pad="1"/>
<contactref element="C18" pad="1"/>
<contactref element="IC4" pad="12"/>
<contactref element="IC5" pad="12"/>
<contactref element="IC8" pad="12"/>
<contactref element="IC10" pad="12"/>
<contactref element="LCD_HEADER" pad="2"/>
<contactref element="LCD_HEADER" pad="4"/>
</signal>
<signal name="CS_POT1">
<contactref element="IC4" pad="9"/>
<contactref element="U$1" pad="2"/>
</signal>
<signal name="CS_POT2">
<contactref element="IC5" pad="9"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="CS_POT3">
<contactref element="IC8" pad="9"/>
<contactref element="U$1" pad="4"/>
</signal>
<signal name="CS_POT4">
<contactref element="IC10" pad="9"/>
<contactref element="U$1" pad="5"/>
</signal>
<signal name="ACT_T2">
<contactref element="R53" pad="2"/>
<contactref element="U$1" pad="23/A9"/>
<contactref element="C7" pad="2"/>
</signal>
<signal name="VMON1">
<contactref element="R26" pad="P$2"/>
<contactref element="R18" pad="1"/>
<contactref element="JP1" pad="7"/>
</signal>
<signal name="ACT_T1">
<contactref element="U$1" pad="A11"/>
<contactref element="C11" pad="2"/>
<contactref element="R15" pad="2"/>
</signal>
<signal name="MOSI_B">
<contactref element="IC3" pad="8"/>
<contactref element="IC4" pad="8"/>
<contactref element="IC5" pad="8"/>
<contactref element="IC8" pad="8"/>
<contactref element="IC10" pad="8"/>
<contactref element="U$1" pad="0"/>
</signal>
<signal name="2.5V">
<contactref element="U$1" pad="AREF"/>
<contactref element="C10" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="IC6" pad="2"/>
<contactref element="TP7" pad="P$1"/>
<contactref element="JP1" pad="9"/>
<contactref element="JP2" pad="9"/>
<contactref element="JP8" pad="9"/>
<contactref element="JP11" pad="9"/>
<contactref element="JP14" pad="2"/>
</signal>
<signal name="SCK_B">
<contactref element="IC3" pad="7"/>
<contactref element="IC4" pad="7"/>
<contactref element="IC5" pad="7"/>
<contactref element="IC8" pad="7"/>
<contactref element="IC10" pad="7"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="VMON1_B">
<contactref element="U$1" pad="A10"/>
<contactref element="R26" pad="P$1"/>
<contactref element="R27" pad="P$2"/>
<contactref element="C9" pad="2"/>
</signal>
<signal name="VMON4_B">
<contactref element="R20" pad="P$1"/>
<contactref element="R21" pad="P$2"/>
<contactref element="C3" pad="2"/>
<contactref element="U$1" pad="18/A4"/>
</signal>
<signal name="VMON3">
<contactref element="R22" pad="P$2"/>
<contactref element="R72" pad="1"/>
<contactref element="JP8" pad="7"/>
</signal>
<signal name="VMON2">
<contactref element="R24" pad="P$2"/>
<contactref element="R54" pad="1"/>
<contactref element="JP2" pad="7"/>
</signal>
<signal name="3.3V">
<contactref element="U$1" pad="3.3V"/>
<contactref element="U$1" pad="3.3V1"/>
<contactref element="LCD_HEADER" pad="1"/>
</signal>
<signal name="VSET1">
<contactref element="IC3" pad="1"/>
<contactref element="IC1" pad="3"/>
<contactref element="IC1" pad="6"/>
<contactref element="JP1" pad="10"/>
<contactref element="TP8" pad="P$1"/>
</signal>
<signal name="N$24">
<contactref element="C27" pad="2"/>
<contactref element="C30" pad="2"/>
<contactref element="IC3" pad="9"/>
<contactref element="L1" pad="1"/>
</signal>
<signal name="VSET2">
<contactref element="IC3" pad="2"/>
<contactref element="IC2" pad="3"/>
<contactref element="IC2" pad="6"/>
<contactref element="JP2" pad="10"/>
<contactref element="TP14" pad="P$1"/>
</signal>
<signal name="VSET3">
<contactref element="IC3" pad="4"/>
<contactref element="IC7" pad="3"/>
<contactref element="IC7" pad="6"/>
<contactref element="JP8" pad="10"/>
<contactref element="TP20" pad="P$1"/>
</signal>
<signal name="VSET4">
<contactref element="IC3" pad="5"/>
<contactref element="IC9" pad="3"/>
<contactref element="IC9" pad="6"/>
<contactref element="JP11" pad="10"/>
<contactref element="TP26" pad="P$1"/>
</signal>
<signal name="N$1">
<contactref element="IC3" pad="10"/>
<contactref element="TP1" pad="P$1"/>
<contactref element="JP14" pad="3"/>
<contactref element="JP14" pad="4"/>
</signal>
<signal name="N$15">
<contactref element="ENC1" pad="C"/>
<contactref element="R30" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="R31" pad="2"/>
<contactref element="ENC1" pad="D"/>
</signal>
<signal name="ENC_SW2">
<contactref element="ENC2" pad="E"/>
<contactref element="R34" pad="1"/>
<contactref element="U$1" pad="15/A1"/>
</signal>
<signal name="N$17">
<contactref element="ENC2" pad="C"/>
<contactref element="R35" pad="2"/>
</signal>
<signal name="N$19">
<contactref element="R36" pad="2"/>
<contactref element="ENC2" pad="D"/>
</signal>
<signal name="+5V">
<contactref element="CP1" pad="+"/>
<contactref element="CP2" pad="1"/>
<contactref element="JP4" pad="2"/>
<contactref element="L4" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="R2" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="JP3" pad="1"/>
<contactref element="S1" pad="P$3"/>
</signal>
<signal name="N$5">
<contactref element="R4" pad="1"/>
<contactref element="R3" pad="2"/>
<contactref element="JP5" pad="1"/>
<contactref element="S1" pad="P$6"/>
</signal>
<signal name="N$6">
<contactref element="R8" pad="1"/>
<contactref element="R6" pad="P$1"/>
<contactref element="TP2" pad="P$1"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="IC1" pad="1"/>
<contactref element="R10" pad="2"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="R10" pad="1"/>
<contactref element="T1" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="R11" pad="1"/>
<contactref element="R7" pad="P$1"/>
<contactref element="TP3" pad="P$1"/>
<contactref element="IC1" pad="5"/>
</signal>
<signal name="N$8">
<contactref element="IC1" pad="7"/>
<contactref element="R13" pad="2"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="R13" pad="1"/>
<contactref element="T2" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="D1" pad="C"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="S1" pad="P$4"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="R14" pad="2"/>
<contactref element="X1" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="R18" pad="2"/>
<contactref element="X2" pad="1"/>
</signal>
<signal name="LIMA1">
<contactref element="R2" pad="2"/>
<contactref element="T1" pad="3"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="LIMB1">
<contactref element="R4" pad="2"/>
<contactref element="T2" pad="3"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="P1">
<contactref element="IC4" pad="2"/>
<contactref element="TP4" pad="P$1"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="+1V_1">
<contactref element="TP5" pad="P$1"/>
<contactref element="JP1" pad="3"/>
<contactref element="IC4" pad="3"/>
<contactref element="IC4" pad="4"/>
<contactref element="IC4" pad="14"/>
<contactref element="IC4" pad="15"/>
</signal>
<signal name="I1">
<contactref element="IC4" pad="16"/>
<contactref element="TP6" pad="P$1"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="N$21">
<contactref element="R38" pad="1"/>
<contactref element="R37" pad="2"/>
<contactref element="JP6" pad="1"/>
<contactref element="S2" pad="P$3"/>
</signal>
<signal name="N$22">
<contactref element="R40" pad="1"/>
<contactref element="R39" pad="2"/>
<contactref element="JP7" pad="1"/>
<contactref element="S2" pad="P$6"/>
</signal>
<signal name="N$23">
<contactref element="R43" pad="1"/>
<contactref element="R41" pad="P$1"/>
<contactref element="TP9" pad="P$1"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="N$26">
<contactref element="IC2" pad="1"/>
<contactref element="R45" pad="2"/>
<contactref element="R44" pad="1"/>
</signal>
<signal name="N$27">
<contactref element="R45" pad="1"/>
<contactref element="T3" pad="1"/>
</signal>
<signal name="N$28">
<contactref element="R46" pad="1"/>
<contactref element="R42" pad="P$1"/>
<contactref element="TP10" pad="P$1"/>
<contactref element="IC2" pad="5"/>
</signal>
<signal name="N$29">
<contactref element="IC2" pad="7"/>
<contactref element="R48" pad="2"/>
<contactref element="R47" pad="1"/>
</signal>
<signal name="N$30">
<contactref element="R48" pad="1"/>
<contactref element="T4" pad="1"/>
</signal>
<signal name="N$31">
<contactref element="D2" pad="C"/>
<contactref element="R49" pad="2"/>
</signal>
<signal name="N$32">
<contactref element="S2" pad="P$4"/>
<contactref element="R49" pad="1"/>
</signal>
<signal name="N$35">
<contactref element="R52" pad="1"/>
<contactref element="R53" pad="1"/>
<contactref element="JP2" pad="8"/>
</signal>
<signal name="N$36">
<contactref element="R52" pad="2"/>
<contactref element="X3" pad="1"/>
</signal>
<signal name="N$37">
<contactref element="R54" pad="2"/>
<contactref element="X4" pad="1"/>
</signal>
<signal name="LIMA2">
<contactref element="R38" pad="2"/>
<contactref element="T3" pad="3"/>
<contactref element="JP2" pad="4"/>
</signal>
<signal name="LIMB2">
<contactref element="R40" pad="2"/>
<contactref element="T4" pad="3"/>
<contactref element="JP2" pad="6"/>
</signal>
<signal name="P2">
<contactref element="IC5" pad="2"/>
<contactref element="TP11" pad="P$1"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="+1V_2">
<contactref element="TP12" pad="P$1"/>
<contactref element="JP2" pad="3"/>
<contactref element="IC5" pad="3"/>
<contactref element="IC5" pad="4"/>
<contactref element="IC5" pad="14"/>
<contactref element="IC5" pad="15"/>
</signal>
<signal name="I2">
<contactref element="IC5" pad="16"/>
<contactref element="TP13" pad="P$1"/>
<contactref element="JP2" pad="5"/>
</signal>
<signal name="N$38">
<contactref element="R56" pad="1"/>
<contactref element="R55" pad="2"/>
<contactref element="JP9" pad="1"/>
<contactref element="S3" pad="P$3"/>
</signal>
<signal name="N$39">
<contactref element="R58" pad="1"/>
<contactref element="R57" pad="2"/>
<contactref element="JP10" pad="1"/>
<contactref element="S3" pad="P$6"/>
</signal>
<signal name="N$40">
<contactref element="R61" pad="1"/>
<contactref element="R59" pad="P$1"/>
<contactref element="TP15" pad="P$1"/>
<contactref element="IC7" pad="2"/>
</signal>
<signal name="N$41">
<contactref element="IC7" pad="1"/>
<contactref element="R63" pad="2"/>
<contactref element="R62" pad="1"/>
</signal>
<signal name="N$42">
<contactref element="R63" pad="1"/>
<contactref element="T5" pad="1"/>
</signal>
<signal name="N$43">
<contactref element="R64" pad="1"/>
<contactref element="R60" pad="P$1"/>
<contactref element="TP16" pad="P$1"/>
<contactref element="IC7" pad="5"/>
</signal>
<signal name="N$44">
<contactref element="IC7" pad="7"/>
<contactref element="R66" pad="2"/>
<contactref element="R65" pad="1"/>
</signal>
<signal name="N$45">
<contactref element="R66" pad="1"/>
<contactref element="T6" pad="1"/>
</signal>
<signal name="N$46">
<contactref element="D3" pad="C"/>
<contactref element="R67" pad="2"/>
</signal>
<signal name="N$47">
<contactref element="S3" pad="P$4"/>
<contactref element="R67" pad="1"/>
</signal>
<signal name="N$50">
<contactref element="R70" pad="1"/>
<contactref element="R71" pad="1"/>
<contactref element="JP8" pad="8"/>
</signal>
<signal name="N$51">
<contactref element="R70" pad="2"/>
<contactref element="X5" pad="1"/>
</signal>
<signal name="N$52">
<contactref element="R72" pad="2"/>
<contactref element="X6" pad="1"/>
</signal>
<signal name="LIMA3">
<contactref element="R56" pad="2"/>
<contactref element="T5" pad="3"/>
<contactref element="JP8" pad="4"/>
</signal>
<signal name="LIMB3">
<contactref element="R58" pad="2"/>
<contactref element="T6" pad="3"/>
<contactref element="JP8" pad="6"/>
</signal>
<signal name="P3">
<contactref element="IC8" pad="2"/>
<contactref element="TP17" pad="P$1"/>
<contactref element="JP8" pad="1"/>
</signal>
<signal name="+1V_3">
<contactref element="TP18" pad="P$1"/>
<contactref element="JP8" pad="3"/>
<contactref element="IC8" pad="3"/>
<contactref element="IC8" pad="4"/>
<contactref element="IC8" pad="14"/>
<contactref element="IC8" pad="15"/>
</signal>
<signal name="I3">
<contactref element="IC8" pad="16"/>
<contactref element="TP19" pad="P$1"/>
<contactref element="JP8" pad="5"/>
</signal>
<signal name="LIMA4">
<contactref element="R74" pad="2"/>
<contactref element="T7" pad="3"/>
<contactref element="JP11" pad="4"/>
</signal>
<signal name="LIMB4">
<contactref element="R76" pad="2"/>
<contactref element="T8" pad="3"/>
<contactref element="JP11" pad="6"/>
</signal>
<signal name="P4">
<contactref element="IC10" pad="2"/>
<contactref element="TP23" pad="P$1"/>
<contactref element="JP11" pad="1"/>
</signal>
<signal name="+1V_4">
<contactref element="TP24" pad="P$1"/>
<contactref element="JP11" pad="3"/>
<contactref element="IC10" pad="3"/>
<contactref element="IC10" pad="4"/>
<contactref element="IC10" pad="14"/>
<contactref element="IC10" pad="15"/>
</signal>
<signal name="I4">
<contactref element="IC10" pad="16"/>
<contactref element="TP25" pad="P$1"/>
<contactref element="JP11" pad="5"/>
</signal>
<signal name="N$53">
<contactref element="R74" pad="1"/>
<contactref element="R73" pad="2"/>
<contactref element="JP12" pad="1"/>
<contactref element="S4" pad="P$3"/>
</signal>
<signal name="N$54">
<contactref element="R76" pad="1"/>
<contactref element="R75" pad="2"/>
<contactref element="JP13" pad="1"/>
<contactref element="S4" pad="P$6"/>
</signal>
<signal name="N$55">
<contactref element="R79" pad="1"/>
<contactref element="R77" pad="P$1"/>
<contactref element="TP21" pad="P$1"/>
<contactref element="IC9" pad="2"/>
</signal>
<signal name="N$56">
<contactref element="IC9" pad="1"/>
<contactref element="R81" pad="2"/>
<contactref element="R80" pad="1"/>
</signal>
<signal name="N$57">
<contactref element="R81" pad="1"/>
<contactref element="T7" pad="1"/>
</signal>
<signal name="N$58">
<contactref element="R82" pad="1"/>
<contactref element="R78" pad="P$1"/>
<contactref element="TP22" pad="P$1"/>
<contactref element="IC9" pad="5"/>
</signal>
<signal name="N$59">
<contactref element="IC9" pad="7"/>
<contactref element="R84" pad="2"/>
<contactref element="R83" pad="1"/>
</signal>
<signal name="N$60">
<contactref element="R84" pad="1"/>
<contactref element="T8" pad="1"/>
</signal>
<signal name="N$61">
<contactref element="D4" pad="C"/>
<contactref element="R85" pad="2"/>
</signal>
<signal name="N$62">
<contactref element="S4" pad="P$4"/>
<contactref element="R85" pad="1"/>
</signal>
<signal name="N$65">
<contactref element="R88" pad="1"/>
<contactref element="R89" pad="1"/>
<contactref element="JP11" pad="8"/>
</signal>
<signal name="N$66">
<contactref element="R88" pad="2"/>
<contactref element="X7" pad="1"/>
</signal>
<signal name="N$67">
<contactref element="R90" pad="2"/>
<contactref element="X8" pad="1"/>
</signal>
<signal name="N$69">
<contactref element="JP1" pad="8"/>
<contactref element="R14" pad="1"/>
<contactref element="R15" pad="1"/>
</signal>
<signal name="VMON3_B">
<contactref element="U$1" pad="20/A6"/>
<contactref element="R22" pad="P$1"/>
<contactref element="R23" pad="P$2"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="VMON2_B">
<contactref element="U$1" pad="22/A8"/>
<contactref element="R24" pad="P$1"/>
<contactref element="R25" pad="P$2"/>
<contactref element="C6" pad="2"/>
</signal>
<signal name="N$18">
<contactref element="C26" pad="1"/>
<contactref element="JP14" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
