<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="1.27" y1="0" x2="29.21" y2="0" width="0" layer="20"/>
<wire x1="30.48" y1="1.27" x2="30.48" y2="21.59" width="0" layer="20"/>
<wire x1="29.21" y1="22.86" x2="1.27" y2="22.86" width="0" layer="20"/>
<wire x1="0" y1="21.59" x2="0" y2="1.27" width="0" layer="20"/>
<wire x1="0" y1="21.59" x2="1.27" y2="22.86" width="0" layer="20" curve="-90"/>
<wire x1="29.21" y1="22.86" x2="30.48" y2="21.59" width="0" layer="20" curve="-90"/>
<wire x1="30.48" y1="1.27" x2="29.21" y2="0" width="0" layer="20" curve="-90"/>
<wire x1="1.27" y1="0" x2="0" y2="1.27" width="0" layer="20" curve="-90"/>
<text>Designed by Ricardo SS</text>
<text>PZT+</text>
<text>PZT-</text>
<text>+</text>
<text>-</text>
<text>PZT</text>
</plain>
<libraries>
<library name="justice">
<packages>
<package name="CLAIRWAYS_LOGO_LUNG">
</package>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
<package name="CLAIRWAYS_COPYRIGHT">
<description>&lt;h3&gt;Creative Commons License Template&lt;/h3&gt;
&lt;p&gt;CC BY-SA 4.0 License with &lt;a href="https://creativecommons.org/licenses/by-sa/4.0/"&gt;link to license&lt;/a&gt; and placeholder for designer name.&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;FRAME_LEDGER&lt;/li&gt;
&lt;li&gt;FRAME_LETTER&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="DUMMY">
<description>&lt;h3&gt;Dummy Footprint&lt;/h3&gt;
&lt;p&gt;NOTHING HERE!!! For when you want a symbol with no package as an option against symbols with a package.&lt;/p&gt;

&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;BADGERHACK_LOGO&lt;/li&gt;
&lt;li&gt;FRAME-LETTER&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="HRS_ZX62-B-5PA(33)">
</package>
<package name="1X01">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="MIC94045">
</package>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
<package name="MSOP10">
</package>
<package name="MSOP08">
<description>&lt;b&gt;8-Lead micro SO&lt;/b&gt; (RM-8)&lt;p&gt;
Source: http://www.analog.com/UploadedFiles/Data_Sheets/703465986AD8611_2_0.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun LEDs&lt;/h3&gt;
This library contains discrete LEDs for illumination or indication, but no displays.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-0603">
<description>&lt;B&gt;LED 0603 SMT&lt;/B&gt;&lt;p&gt;
0603, surface mount.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.075inch &lt;/li&gt;
&lt;li&gt;Area: 0.06" x 0.03"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;LED - BLUE&lt;/li&gt;</description>
</package>
</packages>
</library>
<library name="Antenna">
<packages>
<package name="XC9276BE56ERG">
<description>&lt;b&gt;USP-8B06&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="PTS841ESDGMPSMTRLFS">
<description>&lt;b&gt;PTS841 ESD GMP SMTR LFS-1&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="MSOP-8">
</package>
<package name="PVG3A102C01R00">
<description>&lt;b&gt;PVG3A102C01R00-1&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="PESD5V0S1BL315">
<description>&lt;b&gt;SOD882&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="BLM18AG102BH1D">
<description>&lt;b&gt;BLM18_1 L=1.6 W=0.8 T=0.8&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="CJS1200TA2">
<description>&lt;b&gt;CJS-1200TA2-3&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="AYF530665T">
<description>&lt;b&gt;AYF530665T-2&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="SON50P200X200X80-9N">
<description>&lt;b&gt;EMC1833T-AE/RW&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="5033981892">
<description>&lt;b&gt;5033981892-1&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="CM8V32768TA020125">
<description>&lt;b&gt;CM8V&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="tinycircuits">
<description>TinyCircuits Eagle Library</description>
<packages>
<package name="JST_SH_2X1">
</package>
</packages>
</library>
<library name="SparkFun-IC-Microcontroller">
<description>&lt;h3&gt;SparkFun Microcontrollers&lt;/h3&gt;
This library contains microcontrollers.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="ARTEMIS_FP">
</package>
</packages>
</library>
<library name="SparkFun-IC-Power">
<description>&lt;h3&gt;SparkFun Power Driver and Management ICs&lt;/h3&gt;
In this library you'll find anything that has to do with power delivery, or making power supplies.
&lt;p&gt;Contents:
&lt;ul&gt;&lt;li&gt;LDOs&lt;/li&gt;
&lt;li&gt;Boost/Buck controllers&lt;/li&gt;
&lt;li&gt;Charge pump controllers&lt;/li&gt;
&lt;li&gt;Power sequencers&lt;/li&gt;
&lt;li&gt;Power switches&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="BMP1" library="justice" package="CLAIRWAYS_LOGO_LUNG" value="CLAIRWAYS_LOGOCLAIRWAYS_LUNG"/>
<element name="C1" library="justice" package="0603" value="15pF">
<attribute name="MPN" value="VJ0603A150FXQPW1BC"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="justice" package="0603" value="10uF">
<attribute name="MPN" value="0603ZD106KAT2A"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="justice" package="0603" value="10uF">
<attribute name="MPN" value="0603ZD106KAT2A"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="justice" package="0603" value="0.1uF">
<attribute name="MPN" value="06035C104JAT2A"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="justice" package="0603" value="0.1uF">
<attribute name="MPN" value="06035C104JAT2A"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="justice" package="0603" value="1nF">
<attribute name="MPN" value="C0603C102F3GACAUTO"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="justice" package="0603" value="100nF">
<attribute name="MPN" value="06035C104JAT2A"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C16" library="justice" package="0603" value="100nF">
<attribute name="MPN" value="06035C104JAT2A"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="justice" package="0603" value="100nF">
<attribute name="MPN" value="06035C104JAT2A"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="justice" package="0603" value="10n">
<attribute name="MPN" value="C0603X103G5JAC7867"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C19" library="justice" package="0603" value="2.4n">
<attribute name="MPN" value="
C0603C242J5GAC7867"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="justice" package="0603" value="15pF">
<attribute name="MPN" value="VJ0603A150FXQPW1BC"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C20" library="justice" package="0603" value="2.4n">
<attribute name="MPN" value="
C0603C242J5GAC7867"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C21" library="justice" package="0603" value="10n">
<attribute name="MPN" value="C0603X103G5JAC7867"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="justice" package="0603" value="100n">
<attribute name="MPN" value="06035C104JAT2A"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C23" library="justice" package="0603" value="0.1uF">
<attribute name="MPN" value="06035C104JAT2A"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C24" library="justice" package="0603" value="1uF">
<attribute name="MPN" value="C0603C105Z8VACTU"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="justice" package="0603" value="0.1uF">
<attribute name="MPN" value="06035C104JAT2A"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="justice" package="0603" value="10uF">
<attribute name="MPN" value="0603ZD106KAT2A"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="justice" package="0603" value="1uF">
<attribute name="MPN" value="C0603C105Z8VACTU"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="justice" package="0603" value="0.1uF">
<attribute name="MPN" value="06035C104JAT2A"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="justice" package="0603" value="10uF">
<attribute name="MPN" value="0603ZD106KAT2A"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="justice" package="0603" value="0.1uF">
<attribute name="MPN" value="06035C104JAT2A"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="justice" package="0603" value="1uF">
<attribute name="MPN" value="C0603C105Z8VACTU"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="SparkFun-LED" package="LED-0603" value="Yellow">
<attribute name="MF" value="Vishay"/>
<attribute name="MPN" value="TLMY1000-GS08"/>
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-09003"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="SparkFun-LED" package="LED-0603" value="Orange">
<attribute name="MF" value="Vishay"/>
<attribute name="MPN" value="TLMO1000-GS08"/>
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-08575"/>
<attribute name="VALUE"/>
</element>
<element name="FRAME1" library="justice" package="CLAIRWAYS_COPYRIGHT" value="FRAME-LETTER">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="FRAME2" library="justice" package="DUMMY" value="FRAME-LETTERNO_PACKAGE">
<attribute name="DESIGNER" value="Nobody"/>
<attribute name="VERSION" value="v01"/>
</element>
<element name="IC1" library="Antenna" package="XC9276BE56ERG" value="XC6192AA05ER-G">
<attribute name="DESCRIPTION" value="Power Switch ICs - Power Distribution Power Saving Push Button Load Switch"/>
<attribute name="MF" value="Torex"/>
<attribute name="MPN" value="XC6192AA05ER-G"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="justice" package="HRS_ZX62-B-5PA(33)" value="ZX62-B-5PA(33)">
<attribute name="DESCRIPTION" value=" USB - micro B USB 2.0 Receptacle Connector 5 Position Surface Mount, Right Angle "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="H125270CT-ND"/>
<attribute name="DIGI-KEY_PURCHASE_URL" value="https://www.digikey.com/product-detail/en/hirose-electric-co-ltd/ZX62-B-5PA_33_/H125270CT-ND/5994756?utm_source=snapeda&amp;utm_medium=aggregator&amp;utm_campaign=symbol"/>
<attribute name="MF" value="Hirose"/>
<attribute name="MP" value="ZX62-B-5PA_33_"/>
<attribute name="MPN" value="ZX62-B-5PA(33)"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="tinycircuits" package="JST_SH_2X1" value="SM02B-SRSS">
<attribute name="MF" value="JST"/>
<attribute name="MPN" value="SM02B-SRSS"/>
<attribute name="NAME"/>
<attribute name="PARTNO" value="AS-ITM-00231"/>
<attribute name="PNPROTATION" value="180"/>
</element>
<element name="PZT+" library="justice" package="1X01" value="M01">
<attribute name="MF" value="PUI Audio"/>
<attribute name="MPN" value="AB2025B-LW100-R"/>
<attribute name="SPICEPREFIX" value="P"/>
</element>
<element name="PZT-" library="justice" package="1X01" value="M01"/>
<element name="R1" library="justice" package="0603" value="2k">
<attribute name="MPN" value="ERJ-PA3J202V"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="justice" package="0603" value="1M">
<attribute name="MPN" value="CRCW06031M00FKEC"/>
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" "/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="justice" package="0603" value="1M">
<attribute name="MPN" value="CRCW06031M00FKEC"/>
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" "/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="justice" package="0603" value="13.3k">
<attribute name="MPN" value="RNCF0603DTE13K3"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="justice" package="0603" value="8.87k">
<attribute name="MPN" value="
RNCF0603DTE8K87"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="justice" package="0603" value="13.3k">
<attribute name="MPN" value="RNCF0603DTE13K3"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="justice" package="0603" value="8.87k">
<attribute name="MPN" value="
RNCF0603DTE8K87"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="justice" package="0603" value="16k">
<attribute name="MPN" value="RR0816P-163-D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="justice" package="0603" value="2k">
<attribute name="MPN" value="ERJ-PA3J202V"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="justice" package="0603" value="2k">
<attribute name="MPN" value="ERJ-PA3J202V"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="justice" package="0603" value="100k">
<attribute name="MPN" value="RR0816P-104-D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="justice" package="0603" value="220k">
<attribute name="MPN" value="
RR0816P-224-D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="justice" package="0603" value="220k">
<attribute name="MPN" value="RR0816P-224-D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="justice" package="0603" value="37.4k">
<attribute name="MPN" value="ERJ-PB3B3742V"/>
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" "/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="justice" package="0603" value="37.4k">
<attribute name="MPN" value="ERJ-PB3B3742V"/>
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" "/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="justice" package="0603" value="9.31k">
<attribute name="MPN" value="RR0816P-9311-D-94H"/>
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" "/>
<attribute name="VALUE"/>
</element>
<element name="S3" library="Antenna" package="PTS841ESDGMPSMTRLFS" value="PTS841_ESD_GMP_SMTR_LFS">
<attribute name="DESCRIPTION" value="Tactile Switches Tact Switch 50mA 12VDC, 3.6x3.5, 1.25mmH, 180gf, G leads, pegs, ground pin"/>
<attribute name="MF" value="C &amp; K COMPONENTS"/>
<attribute name="MPN" value="PTS841 ESD GMP SMTR LFS"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="Antenna" package="MSOP-8" value="AD8617ARMZ">
<attribute name="MPN" value="
AD8617ARMZ"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="justice" package="MIC94045" value="MIC94045">
<attribute name="MPN" value="MIC94045YFL-TR"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U10" library="justice" package="SOT23-5" value="MCP1711T-33I/OT">
<attribute name="MPN" value="MCP1711T-33I/OT"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U2" library="SparkFun-IC-Microcontroller" package="ARTEMIS_FP" value="ARTEMIS_MODULESMD">
<attribute name="MF" value="SparkFun"/>
<attribute name="MPN" value="WRL-15484"/>
<attribute name="PROD_ID" value="SUB-14415"/>
</element>
<element name="U3" library="justice" package="MSOP10" value="CH340E_MSOP10">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="IC-14135"/>
<attribute name="VALUE"/>
</element>
<element name="U4" library="SparkFun-IC-Power" package="SOT23-5" value="MCP73831">
<attribute name="MF" value=""/>
<attribute name="MPN" value="MCP73832T-2ATI/OT"/>
<attribute name="NAME"/>
<attribute name="PROD_ID" value="IC-09995"/>
<attribute name="VALUE"/>
</element>
<element name="U5" library="justice" package="SOT23-5" value="MCP1711T-33I/OT">
<attribute name="MPN" value="MCP1711T-33I/OT"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="VR1" library="Antenna" package="PVG3A102C01R00" value="PVG3A102C01R00">
<attribute name="ARROW_PART_NUMBER" value="PVG3A102C01R00"/>
<attribute name="ARROW_PRICE-STOCK" value="https://www.arrow.com/en/products/pvg3a102c01r00/bourns"/>
<attribute name="DESCRIPTION" value="Res Cermet Trimmer 1K Ohm 20% 0.25W(1/4W) 1(Elec)/1(Mech)Turns 2.2mm (3.6 X 3.6 X 2mm) J-Hook SMD T/R"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="MANUFACTURER_NAME" value="Bourns"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="PVG3A102C01R00"/>
<attribute name="MOUSER_PART_NUMBER" value="81-PVG3A102C01R00"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Bourns/PVG3A102C01R00?qs=QnQa2dTVfy7N6mPIxWVTeg%3D%3D"/>
<attribute name="MPN" value="PVG3A102C01R00"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="Antenna" package="PESD5V0S1BL315" value="RB521CS30L,315">
<attribute name="ARROW_PART_NUMBER" value="RB521CS30L,315"/>
<attribute name="ARROW_PRICE-STOCK" value="https://www.arrow.com/en/products/rb521cs30l315/nexperia"/>
<attribute name="DESCRIPTION" value="Nexperia 30V 100mA, Diode, 2-Pin SOD-882 RB521CS30L,315"/>
<attribute name="HEIGHT" value="0mm"/>
<attribute name="MANUFACTURER_NAME" value="Nexperia"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="RB521CS30L,315"/>
<attribute name="MOUSER_PART_NUMBER" value="771-RB521CS30L315"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Nexperia/RB521CS30L315/?qs=A1cBxND5mHIn1i5kyMT1%252Bg%3D%3D"/>
<attribute name="MPN" value="RB521CS30L,315"/>
<attribute name="NAME"/>
</element>
<element name="D4" library="Antenna" package="PESD5V0S1BL315" value="RB521CS30L,315">
<attribute name="ARROW_PART_NUMBER" value="RB521CS30L,315"/>
<attribute name="ARROW_PRICE-STOCK" value="https://www.arrow.com/en/products/rb521cs30l315/nexperia"/>
<attribute name="DESCRIPTION" value="Nexperia 30V 100mA, Diode, 2-Pin SOD-882 RB521CS30L,315"/>
<attribute name="HEIGHT" value="0mm"/>
<attribute name="MANUFACTURER_NAME" value="Nexperia"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="RB521CS30L,315"/>
<attribute name="MOUSER_PART_NUMBER" value="771-RB521CS30L315"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Nexperia/RB521CS30L315/?qs=A1cBxND5mHIn1i5kyMT1%252Bg%3D%3D"/>
<attribute name="MPN" value="RB521CS30L,315"/>
<attribute name="NAME"/>
</element>
<element name="C25" library="justice" package="0603" value="300pF">
<attribute name="MPN" value="0603N301J500CT"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FL1" library="Antenna" package="BLM18AG102BH1D" value="BLM18HB221SN1D">
<attribute name="ARROW_PART_NUMBER" value=""/>
<attribute name="ARROW_PRICE-STOCK" value=""/>
<attribute name="DESCRIPTION" value="BLM18_N1D Series EMI Suppression Filter 220+/-25% at 100MHz 100mA @85"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="MANUFACTURER_NAME" value="Murata Electronics"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="BLM18HB221SN1D"/>
<attribute name="MOUSER_PART_NUMBER" value="81-BLM18HB221SN1D"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Murata-Electronics/BLM18HB221SN1D?qs=h9XNjnv%2FSxuKV9bY5gYGeQ%3D%3D"/>
<attribute name="MPN" value="BLM18HB221SN1D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="Antenna" package="CJS1200TA2" value="CJS-1200TA2">
<attribute name="ARROW_PART_NUMBER" value=""/>
<attribute name="ARROW_PRICE-STOCK" value=""/>
<attribute name="DESCRIPTION" value="SPDT, ON-ON Slide, 100mA @ 6V DC J-Hook SMD Terminals, T&amp;R 1,000 pc Packaging, Non-washable with tape - Tape and Reel"/>
<attribute name="HEIGHT" value="2.5mm"/>
<attribute name="MANUFACTURER_NAME" value="NIDEC COPAL"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="CJS-1200TA2"/>
<attribute name="MOUSER_PART_NUMBER" value="229-CJS-1200TA2"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Nidec-Copal/CJS-1200TA2?qs=XeJtXLiO41Rf26ws0igWdA%3D%3D"/>
<attribute name="MPN" value="CJS-1200TA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U6" library="justice" package="MSOP08" value="AD8236">
<attribute name="MPN" value="AD8226ARMZ"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="Antenna" package="AYF530665T" value="AYF530665T">
<attribute name="ARROW_PART_NUMBER" value="AYF530665T"/>
<attribute name="ARROW_PRICE-STOCK" value="https://www.arrow.com/en/products/ayf530665t/panasonic"/>
<attribute name="DESCRIPTION" value="Conn FPC Connector SKT 6 POS 0.5mm Solder RA SMD T/R"/>
<attribute name="HEIGHT" value="1.76mm"/>
<attribute name="MANUFACTURER_NAME" value="Panasonic"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="AYF530665T"/>
<attribute name="MOUSER_PART_NUMBER" value="769-AYF530665T"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Panasonic-Industrial-Devices/AYF530665T?qs=CoW5K%2FMp%2F72JANoCMSEzJA%3D%3D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="Antenna" package="SON50P200X200X80-9N" value="MCP1501T-10E_RW">
<attribute name="ARROW_PART_NUMBER" value="MCP1501T-10E/RW"/>
<attribute name="ARROW_PRICE-STOCK" value="https://www.arrow.com/en/products/mcp1501t-25erw/microchip-technology"/>
<attribute name="DESCRIPTION" value="Voltage References High Prec Buffered Voltage Reference"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="MANUFACTURER_NAME" value="Microchip"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="MCP1501T-10E/RW"/>
<attribute name="MOUSER_PART_NUMBER" value="579-MCP1501T-10E/RW"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Microchip-Technology/MCP1501T-25E-RW?qs=BA62vJVifGo7hml43fG32Q%3D%3D"/>
<attribute name="MPN" value="MCP1501T-10E/RW"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="Antenna" package="5033981892" value="5033981892">
<attribute name="ARROW_PART_NUMBER" value="5033981892"/>
<attribute name="ARROW_PRICE-STOCK" value="https://www.arrow.com/en/products/503398-1892/molex"/>
<attribute name="DESCRIPTION" value="Conn Micro SD Card SKT 8 POS 1.1mm Solder RA SMD 0.5A/Contact T/R"/>
<attribute name="HEIGHT" value="1.28mm"/>
<attribute name="MANUFACTURER_NAME" value="Molex"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="5033981892"/>
<attribute name="MOUSER_PART_NUMBER" value="N/A"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=N%2FA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Y1" library="Antenna" package="CM8V32768TA020125" value="CM8V-T1A-32.768KHZ-12.5PF-20PPM-TA-QA">
<attribute name="ARROW_PART_NUMBER" value=""/>
<attribute name="ARROW_PRICE-STOCK" value=""/>
<attribute name="DESCRIPTION" value="CM8V-T1A Tuning Fork Crystal 32.768 kHz"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="MANUFACTURER_NAME" value="Micro Crystal AG"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="CM8V-T1A-32.768KHZ-12.5PF-20PPM-TA-QA"/>
<attribute name="MOUSER_PART_NUMBER" value="428-201436-MC01"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Micro-Crystal/CM8V-T1A-32768kHz-7pF-20PPM-TA-QC?qs=7bTaA%2FLYtSYyZWzzv04BxA%3D%3D"/>
<attribute name="MPN" value="CM8V-T1A-32.768KHZ-12.5PF-20PPM-TA-QA"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U2" pad="GND@1"/>
<contactref element="U2" pad="GND@22"/>
<contactref element="U2" pad="GND@38"/>
<contactref element="U2" pad="GND@39"/>
<contactref element="U2" pad="GND@47"/>
<contactref element="U2" pad="GND@59"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="C5" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="U4" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="C11" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="U10" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="D2" pad="C"/>
<contactref element="C3" pad="2"/>
<contactref element="J2" pad="1"/>
<contactref element="U1" pad="2"/>
<contactref element="S3" pad="4"/>
<contactref element="S3" pad="5"/>
<contactref element="S3" pad="3"/>
<contactref element="IC1" pad="6"/>
<contactref element="IC1" pad="9"/>
<contactref element="IC1" pad="7"/>
<contactref element="IC1" pad="2"/>
<contactref element="IC1" pad="5"/>
<contactref element="R5" pad="1"/>
<contactref element="C14" pad="2"/>
<contactref element="J1" pad="5"/>
<contactref element="U3" pad="3"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="U5" pad="2"/>
<contactref element="C23" pad="2"/>
<contactref element="FL1" pad="1"/>
<contactref element="J5" pad="6"/>
<contactref element="J3" pad="6"/>
</signal>
<signal name="3.3V">
<contactref element="C5" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="U2" pad="VDD@36"/>
<contactref element="U2" pad="VDD@37"/>
<contactref element="U10" pad="5"/>
<contactref element="C9" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="U1" pad="3"/>
<contactref element="R4" pad="2"/>
<contactref element="C6" pad="1"/>
<contactref element="U3" pad="7"/>
<contactref element="C7" pad="1"/>
<contactref element="U3" pad="10"/>
<contactref element="U5" pad="1"/>
<contactref element="C23" pad="1"/>
<contactref element="U5" pad="3"/>
<contactref element="J5" pad="1"/>
<contactref element="J3" pad="4"/>
</signal>
<signal name="SWDIO">
<contactref element="U2" pad="SWDIO"/>
<contactref element="J5" pad="2"/>
</signal>
<signal name="!RESET">
<contactref element="U2" pad="~RST"/>
<contactref element="C13" pad="2"/>
<contactref element="C14" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="J5" pad="5"/>
</signal>
<signal name="SWDCK">
<contactref element="U2" pad="SWDCK"/>
<contactref element="J5" pad="3"/>
</signal>
<signal name="PDMDATA">
<contactref element="U2" pad="D15"/>
</signal>
<signal name="PDMCLK">
<contactref element="U2" pad="D14"/>
</signal>
<signal name="BOOT">
<contactref element="U2" pad="BOOT"/>
<contactref element="C12" pad="2"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U2" pad="XO"/>
<contactref element="C1" pad="1"/>
<contactref element="Y1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="U2" pad="XI"/>
<contactref element="C2" pad="2"/>
<contactref element="Y1" pad="1"/>
</signal>
<signal name="V_USB">
<contactref element="U4" pad="4"/>
<contactref element="D1" pad="A"/>
<contactref element="C10" pad="1"/>
<contactref element="J1" pad="1"/>
<contactref element="D3" pad="2"/>
</signal>
<signal name="RXI">
<contactref element="U2" pad="RXI-0"/>
<contactref element="U3" pad="8"/>
</signal>
<signal name="TXO">
<contactref element="U2" pad="TXO-0"/>
<contactref element="U3" pad="9"/>
</signal>
<signal name="V_BATT">
<contactref element="U4" pad="3"/>
<contactref element="C11" pad="1"/>
<contactref element="J2" pad="2"/>
<contactref element="D4" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="U4" pad="5"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="D1" pad="C"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="U4" pad="1"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="SWO">
<contactref element="U2" pad="~D22"/>
<contactref element="J5" pad="4"/>
</signal>
<signal name="N$2">
<contactref element="D2" pad="A"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="VIN">
<contactref element="R6" pad="2"/>
<contactref element="IC1" pad="1"/>
<contactref element="D3" pad="1"/>
<contactref element="D4" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="U2" pad="~D19"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="SDI">
<contactref element="U2" pad="~D6"/>
<contactref element="J3" pad="7"/>
</signal>
<signal name="SCLK">
<contactref element="U2" pad="~D5"/>
<contactref element="J3" pad="5"/>
</signal>
<signal name="SDO">
<contactref element="U2" pad="D7"/>
<contactref element="J3" pad="3"/>
</signal>
<signal name="SCL">
<contactref element="U2" pad="~D27"/>
</signal>
<signal name="SDA">
<contactref element="U2" pad="~D25"/>
</signal>
<signal name="INT1">
<contactref element="U2" pad="~D43"/>
</signal>
<signal name="INT2">
<contactref element="U2" pad="~D42"/>
</signal>
<signal name="PWR_BTN">
<contactref element="U1" pad="4"/>
<contactref element="IC1" pad="3"/>
<contactref element="R6" pad="1"/>
<contactref element="S3" pad="2"/>
<contactref element="S3" pad="1"/>
</signal>
<signal name="USR_BTN">
<contactref element="U2" pad="D8"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="IC1" pad="8"/>
<contactref element="U10" pad="3"/>
<contactref element="U10" pad="1"/>
<contactref element="C8" pad="1"/>
</signal>
<signal name="!RTS">
<contactref element="C13" pad="1"/>
<contactref element="U3" pad="4"/>
<contactref element="C12" pad="1"/>
</signal>
<signal name="D_N">
<contactref element="J1" pad="2"/>
<contactref element="U3" pad="2"/>
</signal>
<signal name="D_P">
<contactref element="J1" pad="3"/>
<contactref element="U3" pad="1"/>
</signal>
<signal name="CS">
<contactref element="U2" pad="~D39"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="R7" pad="2"/>
<contactref element="R8" pad="1"/>
<contactref element="C15" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="R9" pad="2"/>
<contactref element="C16" pad="2"/>
<contactref element="C17" pad="1"/>
</signal>
<signal name="NOTCH_OUT">
<contactref element="R8" pad="2"/>
<contactref element="C17" pad="2"/>
<contactref element="C22" pad="1"/>
</signal>
<signal name="PZT+">
<contactref element="PZT+" pad="1"/>
<contactref element="R10" pad="1"/>
<contactref element="U6" pad="4"/>
</signal>
<signal name="PZT-">
<contactref element="PZT-" pad="1"/>
<contactref element="R11" pad="2"/>
<contactref element="U6" pad="1"/>
</signal>
<signal name="VCC/2">
<contactref element="R10" pad="2"/>
<contactref element="R11" pad="1"/>
<contactref element="C19" pad="2"/>
<contactref element="C20" pad="2"/>
<contactref element="R16" pad="2"/>
<contactref element="U6" pad="6"/>
<contactref element="IC2" pad="7"/>
<contactref element="IC2" pad="8"/>
<contactref element="C25" pad="1"/>
</signal>
<signal name="VPZT">
<contactref element="R7" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="U6" pad="7"/>
</signal>
<signal name="N$11">
<contactref element="VR1" pad="3"/>
<contactref element="U6" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="VR1" pad="2"/>
<contactref element="U6" pad="3"/>
</signal>
<signal name="N$13">
<contactref element="R12" pad="2"/>
<contactref element="R13" pad="1"/>
<contactref element="C18" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="R13" pad="2"/>
<contactref element="U$1" pad="3"/>
<contactref element="C19" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="R14" pad="2"/>
<contactref element="R15" pad="1"/>
<contactref element="C21" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="R15" pad="2"/>
<contactref element="U$1" pad="5"/>
<contactref element="C20" pad="1"/>
</signal>
<signal name="LP_S1_OUT">
<contactref element="C18" pad="1"/>
<contactref element="U$1" pad="1"/>
<contactref element="U$1" pad="2"/>
<contactref element="R14" pad="1"/>
<contactref element="S1" pad="1"/>
</signal>
<signal name="LP_S2_OUT">
<contactref element="C21" pad="2"/>
<contactref element="U$1" pad="7"/>
<contactref element="U$1" pad="6"/>
<contactref element="S1" pad="3"/>
</signal>
<signal name="HP_OUT">
<contactref element="C22" pad="2"/>
<contactref element="R16" pad="1"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="C24" pad="1"/>
<contactref element="U5" pad="5"/>
<contactref element="U$1" pad="8"/>
<contactref element="U6" pad="8"/>
<contactref element="IC2" pad="3"/>
<contactref element="IC2" pad="1"/>
</signal>
<signal name="AGND">
<contactref element="C24" pad="2"/>
<contactref element="C15" pad="1"/>
<contactref element="R9" pad="1"/>
<contactref element="U$1" pad="4"/>
<contactref element="FL1" pad="2"/>
<contactref element="U6" pad="5"/>
<contactref element="IC2" pad="2"/>
<contactref element="IC2" pad="4"/>
<contactref element="IC2" pad="6"/>
<contactref element="IC2" pad="5"/>
<contactref element="C25" pad="2"/>
<contactref element="IC2" pad="9"/>
</signal>
<signal name="PZT_OUT">
<contactref element="S1" pad="2"/>
<contactref element="U2" pad="~AD31"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
