<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="20.625" y2="0" width="0" layer="20"/>
<wire x1="20.625" y1="0" x2="20.625" y2="20.31" width="0" layer="20"/>
<wire x1="20.625" y1="20.31" x2="0" y2="20.31" width="0" layer="20"/>
<wire x1="0" y1="20.31" x2="0" y2="0" width="0" layer="20"/>
<hole x="3.81" y="16.51" drill="3.2"/>
<hole x="16.51" y="3.81" drill="3.2"/>
<wire x1="10.795" y1="3.81" x2="6.35" y2="3.81" width="0.254" layer="46"/>
<wire x1="3.81" y1="10.795" x2="3.81" y2="6.35" width="0.254" layer="46"/>
<wire x1="3.81" y1="6.35" x2="6.35" y2="3.81" width="0.254" layer="46"/>
<wire x1="10.16" y1="16.51" x2="6.35" y2="18.415" width="0.254" layer="46" curve="-73.739795"/>
<wire x1="16.51" y1="10.16" x2="18.415" y2="6.35" width="0.254" layer="46" curve="53.130102"/>
<wire x1="1.905" y1="13.97" x2="3.81" y2="10.795" width="0.254" layer="46" curve="-53.130102"/>
<wire x1="6.35" y1="18.415" x2="1.905" y2="13.97" width="0.254" layer="46" curve="196.260205"/>
<wire x1="13.97" y1="1.905" x2="10.795" y2="3.81" width="0.254" layer="46" curve="63.434949"/>
<wire x1="13.97" y1="1.905" x2="18.415" y2="6.35" width="0.254" layer="46" curve="196.260205"/>
<hole x="12.7" y="14.605" drill="1.2"/>
<hole x="14.605" y="12.7" drill="1.2"/>
<wire x1="16.51" y1="13.335" x2="16.51" y2="10.16" width="0.254" layer="46"/>
<wire x1="10.16" y1="16.51" x2="13.335" y2="16.51" width="0.254" layer="46"/>
<wire x1="13.335" y1="16.51" x2="16.51" y2="13.335" width="0.254" layer="46"/>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02_LOCK">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="EVQ-Q2">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="SparkFun-Connectors" package="1X02_LOCK" value="">
<attribute name="VALUE"/>
</element>
<element name="SW1" library="adafruit" package="EVQ-Q2" value="SPST_TACT-EVQQ2"/>
</elements>
<signals>
<signal name="N$1">
<contactref element="SW1" pad="B"/>
<contactref element="SW1" pad="B'"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="SW1" pad="A"/>
<contactref element="SW1" pad="A'"/>
<contactref element="JP1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
