<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.2.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="390" y2="0" width="0" layer="20"/>
<wire x1="390" y1="0" x2="390" y2="7" width="0" layer="20"/>
<wire x1="390" y1="7" x2="0" y2="7" width="0" layer="20"/>
<wire x1="0" y1="7" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="JST-3-PTH-VERT">
<description>&lt;h3&gt;JST 3 Pin Vertical Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:2mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/ePH.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
<description>&lt;h3&gt;AXIAL-0.3&lt;/h3&gt;
&lt;p&gt;Commonly used for 1/4W through-hole resistors. 0.3" pitch between holes.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Sensors">
<description>&lt;h3&gt;SparkFun Sensors&lt;/h3&gt;
This library contains sensors- accelerometers, gyros, compasses, magnetometers, light sensors, imagers, temp sensors, etc.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TO-92-AMMO">
<description>&lt;h3&gt;TO-92 3-Pin PTH AMMO package&lt;/h3&gt;
&lt;p&gt;&lt;a href=""&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;
&lt;li&gt;Pin Count: 3&lt;/li&gt;
&lt;li&gt;Dimensions:  3.68 x 4.83 x 4.83 mm&lt;/li&gt;
&lt;li&gt;Pitch: 2.54 mm&lt;/li&gt;
&lt;/ul&gt;
&lt;p&gt;Devices Using:&lt;/p&gt;
&lt;ul&gt;
&lt;li&gt;DS18B20&lt;/li&gt;
&lt;/ul&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Connectors" package="JST-3-PTH-VERT" value="JST_Header">
<attribute name="PROD_ID" value="CONN-13230"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.3" value="4.7k">
<attribute name="PROD_ID" value="RES-12182"/>
</element>
<element name="U1" library="SparkFun-Sensors" package="TO-92-AMMO" value="DS18B20">
<attribute name="STORE_ID" value="SEN-00245"/>
</element>
<element name="U2" library="SparkFun-Sensors" package="TO-92-AMMO" value="DS18B20">
<attribute name="STORE_ID" value="SEN-00245"/>
</element>
<element name="U3" library="SparkFun-Sensors" package="TO-92-AMMO" value="DS18B20">
<attribute name="STORE_ID" value="SEN-00245"/>
</element>
<element name="U4" library="SparkFun-Sensors" package="TO-92-AMMO" value="DS18B20">
<attribute name="STORE_ID" value="SEN-00245"/>
</element>
<element name="U5" library="SparkFun-Sensors" package="TO-92-AMMO" value="DS18B20">
<attribute name="STORE_ID" value="SEN-00245"/>
</element>
<element name="U6" library="SparkFun-Sensors" package="TO-92-AMMO" value="DS18B20">
<attribute name="STORE_ID" value="SEN-00245"/>
</element>
<element name="U7" library="SparkFun-Sensors" package="TO-92-AMMO" value="DS18B20">
<attribute name="STORE_ID" value="SEN-00245"/>
</element>
<element name="U8" library="SparkFun-Sensors" package="TO-92-AMMO" value="DS18B20">
<attribute name="STORE_ID" value="SEN-00245"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="J1" pad="3"/>
<contactref element="U8" pad="1"/>
<contactref element="U7" pad="1"/>
<contactref element="U6" pad="1"/>
<contactref element="U5" pad="1"/>
<contactref element="U4" pad="1"/>
<contactref element="U3" pad="1"/>
<contactref element="U2" pad="1"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="DQ">
<contactref element="J1" pad="2"/>
<contactref element="U8" pad="2"/>
<contactref element="U7" pad="2"/>
<contactref element="U6" pad="2"/>
<contactref element="U5" pad="2"/>
<contactref element="U4" pad="2"/>
<contactref element="U3" pad="2"/>
<contactref element="U2" pad="2"/>
<contactref element="U1" pad="2"/>
<contactref element="R1" pad="P$1"/>
</signal>
<signal name="VDD">
<contactref element="J1" pad="1"/>
<contactref element="U8" pad="3"/>
<contactref element="U7" pad="3"/>
<contactref element="U6" pad="3"/>
<contactref element="U5" pad="3"/>
<contactref element="U4" pad="3"/>
<contactref element="U3" pad="3"/>
<contactref element="U2" pad="3"/>
<contactref element="U1" pad="3"/>
<contactref element="R1" pad="P$2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
