<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="5.08" y1="2.54" x2="23.495" y2="2.54" width="0" layer="20"/>
<wire x1="26.67" y1="6.35" x2="26.67" y2="24.13" width="0" layer="20"/>
<wire x1="23.495" y1="26.67" x2="5.08" y2="26.67" width="0" layer="20"/>
<wire x1="2.54" y1="24.13" x2="2.54" y2="6.35" width="0" layer="20"/>
<wire x1="26.67" y1="6.35" x2="23.495" y2="2.54" width="0" layer="20" curve="-90"/>
<wire x1="23.495" y1="26.67" x2="26.67" y2="24.13" width="0" layer="20" curve="-90"/>
<wire x1="2.54" y1="24.13" x2="5.08" y2="26.67" width="0" layer="20" curve="-90"/>
<wire x1="5.08" y1="2.54" x2="2.54" y2="6.35" width="0" layer="20" curve="-90"/>
<hole x="24.13" y="24.13" drill="1.016"/>
<hole x="5.08" y="6.35" drill="1.016"/>
<text>R</text>
<text>V</text>
<text>G</text>
<text>1</text>
<text>0</text>
</plain>
<libraries>
<library name="RFD22301-11.25.13">
<packages>
<package name="RFD21733">
<description>RF Digital RFD22301</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="RGBLED5050">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="BATTCON_20MM_4LEGS">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="PAD.03X.03">
</package>
<package name="0805">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="RFD22301-11.25.13" package="RFD21733" value="RFD22301"/>
<element name="BAT1" library="SparkFun-Electromechanical" package="BATTCON_20MM_4LEGS" value="20mm coincell">
<attribute name="VALUE" value="20mm coincell"/>
<attribute name="PROD_ID" value="BATT-10373"/>
</element>
<element name="LED3" library="adafruit" package="RGBLED5050" value="RGBLED5050"/>
<element name="A1" library="SparkFun-Passives" package="PAD.03X.03" value="TEST-POINT3"/>
<element name="A0" library="SparkFun-Passives" package="PAD.03X.03" value="TEST-POINT3"/>
<element name="RST" library="SparkFun-Passives" package="PAD.03X.03" value="TEST-POINT3"/>
<element name="GND" library="SparkFun-Passives" package="PAD.03X.03" value="TEST-POINT3"/>
<element name="3V3" library="SparkFun-Passives" package="PAD.03X.03" value="TEST-POINT3"/>
<element name="R1" library="SparkFun-Passives" package="0805" value="100"/>
<element name="R2" library="SparkFun-Passives" package="0805" value="100"/>
<element name="R3" library="SparkFun-Passives" package="0805" value="100"/>
</elements>
<signals>
<signal name="3V3">
<contactref element="U$1" pad="P$13"/>
<contactref element="3V3" pad="P$1"/>
<contactref element="BAT1" pad="1"/>
</signal>
<signal name="RESET">
<contactref element="U$1" pad="P$14"/>
<contactref element="RST" pad="P$1"/>
</signal>
<signal name="A0">
<contactref element="U$1" pad="P$16"/>
<contactref element="A0" pad="P$1"/>
</signal>
<signal name="A1">
<contactref element="U$1" pad="P$17"/>
<contactref element="A1" pad="P$1"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="P$12"/>
<contactref element="U$1" pad="P$10"/>
<contactref element="U$1" pad="P$9"/>
<contactref element="BAT1" pad="2"/>
<contactref element="LED3" pad="5"/>
<contactref element="LED3" pad="6"/>
<contactref element="LED3" pad="4"/>
<contactref element="GND" pad="P$1"/>
</signal>
<signal name="A7">
<contactref element="U$1" pad="P$7"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="A6">
<contactref element="U$1" pad="P$6"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="A5">
<contactref element="U$1" pad="P$5"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="LED3" pad="3"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="LED3" pad="1"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="LED3" pad="2"/>
<contactref element="R3" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
