<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="38.532" x2="0" y2="1.27" width="0" layer="20"/>
<wire x1="0" y1="1.27" x2="1.27" y2="0" width="0" layer="20" curve="90"/>
<wire x1="1.27" y1="0" x2="60.432" y2="0" width="0" layer="20"/>
<wire x1="60.432" y1="0" x2="61.702" y2="1.27" width="0" layer="20" curve="90"/>
<wire x1="61.702" y1="1.27" x2="61.702" y2="38.532" width="0" layer="20"/>
<wire x1="61.702" y1="38.532" x2="60.432" y2="39.802" width="0" layer="20" curve="90"/>
<wire x1="60.432" y1="39.802" x2="1.27" y2="39.802" width="0" layer="20"/>
<wire x1="1.27" y1="39.802" x2="0" y2="38.532" width="0" layer="20" curve="90"/>
<text>PowerProf r1</text>
<text>MIT License - by ayan4m1</text>
<text>https://github.com/powerprof</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X08_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole -8 Pin No Silk&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:8&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_08&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="282834-2">
<packages>
<package name="CONN_282834-2">
</package>
</packages>
</library>
<library name="microcontroller">
<packages>
<package name="LOLIND32">
<description>Wemos Lolin D32 ESP32 development board with battery port.
VP and VN are Not Connected pins</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Aesthetics&lt;/h3&gt;
This library contiains non-functional items such as logos, build/ordering notes, frame blocks, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-S">
<description>&lt;h3&gt;Open-Source Hardware (OSHW) Logo - Small - Silkscreen&lt;/h3&gt;
&lt;p&gt;Silkscreen logo for open-source hardware designs.&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;OSHW_LOGO&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Connectors" package="1X08_NO_SILK" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08438"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="282834-2" package="CONN_282834-2" value="">
<attribute name="AVAILABILITY" value="Good"/>
<attribute name="CENTERLINE_PITCH" value="2.54 mm[.1 in]"/>
<attribute name="COMMENT" value="282834-2"/>
<attribute name="DESCRIPTION" value=" Wire-To-Board Terminal Block, 2, 150 V, 10 A, 30 Awg, 16 Awg, 1.4 Mm "/>
<attribute name="EU_ROHS_COMPLIANCE" value="Compliant with Exemptions"/>
<attribute name="MF" value="TE Connectivity"/>
<attribute name="MP" value="282834-2"/>
<attribute name="NAME"/>
<attribute name="NUMBER_OF_POSITIONS" value="2"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
<attribute name="PURCHASE-URL" value="https://pricing.snapeda.com/search/part/282834-2/?ref=eda"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="microcontroller" package="LOLIND32" value="">
<attribute name="NAME"/>
</element>
<element name="LOGO1" library="SparkFun-Aesthetics" package="OSHW-LOGO-S" value="OSHW-LOGOS"/>
</elements>
<signals>
<signal name="USB">
<contactref element="U1" pad="15"/>
</signal>
<signal name="BAT">
<contactref element="U1" pad="16"/>
</signal>
<signal name="SCL">
<contactref element="U1" pad="30"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="SDA">
<contactref element="U1" pad="27"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="ALERT">
<contactref element="U1" pad="5"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="VBUS">
<contactref element="J2" pad="2"/>
<contactref element="J1" pad="6"/>
</signal>
<signal name="3.3V">
<contactref element="U1" pad="1"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="17" route="any" routetag="G$1.GND"/>
<contactref element="U1" pad="32" route="any" routetag="G$1.GND"/>
<contactref element="J2" pad="1"/>
<contactref element="J1" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
