<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.2.1">
<drawing>
<board>
<plain>
<wire x1="5.896" y1="71.845" x2="5.896" y2="55.145" width="0" layer="20"/>
<wire x1="5.896" y1="55.145" x2="6.531" y2="54.51" width="0" layer="20"/>
<wire x1="6.531" y1="54.51" x2="54.037" y2="54.51" width="0" layer="20"/>
<wire x1="54.037" y1="54.51" x2="54.672" y2="55.145" width="0" layer="20"/>
<wire x1="54.672" y1="55.145" x2="54.672" y2="71.845" width="0" layer="20"/>
<wire x1="54.672" y1="71.845" x2="54.037" y2="72.48" width="0" layer="20"/>
<wire x1="54.037" y1="72.48" x2="6.531" y2="72.48" width="0" layer="20"/>
<wire x1="6.531" y1="72.48" x2="5.896" y2="71.845" width="0" layer="20"/>
<text>GND</text>
<text>VCC</text>
<text>Data</text>
<text>ANT</text>
<text>FS1000A</text>
<text>RXB6</text>
<text>Poor rflink by CHRIS V0.6 06/17</text>
<text>+5vcc</text>
<text>ANT</text>
<text>GND</text>
<text>vcc</text>
<text>Data</text>
<text>Poor rflink by CHRIS V0.6 06/17</text>
<text>GND</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X08">
</package>
<package name="1X02">
</package>
<package name="1X01">
</package>
</packages>
</library>
<library name="con-coax">
<description>&lt;b&gt;Coax Connectors&lt;/b&gt;&lt;p&gt;
Radiall  and M/A COM.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="BU-SMA-V">
<description>FEMALE &lt;b&gt;SMA CONNECTOR&lt;/b&gt;&lt;p&gt;
Radiall&lt;p&gt;
distributor RS 112-3794</description>
</package>
</packages>
</library>
<library name="SparkFun-RFnew">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find things that send or receive RF- GPS, cellular modules, Bluetooth, WiFi, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="RF-LINK_RX">
<description>RF-LINK receivers WRL-8947, 8948, 8949, 8950</description>
</package>
<package name="RF-LINK_TX">
<description>RF-LINK transmitters WRL-8945, 8946</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="SparkFun-Connectors" package="1X08" value="">
<attribute name="VALUE"/>
</element>
<element name="U$2" library="SparkFun-RFnew" package="RF-LINK_RX" value="RXB6"/>
<element name="U$3" library="SparkFun-RFnew" package="RF-LINK_TX" value="FS1000A"/>
<element name="TX" library="con-coax" package="BU-SMA-V" value="BU-SMA-V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="RX" library="con-coax" package="BU-SMA-V" value="BU-SMA-V">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X02" value="M02PTH"/>
<element name="JP3" library="SparkFun-Connectors" package="1X02" value="M02PTH"/>
<element name="JP4" library="SparkFun-Connectors" package="1X01" value="M01PTH"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U$3" pad="GND"/>
<contactref element="U$2" pad="GND@1"/>
<contactref element="TX" pad="4"/>
<contactref element="TX" pad="2"/>
<contactref element="TX" pad="5"/>
<contactref element="TX" pad="3"/>
<contactref element="RX" pad="4"/>
<contactref element="RX" pad="2"/>
<contactref element="RX" pad="5"/>
<contactref element="RX" pad="3"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="U$3" pad="ANT"/>
<contactref element="TX" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="U$2" pad="ANT"/>
<contactref element="RX" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="U$2" pad="+5V@1"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$10">
<contactref element="U$2" pad="DATA@1"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="N$11">
<contactref element="U$3" pad="VCC"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="U$3" pad="DATA"/>
<contactref element="JP1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
