<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.2.2">
<drawing>
<board>
<plain>
<wire x1="-11.43" y1="7.62" x2="11.43" y2="7.62" width="0.1524" layer="20"/>
<wire x1="11.43" y1="7.62" x2="12.7" y2="6.35" width="0.1524" layer="20" curve="-90"/>
<wire x1="12.7" y1="6.35" x2="12.7" y2="-6.35" width="0.1524" layer="20"/>
<wire x1="12.7" y1="-6.35" x2="11.43" y2="-7.62" width="0.1524" layer="20" curve="-90"/>
<wire x1="11.43" y1="-7.62" x2="-11.43" y2="-7.62" width="0.1524" layer="20"/>
<wire x1="-11.43" y1="-7.62" x2="-12.7" y2="-6.35" width="0.1524" layer="20" curve="-90"/>
<wire x1="-12.7" y1="-6.35" x2="-12.7" y2="6.35" width="0.1524" layer="20"/>
<wire x1="-12.7" y1="6.35" x2="-11.43" y2="7.62" width="0.1524" layer="20" curve="-90"/>
<text>PET 5040 CAPACITOR BOARD</text>
<text>200731 R0.1</text>
<text>P SALVAGIONE</text>
</plain>
<libraries>
<library name="Salvagione-Passives">
<packages>
<package name="C5040">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X01_NO_SILK">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C3" library="Salvagione-Passives" package="C5040" value=".33uF @ 250V"/>
<element name="J1" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X01_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="C4" library="Salvagione-Passives" package="C5040" value="2X .33uF @ 250V">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$3">
<contactref element="J1" pad="1"/>
<contactref element="C3" pad="P$1"/>
<contactref element="C4" pad="P$2"/>
</signal>
<signal name="N$4">
<contactref element="J2" pad="1"/>
<contactref element="C3" pad="P$2"/>
<contactref element="C4" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
