<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="22.84" y2="0" width="0" layer="20"/>
<wire x1="22.84" y1="0" x2="22.86" y2="20.828" width="0" layer="20"/>
<wire x1="22.86" y1="20.828" x2="0" y2="20.828" width="0" layer="20"/>
<wire x1="0" y1="20.828" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X8">
<description>&lt;h3&gt;Plated Through Hole - 2x8&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:16&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_08x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="russian-nixies_custom_iv3">
<description>&lt;b&gt;Russian IN series nixie tubes&lt;/b&gt;&lt;br&gt;&lt;br&gt;

Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Measurements taken from nixies in my collection
&lt;li&gt;http://www.tube-tester.com
&lt;/ul&gt;&lt;br&gt;
&lt;author&gt;Created by p.s.troost@student.tue.nl&lt;/author&gt;</description>
<packages>
<package name="IV-3A">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="LED3535">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Connectors" package="2X8" value="2X6 FEMALE"/>
<element name="N1" library="russian-nixies_custom_iv3" package="IV-3A" value="IV-3a"/>
<element name="LED2" library="adafruit" package="LED3535" value="WS2812B3535"/>
</elements>
<signals>
<signal name="FIL+">
<contactref element="N1" pad="7"/>
<contactref element="J1" pad="7"/>
</signal>
<signal name="3">
<contactref element="J1" pad="3"/>
<contactref element="N1" pad="3"/>
</signal>
<signal name="5">
<contactref element="J1" pad="5"/>
<contactref element="N1" pad="5"/>
</signal>
<signal name="4">
<contactref element="J1" pad="4"/>
<contactref element="N1" pad="4"/>
</signal>
<signal name="6">
<contactref element="J1" pad="6"/>
<contactref element="N1" pad="6"/>
</signal>
<signal name="10">
<contactref element="J1" pad="10"/>
<contactref element="N1" pad="10"/>
</signal>
<signal name="12">
<contactref element="J1" pad="12"/>
</signal>
<signal name="11">
<contactref element="J1" pad="11"/>
<contactref element="N1" pad="11"/>
</signal>
<signal name="FIL-">
<contactref element="N1" pad="8"/>
<contactref element="J1" pad="8"/>
</signal>
<signal name="GRID">
<contactref element="N1" pad="9"/>
<contactref element="J1" pad="9"/>
</signal>
<signal name="1">
<contactref element="J1" pad="1"/>
<contactref element="N1" pad="1"/>
</signal>
<signal name="2">
<contactref element="J1" pad="2"/>
<contactref element="N1" pad="2"/>
</signal>
<signal name="VDD">
<contactref element="LED2" pad="2"/>
<contactref element="J1" pad="13"/>
</signal>
<signal name="LED_DO">
<contactref element="LED2" pad="3"/>
<contactref element="J1" pad="15"/>
</signal>
<signal name="GND">
<contactref element="LED2" pad="4"/>
<contactref element="J1" pad="16"/>
</signal>
<signal name="LED_DI">
<contactref element="LED2" pad="1"/>
<contactref element="J1" pad="14"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
