<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.4.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="33.198" y2="0" width="0" layer="20"/>
<wire x1="33.198" y1="0" x2="33.198" y2="20.31" width="0" layer="20"/>
<wire x1="33.198" y1="20.31" x2="0" y2="20.31" width="0" layer="20"/>
<wire x1="0" y1="20.31" x2="0" y2="0" width="0" layer="20"/>
<text>3V3</text>
<text>GND</text>
<text>RST</text>
<text>IO0</text>
<text>RST</text>
<text>IO0</text>
<text>TX</text>
<text>RX</text>
<text>Q1</text>
<text>Q2</text>
<text>github.com/pimvanpelt/
CP2102 Breakout
with RST/IO0 
v1.1</text>
<text>ON</text>
<text>TX</text>
<text>RX</text>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
<description>&lt;p&gt;&lt;b&gt;Generic 2012 (0805) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
<description>&lt;p&gt;&lt;b&gt;Generic 2012 (0805) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="transistor">
<description>&lt;b&gt;Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23-BEC">
<description>TO-236 ITT Intermetall</description>
</package>
</packages>
</library>
<library name="microusb">
<packages>
<package name="MICRO-USB">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Switches">
<description>&lt;h3&gt;SparkFun Switches, Buttons, Encoders&lt;/h3&gt;
In this library you'll find switches, buttons, joysticks, and anything that moves to create or disrupt an electrical connection.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE_SWITCH_SMD_6.0X3.5MM">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - SMD, 6.0 x 3.5 mm&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.sparkfun.com/datasheets/Components/1101.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="CHIP-LED0805">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB R99A&lt;br&gt;
Source: http://www.osram.convergy.de/ ... lb_r99a.pdf</description>
</package>
</packages>
</library>
<library name="CP2102N-A01-GQFN28">
<packages>
<package name="QFN50P500X500X80-29N">
</package>
</packages>
</library>
<library name="AP2112">
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Capacitors" package="0805" value="100nF">
<attribute name="NAME"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0805" value="1uF">
<attribute name="NAME"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="0805" value="100nF">
<attribute name="NAME"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0805" value="1uF">
<attribute name="NAME"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0805" value=" ">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0805" value="12k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0805" value="12k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" "/>
</element>
<element name="T1" library="transistor" package="SOT23-BEC" value="">
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="T2" library="transistor" package="SOT23-BEC" value="">
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="microusb" package="MICRO-USB" value="MICRO-USB"/>
<element name="J1" library="SparkFun-Connectors" package="1X06" value="">
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
<element name="S1" library="SparkFun-Switches" package="TACTILE_SWITCH_SMD_6.0X3.5MM" value="MOMENTARY-SWITCH-SPST-SMD-6.0X3.5MM">
<attribute name="PROD_ID" value="SWCH-14278"/>
<attribute name="SF_SKU" value="COM-08229"/>
</element>
<element name="S2" library="SparkFun-Switches" package="TACTILE_SWITCH_SMD_6.0X3.5MM" value="MOMENTARY-SWITCH-SPST-SMD-6.0X3.5MM">
<attribute name="PROD_ID" value="SWCH-14278"/>
<attribute name="SF_SKU" value="COM-08229"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0805" value="470">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R5" library="SparkFun-Resistors" package="0805" value="470">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" "/>
</element>
<element name="LED1" library="led" package="CHIP-LED0805" value="">
<attribute name="POPULARITY" value="68"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="0805" value="1k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" "/>
</element>
<element name="U2" library="CP2102N-A01-GQFN28" package="QFN50P500X500X80-29N" value="CP2102N-A01-GQFN28">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" USB Bridge, USB to UART USB 2.0 UART Interface 28-QFN _5x5_ "/>
<attribute name="MF" value="Silicon Labs"/>
<attribute name="MP" value="CP2102N-A01-GQFN28"/>
<attribute name="PACKAGE" value="QFN-28 Silicon Labs"/>
<attribute name="PRICE" value="None"/>
</element>
<element name="U1" library="AP2112" package="SOT23-5" value="3.3V">
<attribute name="PROD_ID" value="VREG-12457"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="0805" value="1k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R8" library="SparkFun-Resistors" package="0805" value="1k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" "/>
</element>
<element name="R9" library="SparkFun-Resistors" package="0805" value="1k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" "/>
</element>
<element name="LED2" library="led" package="CHIP-LED0805" value="">
<attribute name="POPULARITY" value="68"/>
<attribute name="VALUE"/>
</element>
<element name="LED3" library="led" package="CHIP-LED0805" value="">
<attribute name="POPULARITY" value="68"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="0805" value="1uF">
<attribute name="NAME"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="0805" value="1uF">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="VDDUSB">
<contactref element="U$1" pad="1"/>
<contactref element="U2" pad="8"/>
<contactref element="C4" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="U2" pad="7"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="1"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="D-">
<contactref element="U$1" pad="2"/>
<contactref element="U2" pad="5"/>
</signal>
<signal name="D+">
<contactref element="U$1" pad="3"/>
<contactref element="U2" pad="4"/>
</signal>
<signal name="RX">
<contactref element="J1" pad="2"/>
<contactref element="U2" pad="25"/>
</signal>
<signal name="RTS">
<contactref element="R3" pad="2"/>
<contactref element="T2" pad="E"/>
<contactref element="U2" pad="24"/>
</signal>
<signal name="DTR">
<contactref element="R2" pad="2"/>
<contactref element="T1" pad="E"/>
<contactref element="U2" pad="28"/>
</signal>
<signal name="TX">
<contactref element="J1" pad="3"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="T2" pad="B"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="T1" pad="B"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="IO0">
<contactref element="T1" pad="C"/>
<contactref element="J1" pad="4"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="RST">
<contactref element="T2" pad="C"/>
<contactref element="C1" pad="1"/>
<contactref element="J1" pad="5"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="GND">
<contactref element="J1" pad="1"/>
<contactref element="U$1" pad="GND2"/>
<contactref element="LED1" pad="C"/>
<contactref element="C1" pad="2"/>
<contactref element="U$1" pad="5"/>
<contactref element="S2" pad="1"/>
<contactref element="S1" pad="1"/>
<contactref element="U2" pad="29"/>
<contactref element="U2" pad="3"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="U$1" pad="GND1"/>
<contactref element="U1" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
</signal>
<signal name="VDD33">
<contactref element="J1" pad="6"/>
<contactref element="U1" pad="5"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="S2" pad="2"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="S1" pad="2"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="R6" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$13">
<contactref element="U2" pad="26"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="RXT">
<contactref element="LED3" pad="C"/>
<contactref element="U2" pad="18"/>
</signal>
<signal name="TXT">
<contactref element="LED2" pad="C"/>
<contactref element="U2" pad="19"/>
</signal>
<signal name="N$8">
<contactref element="R7" pad="1"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="N$9">
<contactref element="R8" pad="1"/>
<contactref element="LED3" pad="A"/>
</signal>
<signal name="N$10">
<contactref element="U2" pad="9"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="VDD">
<contactref element="R9" pad="1"/>
<contactref element="U2" pad="6"/>
<contactref element="C2" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="R7" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
