<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="-1.27" x2="22.84" y2="-1.27" width="0" layer="20"/>
<wire x1="22.84" y1="-1.27" x2="22.84" y2="6.02" width="0" layer="20"/>
<wire x1="22.84" y1="6.02" x2="0" y2="6.02" width="0" layer="20"/>
<wire x1="0" y1="6.02" x2="0" y2="-1.27" width="0" layer="20"/>
<text>By TinLethax</text>
</plain>
<libraries>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun LEDs&lt;/h3&gt;
This library contains discrete LEDs for illumination or indication, but no displays.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="APA102-2020">
<description>&lt;h3&gt;APA102-2020&lt;/h3&gt;

&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 8&lt;/li&gt;
&lt;li&gt;Size: 2.0 x 2.0 mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint:&lt;/b&gt; &lt;a href="https://cdn.sparkfun.com/assets/home_page_posts/2/3/9/8/APA102-2020_1.pdf"&gt;APA102-2020&lt;/a&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TP20SQ">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="D1" library="SparkFun-LED" package="APA102-2020" value="APA102-2020">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-13883"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="SparkFun-LED" package="APA102-2020" value="APA102-2020">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-13883"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="SparkFun-LED" package="APA102-2020" value="APA102-2020">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-13883"/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="SparkFun-LED" package="APA102-2020" value="APA102-2020">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-13883"/>
<attribute name="VALUE"/>
</element>
<element name="TP1" library="testpad" package="TP20SQ" value="TPTP20SQ">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="2"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP2" library="testpad" package="TP20SQ" value="TPTP20SQ">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="2"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP3" library="testpad" package="TP20SQ" value="TPTP20SQ">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="2"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP4" library="testpad" package="TP20SQ" value="TPTP20SQ">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="2"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP5" library="testpad" package="TP20SQ" value="TPTP20SQ">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="2"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP6" library="testpad" package="TP20SQ" value="TPTP20SQ">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="2"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP7" library="testpad" package="TP20SQ" value="TPTP20SQ">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="2"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="TP8" library="testpad" package="TP20SQ" value="TPTP20SQ">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="2"/>
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="VALUE"/>
</element>
<element name="D5" library="SparkFun-LED" package="APA102-2020" value="APA102-2020">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-13883"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="D1" pad="CO"/>
<contactref element="D2" pad="CI"/>
</signal>
<signal name="N$2">
<contactref element="D1" pad="DO"/>
<contactref element="D2" pad="DI"/>
</signal>
<signal name="N$3">
<contactref element="D2" pad="CO"/>
<contactref element="D3" pad="CI"/>
</signal>
<signal name="N$4">
<contactref element="D2" pad="DO"/>
<contactref element="D3" pad="DI"/>
</signal>
<signal name="N$5">
<contactref element="D3" pad="CO"/>
<contactref element="D4" pad="CI"/>
</signal>
<signal name="N$6">
<contactref element="D3" pad="DO"/>
<contactref element="D4" pad="DI"/>
</signal>
<signal name="N$7">
<contactref element="D1" pad="VDD"/>
<contactref element="D2" pad="VDD"/>
<contactref element="D3" pad="VDD"/>
<contactref element="TP3" pad="TP"/>
<contactref element="D4" pad="VDD"/>
<contactref element="D5" pad="VDD"/>
<contactref element="TP7" pad="TP"/>
</signal>
<signal name="N$8">
<contactref element="D1" pad="GND"/>
<contactref element="D2" pad="GND"/>
<contactref element="D3" pad="GND"/>
<contactref element="TP4" pad="TP"/>
<contactref element="D4" pad="GND"/>
<contactref element="D5" pad="GND"/>
<contactref element="TP8" pad="TP"/>
</signal>
<signal name="N$9">
<contactref element="D1" pad="CI"/>
<contactref element="TP1" pad="TP"/>
</signal>
<signal name="N$10">
<contactref element="D1" pad="DI"/>
<contactref element="TP2" pad="TP"/>
</signal>
<signal name="N$11">
<contactref element="D4" pad="CO"/>
<contactref element="D5" pad="CI"/>
</signal>
<signal name="N$12">
<contactref element="D4" pad="DO"/>
<contactref element="D5" pad="DI"/>
</signal>
<signal name="N$13">
<contactref element="D5" pad="CO"/>
<contactref element="TP5" pad="TP"/>
</signal>
<signal name="N$14">
<contactref element="D5" pad="DO"/>
<contactref element="TP6" pad="TP"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
