<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<wire x1="1.27" y1="0" x2="24.13" y2="0" width="0" layer="20"/>
<wire x1="0" y1="46.99" x2="0" y2="1.27" width="0" layer="20"/>
<wire x1="1.27" y1="48.26" x2="0" y2="46.99" width="0" layer="20" curve="90"/>
<wire x1="24.13" y1="48.26" x2="25.4" y2="46.99" width="0" layer="20" curve="-90"/>
<wire x1="24.13" y1="0" x2="25.4" y2="1.27" width="0" layer="20" curve="90"/>
<wire x1="1.27" y1="0" x2="0" y2="1.27" width="0" layer="20" curve="-90"/>
<wire x1="1.27" y1="48.26" x2="24.13" y2="48.26" width="0" layer="20"/>
<wire x1="25.4" y1="46.99" x2="25.4" y2="1.27" width="0" layer="20"/>
<text>Particle
Spark/Photon
NodeMCU
Adapter
V1.0</text>
<text>hallard.me</text>
<text>Open to upload firmware
Close to enable Téléinfo
</text>
<text>Particle
NodeMCU
Adapter
V1.0</text>
<text>Open to upload
Close Téléinfo
</text>
<text>hallard.me</text>
<text>Spark
A0
</text>
<text>Spark
D0
</text>
<text>Spark
VIN
</text>
<text>Spark
3V3
</text>
<text>Node
VIN
</text>
<text>Node
3V3
</text>
<text>Spark
A0
</text>
<text>Spark
D0
</text>
<text>Spark
VIN
</text>
<text>Spark
3V3
</text>
<text>Node 3V3
</text>
<text>Node VIN
</text>
<text>Node A0
</text>
<text>Node D0
</text>
<text>Node A0
</text>
<text>Node D0
</text>
<text>JP1</text>
</plain>
<libraries>
<library name="Spark">
<packages>
<package name="SPARK_CORE">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02_LOCK">
</package>
<package name="1X15">
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-M">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$2" library="Spark" package="SPARK_CORE" value="SPARK_CORECORE"/>
<element name="JP1" library="SparkFun-Connectors" package="1X02_LOCK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X15" value="">
<attribute name="VALUE"/>
</element>
<element name="JP3" library="SparkFun-Connectors" package="1X15" value="">
<attribute name="VALUE"/>
</element>
<element name="LOGO1" library="SparkFun-Aesthetics" package="OSHW-LOGO-M" value="OSHW-LOGOM"/>
<element name="LOGO2" library="SparkFun-Aesthetics" package="OSHW-LOGO-M" value="OSHW-LOGOM"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U$2" pad="2"/>
<contactref element="U$2" pad="21"/>
<contactref element="JP2" pad="14"/>
<contactref element="JP2" pad="10"/>
<contactref element="JP3" pad="14"/>
<contactref element="JP3" pad="7"/>
</signal>
<signal name="RST">
<contactref element="U$2" pad="23"/>
<contactref element="JP2" pad="13"/>
</signal>
<signal name="A0">
<contactref element="U$2" pad="12"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="MOSI">
<contactref element="U$2" pad="7"/>
<contactref element="JP3" pad="10"/>
</signal>
<signal name="MISO">
<contactref element="U$2" pad="8"/>
<contactref element="JP3" pad="9"/>
</signal>
<signal name="SCK">
<contactref element="U$2" pad="9"/>
<contactref element="JP3" pad="8"/>
</signal>
<signal name="3V3*">
<contactref element="U$2" pad="22"/>
</signal>
<signal name="3V3">
<contactref element="U$2" pad="24"/>
<contactref element="JP2" pad="11"/>
<contactref element="JP3" pad="15"/>
<contactref element="JP3" pad="6"/>
</signal>
<signal name="N$1">
<contactref element="JP1" pad="1"/>
<contactref element="U$2" pad="4"/>
</signal>
<signal name="SDA">
<contactref element="U$2" pad="13"/>
<contactref element="JP3" pad="3"/>
</signal>
<signal name="SCL">
<contactref element="U$2" pad="14"/>
<contactref element="JP3" pad="2"/>
</signal>
<signal name="SS">
<contactref element="JP3" pad="11"/>
<contactref element="U$2" pad="10"/>
</signal>
<signal name="VIN">
<contactref element="JP2" pad="15"/>
<contactref element="U$2" pad="1"/>
</signal>
<signal name="GPIO16">
<contactref element="JP3" pad="1"/>
<contactref element="U$2" pad="20"/>
</signal>
<signal name="GPIO1">
<contactref element="JP3" pad="13"/>
</signal>
<signal name="GPIO3">
<contactref element="JP3" pad="12"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="GPIO2">
<contactref element="JP3" pad="5"/>
<contactref element="U$2" pad="15"/>
</signal>
<signal name="GPIO0">
<contactref element="JP3" pad="4"/>
<contactref element="U$2" pad="19"/>
<contactref element="U$2" pad="17"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
