<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.2.2">
<drawing>
<board>
<plain>
<wire x1="24.13" y1="34.29" x2="39.37" y2="34.29" width="0.1524" layer="20"/>
<wire x1="39.37" y1="34.29" x2="39.37" y2="19.05" width="0.1524" layer="20"/>
<wire x1="39.37" y1="19.05" x2="24.13" y2="19.05" width="0.1524" layer="20"/>
<wire x1="24.13" y1="19.05" x2="24.13" y2="34.29" width="0.1524" layer="20"/>
<text>V2</text>
<text>3V</text>
<text>CSB</text>
<text>GND</text>
<text>GND</text>
<text>EN</text>
<text>SDA</text>
<text>SCL</text>
<text>5V</text>
<text>Baro Pressure</text>
<text>MS5607-02BA03 with
PCA9617 BOB</text>
<text>10Nov17</text>
<text>MicroWeather Project</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X05_NO_SILK">
<description>No outline in silkscreen</description>
</package>
</packages>
</library>
<library name="TE">
<packages>
<package name="MS5607-02BA03">
</package>
</packages>
</library>
<library name="KEMET">
<packages>
<package name="0805_B">
</package>
</packages>
</library>
<library name="ERIC">
<description>CDS Photoconductive Photocell.
PDV-P7002
Digikey part PDV-P7002-ND</description>
<packages>
<package name="MSOP_8_LEAD">
<description>Based off of Microchip packaging document. with of pads geometric mean of largest and smallest. Pad extends beyond largest width by 0.03, while centered on 2.2mm&lt;br&gt;
70% cream coverage</description>
</package>
</packages>
</library>
<library name="Stackpole">
<packages>
<package name="0805">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="TE" package="MS5607-02BA03" value="MS5607-02BA03"/>
<element name="CS" library="KEMET" package="0805_B" value="0.1u">
<attribute name="VALUE"/>
</element>
<element name="U$2" library="ERIC" package="MSOP_8_LEAD" value="PCA9617A"/>
<element name="CA" library="KEMET" package="0805_B" value="0.1u"/>
<element name="CB" library="KEMET" package="0805_B" value="0.1u"/>
<element name="RSDA" library="Stackpole" package="0805" value="10K"/>
<element name="RSCL" library="Stackpole" package="0805" value="10K"/>
<element name="J1" library="SparkFun-Connectors" package="1X05_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X05_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="3V">
<contactref element="U$1" pad="1"/>
<contactref element="CS" pad="2"/>
<contactref element="RSCL" pad="2"/>
<contactref element="RSDA" pad="2"/>
<contactref element="CA" pad="2"/>
<contactref element="U$2" pad="1"/>
<contactref element="U$1" pad="2"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="GND">
<contactref element="U$2" pad="4"/>
<contactref element="U$1" pad="3"/>
<contactref element="CA" pad="1"/>
<contactref element="CB" pad="1"/>
<contactref element="CS" pad="1"/>
<contactref element="J1" pad="5"/>
<contactref element="J2" pad="5"/>
</signal>
<signal name="5V">
<contactref element="U$2" pad="8"/>
<contactref element="CB" pad="2"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="8"/>
<contactref element="U$2" pad="2"/>
<contactref element="RSCL" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="U$1" pad="7"/>
<contactref element="U$2" pad="3"/>
<contactref element="RSDA" pad="1"/>
</signal>
<signal name="SDA">
<contactref element="U$2" pad="6"/>
<contactref element="J1" pad="3"/>
</signal>
<signal name="SCL">
<contactref element="U$2" pad="7"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="EN">
<contactref element="U$2" pad="5"/>
<contactref element="J1" pad="4"/>
</signal>
<signal name="CSB">
<contactref element="U$1" pad="5"/>
<contactref element="U$1" pad="4"/>
<contactref element="J2" pad="4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
