<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<hole x="2.54" y="35.56" drill="3.2"/>
<hole x="48.26" y="35.56" drill="3.2"/>
<hole x="48.26" y="2.54" drill="3.2"/>
<hole x="2.54" y="2.54" drill="3.2"/>
<wire x1="0" y1="0" x2="0" y2="38.1" width="0" layer="20"/>
<wire x1="0" y1="38.1" x2="50.8" y2="38.1" width="0" layer="20"/>
<wire x1="50.8" y1="38.1" x2="50.8" y2="0" width="0" layer="20"/>
<wire x1="50.8" y1="0" x2="0" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="con-lstb">
<description>&lt;b&gt;Pin Headers&lt;/b&gt;&lt;p&gt;
Naming:&lt;p&gt;
MA = male&lt;p&gt;
# contacts - # rows&lt;p&gt;
W = angled&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MA04-1">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="MA08-1">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Particle-Devices">
<description>&lt;h3&gt;Reference foot prints for Particle devices&lt;/h3&gt;
In this library you'll find foot prints to make circuit boards using the Particle devices: Spark Core, Photon and Electron.&lt;br&gt;&lt;br&gt;
There are for reference and you may need to adjust them for your application. See https://docs.particle.io for more details on the recommended layouts for Particle devices.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Designed by Particle. Distributed under a Creative Commons Attribution, Share-Alike license. Development kits based on this library should be distributed under a similar license. Commercial products using this library as a reference design need not comply with this license; further questions can be sent to hello@particle.io. Check license.txt for more information.</description>
<packages>
<package name="PHOTON_SMD">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="H3" library="con-lstb" package="MA04-1" value="Display">
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="H2" library="con-lstb" package="MA04-1" value="PBSW">
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="H1" library="con-lstb" package="MA08-1" value="Tmp Sensors">
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="PHOTON" library="Particle-Devices" package="PHOTON_SMD" value="PHOTON_SMD"/>
</elements>
<signals>
<signal name="VBAT">
<contactref element="PHOTON" pad="22"/>
</signal>
<signal name="SCL">
<contactref element="H3" pad="1"/>
<contactref element="PHOTON" pad="14"/>
</signal>
<signal name="SDA">
<contactref element="H3" pad="2"/>
<contactref element="PHOTON" pad="13"/>
</signal>
<signal name="GND">
<contactref element="PHOTON" pad="21"/>
<contactref element="PHOTON" pad="2"/>
<contactref element="H1" pad="1"/>
<contactref element="H1" pad="8"/>
<contactref element="H3" pad="4"/>
<contactref element="H2" pad="4"/>
<contactref element="H2" pad="1"/>
</signal>
<signal name="SDI">
<contactref element="H1" pad="6"/>
<contactref element="PHOTON" pad="7"/>
</signal>
<signal name="CS1">
<contactref element="H1" pad="5"/>
<contactref element="PHOTON" pad="11"/>
</signal>
<signal name="CS0">
<contactref element="H1" pad="4"/>
<contactref element="PHOTON" pad="10"/>
</signal>
<signal name="SDO">
<contactref element="H1" pad="3"/>
<contactref element="PHOTON" pad="8"/>
</signal>
<signal name="3V3">
<contactref element="H1" pad="2"/>
<contactref element="PHOTON" pad="24"/>
</signal>
<signal name="SCK">
<contactref element="H1" pad="7"/>
<contactref element="PHOTON" pad="9"/>
</signal>
<signal name="VIN">
<contactref element="H3" pad="3"/>
<contactref element="PHOTON" pad="1"/>
</signal>
<signal name="ON">
<contactref element="PHOTON" pad="17"/>
<contactref element="H2" pad="2"/>
</signal>
<signal name="F/C">
<contactref element="PHOTON" pad="15"/>
<contactref element="H2" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
