<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.3.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="17.78" y2="0" width="0" layer="20"/>
<wire x1="17.78" y1="0" x2="17.8308" y2="36.449" width="0" layer="20"/>
<wire x1="17.8308" y1="36.449" x2="0.0508" y2="36.449" width="0" layer="20"/>
<wire x1="0.0508" y1="36.449" x2="0" y2="0" width="0" layer="20"/>
<text>ANT</text>
<text>3V3</text>
<text>GND</text>
<text>SCK</text>
<text>MISO</text>
<text>MOSI</text>
<text>IRQ</text>
<text>CSN</text>
<text>GND</text>
<text>TD RFM69 V1.0</text>
<text>3.3V Signals: No R's
   Bridge 3 jumpers</text>
<text>5V Signals: All R's
   3 jumpers open</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X01">
</package>
<package name="1X07">
</package>
</packages>
</library>
<library name="TD22057">
<packages>
<package name="R_0805">
<description>&lt;b&gt;0805 Large pad size&lt;/b&gt;&lt;p&gt;

Digikey recommended sizing</description>
</package>
<package name="RFM69W_MS">
<description>Radio module based on the RFM69 chip from HopeRF</description>
</package>
<package name="CAP_0805">
<description>&lt;b&gt;0805 Large pad size&lt;/b&gt;&lt;p&gt;

Digikey recommended sizing</description>
</package>
<package name="PAD-JUMPER-2-NO_YES_SILK">
<description>Small solder jumper with no paste layer so it will open after reflow.</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="RFM69W" library="TD22057" package="RFM69W_MS" value="RADIO_RFM69W_MS"/>
<element name="R1" library="TD22057" package="R_0805" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="TD22057" package="R_0805" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="TD22057" package="R_0805" value="4k7">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="TD22057" package="R_0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="TD22057" package="R_0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="TD22057" package="R_0805" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SJ1" library="TD22057" package="PAD-JUMPER-2-NO_YES_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="SJ2" library="TD22057" package="PAD-JUMPER-2-NO_YES_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="SJ3" library="TD22057" package="PAD-JUMPER-2-NO_YES_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X01" value="ANT"/>
<element name="JP3" library="SparkFun-Connectors" package="1X01" value="GND"/>
<element name="JP1" library="SparkFun-Connectors" package="1X07" value=""/>
<element name="C1" library="TD22057" package="CAP_0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="TD22057" package="CAP_0805" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="SJ3" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="RFM69W" pad="12"/>
</signal>
<signal name="N$7">
<contactref element="SJ2" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$9">
<contactref element="SJ3" pad="2"/>
<contactref element="R5" pad="2"/>
<contactref element="JP1" pad="5"/>
</signal>
<signal name="N$5">
<contactref element="SJ2" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="RFM69W" pad="14"/>
</signal>
<signal name="N$6">
<contactref element="R1" pad="2"/>
<contactref element="SJ1" pad="2"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$10">
<contactref element="SJ1" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="RFM69W" pad="15"/>
</signal>
<signal name="N$8">
</signal>
<signal name="+3V3">
<contactref element="C2" pad="1"/>
<contactref element="RFM69W" pad="8"/>
<contactref element="C1" pad="1"/>
<contactref element="JP1" pad="7"/>
</signal>
<signal name="GND">
<contactref element="R2" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="RFM69W" pad="9"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="RFM69W" pad="11"/>
<contactref element="JP3" pad="1"/>
<contactref element="JP1" pad="6"/>
</signal>
<signal name="N$3">
<contactref element="RFM69W" pad="10"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="IRQ">
<contactref element="RFM69W" pad="2"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="JP1" pad="4"/>
<contactref element="RFM69W" pad="13"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
