<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.1.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="90" y2="0" width="0" layer="20"/>
<wire x1="90" y1="0" x2="90" y2="50" width="0" layer="20"/>
<wire x1="90" y1="50" x2="0" y2="50" width="0" layer="20"/>
<wire x1="0" y1="50" x2="0" y2="39.1" width="0" layer="20"/>
<wire x1="0" y1="5.4" x2="0" y2="0" width="0" layer="20"/>
<wire x1="0" y1="39.1" x2="4.25" y2="39.1" width="0" layer="20"/>
<wire x1="4.25" y1="39.1" x2="7.35" y2="36" width="0" layer="20" curve="-90"/>
<wire x1="7.35" y1="8.5" x2="4.25" y2="5.4" width="0" layer="20" curve="-90"/>
<wire x1="4.25" y1="5.4" x2="0" y2="5.4" width="0" layer="20"/>
<hole x="21" y="45" drill="3.5"/>
<hole x="21" y="20" drill="3.5"/>
<hole x="58" y="45" drill="3.5"/>
<hole x="65" y="20" drill="3.5"/>
<text>+5V</text>
<text>+3.3v</text>
<wire x1="7.375" y1="36" x2="7.375" y2="8.5" width="0" layer="20"/>
</plain>
<libraries>
<library name="con-molex">
<description>&lt;b&gt;Molex Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="53047-06">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 1.25 mm (.049 inch) pitch header&lt;p&gt;
straight&lt;br&gt;
Sourcxe: http://www.molex.com/pdm_docs/sd/530470210_sd.pdf</description>
</package>
<package name="53398-02">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 1.25 mm (.049 inch) pitch header&lt;p&gt;
SMT&lt;p&gt;
straight</description>
</package>
<package name="53047-02">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 1.25 mm (.049 inch) pitch header&lt;p&gt;
straight&lt;br&gt;
Sourcxe: http://www.molex.com/pdm_docs/sd/530470210_sd.pdf</description>
</package>
<package name="53047-08">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 1.25 mm (.049 inch) pitch header&lt;p&gt;
straight&lt;br&gt;
Sourcxe: http://www.molex.com/pdm_docs/sd/530470210_sd.pdf</description>
</package>
<package name="53047-05">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 1.25 mm (.049 inch) pitch header&lt;p&gt;
straight&lt;br&gt;
Sourcxe: http://www.molex.com/pdm_docs/sd/530470210_sd.pdf</description>
</package>
<package name="53047-10">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 1.25 mm (.049 inch) pitch header&lt;p&gt;
straight&lt;br&gt;
Sourcxe: http://www.molex.com/pdm_docs/sd/530470210_sd.pdf</description>
</package>
<package name="53047-04">
<description>&lt;b&gt;CONNECTOR&lt;/b&gt;&lt;p&gt;
wire to board 1.25 mm (.049 inch) pitch header&lt;p&gt;
straight&lt;br&gt;
Sourcxe: http://www.molex.com/pdm_docs/sd/530470210_sd.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CPOL-RADIAL-1000UF-63V">
</package>
<package name="0603-CAP">
</package>
<package name="0603-RES">
</package>
<package name="0603">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
<package name="PANASONIC_D">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-3">
</package>
<package name="SOD-323">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-0603">
</package>
</packages>
</library>
<library name="SparkFun-AnalogIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of analog ICs- DACs, ADCs, video chips, op-amps, and others.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt;Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; Fits JEDEC packages (narrow SOIC-8)</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X01NS-KIT">
</package>
</packages>
</library>
<library name="texas">
<description>&lt;b&gt;Texas Instruments Devices&lt;/b&gt;&lt;p&gt;
 &lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SO-16">
<description>&lt;b&gt;Small Outline Integrated Circuit&lt;/b&gt;</description>
</package>
<package name="SSOP-8">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="murata-supplys">
<packages>
<package name="MURATA_NMH">
</package>
</packages>
</library>
<library name="Elmo">
<packages>
<package name="ELMO_TWITTER_SOCKET">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SMD_DIP6">
</package>
</packages>
</library>
<library name="dc-dc-converter">
<description>&lt;b&gt;DC-DC Converters&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SIP_4">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="ABS_RMB20" library="con-molex" package="53047-06" value="">
<attribute name="OC_NEWARK" value="03M2965"/>
<attribute name="MPN" value="53047-0610-C"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="9733078"/>
</element>
<element name="C1" library="SparkFun-Passives" package="CPOL-RADIAL-1000UF-63V" value="220uF"/>
<element name="C10" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF">
<attribute name="PROD_ID" value="CAP-08604"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF">
<attribute name="PROD_ID" value="CAP-08604"/>
</element>
<element name="C3" library="SparkFun-Passives" package="0603-CAP" value=".1uF"/>
<element name="C4" library="SparkFun-Passives" package="0603-CAP" value=".1uF"/>
<element name="C5" library="SparkFun-Passives" package="0603-CAP" value=".1uf"/>
<element name="ERROR" library="SparkFun-LED" package="LED-0603" value="RED">
<attribute name="PROD_ID" value="DIO-00819"/>
</element>
<element name="FAN_CON" library="SparkFun-AnalogIC" package="SO08" value="MIC502"/>
<element name="FILM_CAP" library="SparkFun-Connectors" package="1X01NS-KIT" value=""/>
<element name="FILM_CAP-" library="SparkFun-Connectors" package="1X01NS-KIT" value=""/>
<element name="HALLS" library="con-molex" package="53047-05" value="53047-05">
<attribute name="OC_NEWARK" value="38C9901"/>
<attribute name="MPN" value="53047-0510"/>
<attribute name="MF" value="MOLEX"/>
<attribute name="OC_FARNELL" value="9732861"/>
</element>
<element name="INC_RMB20" library="con-molex" package="53047-08" value="">
<attribute name="OC_NEWARK" value="98K9826"/>
<attribute name="MPN" value="53047-0810"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1012258"/>
</element>
<element name="LC_AMP" library="texas" package="SO-16" value="INA125"/>
<element name="LED1" library="SparkFun-LED" package="LED-0603" value="RED">
<attribute name="PROD_ID" value="DIO-00819"/>
</element>
<element name="LED2" library="SparkFun-LED" package="LED-0603" value="GREEN">
<attribute name="PROD_ID" value="DIO-00821"/>
</element>
<element name="LOAD_CELL" library="con-molex" package="53047-05" value="">
<attribute name="OC_NEWARK" value="38C9901"/>
<attribute name="MPN" value="53047-0510"/>
<attribute name="MF" value="MOLEX"/>
<attribute name="OC_FARNELL" value="9732861"/>
</element>
<element name="LOCK" library="con-molex" package="53047-05" value="">
<attribute name="OC_NEWARK" value="38C9901"/>
<attribute name="MPN" value="53047-0510"/>
<attribute name="MF" value="MOLEX"/>
<attribute name="OC_FARNELL" value="9732861"/>
</element>
<element name="LOGIC_IN" library="con-molex" package="53047-10" value="">
<attribute name="OC_NEWARK" value="57H4711"/>
<attribute name="MPN" value="53047-1010"/>
<attribute name="MF" value="MOLEX"/>
<attribute name="OC_FARNELL" value="9733086"/>
</element>
<element name="LOGIC_OUT" library="con-molex" package="53047-10" value="">
<attribute name="OC_NEWARK" value="57H4711"/>
<attribute name="MPN" value="53047-1010"/>
<attribute name="MF" value="MOLEX"/>
<attribute name="OC_FARNELL" value="9733086"/>
</element>
<element name="OVERTEMP" library="SparkFun-LED" package="LED-0603" value="RED">
<attribute name="PROD_ID" value="DIO-00819"/>
</element>
<element name="Q1" library="SparkFun-DiscreteSemi" package="SOT23-3" value="MMBT2222A">
<attribute name="PROD_ID" value="TRANS-08049"/>
</element>
<element name="Q2" library="SparkFun-DiscreteSemi" package="SOT23-3" value="PMBT3906">
<attribute name="PROD_ID" value="TRANS-08052"/>
</element>
<element name="Q3" library="SparkFun-DiscreteSemi" package="SOT23-3" value="MMBT2222A">
<attribute name="PROD_ID" value="TRANS-08049"/>
</element>
<element name="R1" library="SparkFun-Passives" package="0603-RES" value="400"/>
<element name="R10" library="SparkFun-Passives" package="0603-RES" value="60"/>
<element name="R11" library="SparkFun-Resistors" package="0603-RES" value="33k"/>
<element name="R12" library="SparkFun-Resistors" package="0603-RES" value="100"/>
<element name="R13" library="SparkFun-Resistors" package="0603-RES" value="250"/>
<element name="R14" library="SparkFun-Resistors" package="0603-RES" value="10k"/>
<element name="R15" library="SparkFun-Resistors" package="0603-RES" value="56k"/>
<element name="R16" library="SparkFun-Resistors" package="0603-RES" value="56k"/>
<element name="R17" library="SparkFun-Resistors" package="0603-RES" value="47k"/>
<element name="R18" library="SparkFun-Resistors" package="0603-RES" value="2.2k"/>
<element name="R20" library="SparkFun-Resistors" package="0603-RES" value="33k"/>
<element name="R22" library="SparkFun-Passives" package="0603-RES" value="1.6k/4k"/>
<element name="R3" library="SparkFun-Resistors" package="0603-RES" value="100k"/>
<element name="R6" library="SparkFun-Passives" package="0603-RES" value="400"/>
<element name="RUN" library="SparkFun-LED" package="LED-0603" value="GREEN">
<attribute name="PROD_ID" value="DIO-00821"/>
</element>
<element name="THERM1" library="con-molex" package="53047-02" value="">
<attribute name="OC_NEWARK" value="57H4701"/>
<attribute name="MPN" value="53047-0210"/>
<attribute name="MF" value="MOLEX"/>
<attribute name="OC_FARNELL" value="9733051"/>
</element>
<element name="THERM2" library="con-molex" package="53047-02" value="">
<attribute name="OC_NEWARK" value="57H4701"/>
<attribute name="MPN" value="53047-0210"/>
<attribute name="MF" value="MOLEX"/>
<attribute name="OC_FARNELL" value="9733051"/>
</element>
<element name="24-&gt;15" library="murata-supplys" package="MURATA_NMH" value=""/>
<element name="C7" library="SparkFun-Passives" package="0603-CAP" value=".1uF"/>
<element name="D1" library="SparkFun-LED" package="LED-0603" value="LINK_IN">
<attribute name="PROD_ID" value="DIO-00821"/>
</element>
<element name="D2" library="SparkFun-LED" package="LED-0603" value="SPEED_IN">
<attribute name="PROD_ID" value="DIO-09003"/>
</element>
<element name="R4" library="SparkFun-Passives" package="0603-RES" value="200"/>
<element name="R5" library="SparkFun-Passives" package="0603-RES" value="200"/>
<element name="D3" library="SparkFun-LED" package="LED-0603" value="LINK_OUT">
<attribute name="PROD_ID" value="DIO-00821"/>
</element>
<element name="D5" library="SparkFun-LED" package="LED-0603" value="SPEED_OUT">
<attribute name="PROD_ID" value="DIO-09003"/>
</element>
<element name="R7" library="SparkFun-Passives" package="0603-RES" value="200"/>
<element name="R8" library="SparkFun-Passives" package="0603-RES" value="200"/>
<element name="D4" library="SparkFun-DiscreteSemi" package="SOD-323" value="">
<attribute name="PROD_ID" value="DIO-09646"/>
</element>
<element name="USB" library="con-molex" package="53047-04" value="">
<attribute name="OC_NEWARK" value="38C9900"/>
<attribute name="MPN" value="53047-0410"/>
<attribute name="MF" value="WALDOM/MOLEX"/>
<attribute name="OC_FARNELL" value="9733060"/>
</element>
<element name="LEDS" library="con-molex" package="53047-04" value="">
<attribute name="OC_NEWARK" value="38C9900"/>
<attribute name="MPN" value="53047-0410"/>
<attribute name="MF" value="WALDOM/MOLEX"/>
<attribute name="OC_FARNELL" value="9733060"/>
</element>
<element name="C8" library="SparkFun-Capacitors" package="PANASONIC_D" value="100uF"/>
<element name="U$3" library="SparkFun-Passives" package="0603" value="603_FILLTER_BEAD"/>
<element name="U$4" library="SparkFun-Passives" package="0603" value="BEAD"/>
<element name="U$5" library="SparkFun-Passives" package="0603" value="BEAD"/>
<element name="48V" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="24V" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="15V" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="5V" library="SparkFun-LED" package="LED-0603" value=""/>
<element name="R21" library="SparkFun-Resistors" package="0603-RES" value="4.7k"/>
<element name="R23" library="SparkFun-Resistors" package="0603-RES" value="2.2k"/>
<element name="R24" library="SparkFun-Resistors" package="0603-RES" value="1.3k"/>
<element name="R25" library="SparkFun-Resistors" package="0603-RES" value="100"/>
<element name="R19" library="SparkFun-Resistors" package="0603-RES" value="10k"/>
<element name="FOOT_SENSOR" library="con-molex" package="53047-04" value="">
<attribute name="OC_NEWARK" value="38C9900"/>
<attribute name="MPN" value="53047-0410"/>
<attribute name="MF" value="WALDOM/MOLEX"/>
<attribute name="OC_FARNELL" value="9733060"/>
</element>
<element name="U$1" library="Elmo" package="ELMO_TWITTER_SOCKET" value="ELMO_TWITTERSOCKET_TWITTER"/>
<element name="U$7" library="texas" package="SSOP-8" value="SN74LVC2G86"/>
<element name="U$2" library="SparkFun-Electromechanical" package="SMD_DIP6" value="LCA710S"/>
<element name="R2" library="SparkFun-Resistors" package="0603-RES" value="360"/>
<element name="FAN" library="con-molex" package="53398-02" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="24-&gt;5" library="dc-dc-converter" package="SIP_4" value="SPU02N-05"/>
</elements>
<signals>
<signal name="VP+">
<contactref element="C1" pad="1"/>
<contactref element="FILM_CAP" pad="1"/>
<contactref element="R21" pad="2"/>
<contactref element="U$1" pad="VP+"/>
</signal>
<signal name="PR">
<contactref element="C1" pad="2"/>
<contactref element="FILM_CAP-" pad="1"/>
<contactref element="48V" pad="C"/>
<contactref element="U$1" pad="PR"/>
</signal>
<signal name="GND">
<contactref element="24-&gt;15" pad="0V"/>
<contactref element="LOGIC_IN" pad="10"/>
<contactref element="LOGIC_OUT" pad="10"/>
<contactref element="HALLS" pad="5"/>
<contactref element="ABS_RMB20" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="LOAD_CELL" pad="3"/>
<contactref element="LOAD_CELL" pad="5"/>
<contactref element="LC_AMP" pad="12"/>
<contactref element="INC_RMB20" pad="8"/>
<contactref element="C10" pad="2"/>
<contactref element="LC_AMP" pad="5"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="Q3" pad="2"/>
<contactref element="R12" pad="1"/>
<contactref element="FAN_CON" pad="4"/>
<contactref element="C5" pad="2"/>
<contactref element="R11" pad="1"/>
<contactref element="R16" pad="1"/>
<contactref element="LOCK" pad="3"/>
<contactref element="R20" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="USB" pad="4"/>
<contactref element="LEDS" pad="1"/>
<contactref element="C8" pad="-"/>
<contactref element="15V" pad="C"/>
<contactref element="5V" pad="C"/>
<contactref element="FOOT_SENSOR" pad="2"/>
<contactref element="U$1" pad="COMRET"/>
<contactref element="U$1" pad="COMRET_2"/>
<contactref element="U$1" pad="COMRET_3"/>
<contactref element="U$1" pad="COMRET_4"/>
<contactref element="U$1" pad="COMRET_5"/>
<contactref element="U$1" pad="COMRET_6"/>
<contactref element="U$1" pad="ANALOG1-"/>
<contactref element="U$1" pad="COMRET_7"/>
<contactref element="U$7" pad="GND"/>
<contactref element="U$2" pad="-LED"/>
<contactref element="24-&gt;5" pad="-VOUT"/>
</signal>
<signal name="+5VE">
<contactref element="HALLS" pad="1"/>
<contactref element="ABS_RMB20" pad="6"/>
<contactref element="INC_RMB20" pad="1"/>
<contactref element="R14" pad="2"/>
<contactref element="Q2" pad="2"/>
<contactref element="LOCK" pad="1"/>
<contactref element="FAN_CON" pad="8"/>
<contactref element="R15" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="R17" pad="2"/>
<contactref element="THERM1" pad="2"/>
<contactref element="LOCK" pad="4"/>
<contactref element="THERM2" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="D4" pad="C"/>
<contactref element="LEDS" pad="2"/>
<contactref element="C8" pad="+"/>
<contactref element="R25" pad="2"/>
<contactref element="OVERTEMP" pad="A"/>
<contactref element="R19" pad="2"/>
<contactref element="U$1" pad="+5VE"/>
<contactref element="U$7" pad="VCC"/>
<contactref element="U$7" pad="2A"/>
<contactref element="24-&gt;5" pad="+VOUT"/>
</signal>
<signal name="VL+">
<contactref element="24-&gt;15" pad="+VIN"/>
<contactref element="LOGIC_IN" pad="1"/>
<contactref element="LOGIC_OUT" pad="1"/>
<contactref element="R23" pad="2"/>
<contactref element="FOOT_SENSOR" pad="3"/>
<contactref element="U$1" pad="VL+"/>
<contactref element="FAN" pad="1"/>
<contactref element="24-&gt;5" pad="-VIN"/>
</signal>
<signal name="VL-">
<contactref element="24-&gt;15" pad="-VIN"/>
<contactref element="LOGIC_IN" pad="8"/>
<contactref element="LOGIC_OUT" pad="8"/>
<contactref element="24V" pad="C"/>
<contactref element="FOOT_SENSOR" pad="4"/>
<contactref element="U$1" pad="VL-"/>
<contactref element="U$2" pad="LOAD2"/>
<contactref element="24-&gt;5" pad="+VIN"/>
</signal>
<signal name="-15V">
<contactref element="24-&gt;15" pad="-VOUT"/>
<contactref element="LC_AMP" pad="3"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="+15V">
<contactref element="24-&gt;15" pad="+VOUT"/>
<contactref element="LC_AMP" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="LC_AMP" pad="2"/>
<contactref element="R24" pad="2"/>
</signal>
<signal name="STO_RET">
<contactref element="LOGIC_IN" pad="7"/>
<contactref element="LOGIC_OUT" pad="7"/>
<contactref element="U$1" pad="STO_RET"/>
</signal>
<signal name="IN_RX-">
<contactref element="LOGIC_IN" pad="4"/>
<contactref element="U$1" pad="PHY_IN_TX-"/>
</signal>
<signal name="IN_RX+">
<contactref element="LOGIC_IN" pad="5"/>
<contactref element="U$1" pad="PHY_IN_TX+"/>
</signal>
<signal name="IN_TX-">
<contactref element="LOGIC_IN" pad="3"/>
<contactref element="U$1" pad="PHY_IN_RX-"/>
</signal>
<signal name="IN_TX+">
<contactref element="LOGIC_IN" pad="2"/>
<contactref element="U$1" pad="PHY_IN_RX+"/>
</signal>
<signal name="OUT_TX+">
<contactref element="LOGIC_OUT" pad="2"/>
<contactref element="U$1" pad="PHY_OUT_TX+"/>
</signal>
<signal name="OUT_TX-">
<contactref element="LOGIC_OUT" pad="3"/>
<contactref element="U$1" pad="PHY_OUT_TX-"/>
</signal>
<signal name="OUT_RX+">
<contactref element="LOGIC_OUT" pad="5"/>
<contactref element="U$1" pad="PHY_OUT_RX+"/>
</signal>
<signal name="OUT_RX-">
<contactref element="LOGIC_OUT" pad="4"/>
<contactref element="U$1" pad="PHY_OUT_RX-"/>
</signal>
<signal name="STO">
<contactref element="LOGIC_OUT" pad="6"/>
<contactref element="LOGIC_IN" pad="6"/>
<contactref element="U$1" pad="STO1"/>
<contactref element="U$1" pad="STO2"/>
</signal>
<signal name="LED_DATA_IN">
<contactref element="LOGIC_IN" pad="9"/>
<contactref element="LEDS" pad="3"/>
</signal>
<signal name="LED_DATA_OUT">
<contactref element="LOGIC_OUT" pad="9"/>
<contactref element="LEDS" pad="4"/>
</signal>
<signal name="3.3V">
<contactref element="R1" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="U$1" pad="3.3V"/>
<contactref element="U$1" pad="3.3V_2"/>
</signal>
<signal name="ABS_CLK+">
<contactref element="ABS_RMB20" pad="5"/>
<contactref element="U$1" pad="PORTA_ENC_A+/ABS_CLK+"/>
</signal>
<signal name="ABS_CLK-">
<contactref element="ABS_RMB20" pad="4"/>
<contactref element="U$1" pad="PORTA_ENC_A-/ABS_CLK-"/>
</signal>
<signal name="ABS_DATA+">
<contactref element="ABS_RMB20" pad="3"/>
<contactref element="U$1" pad="PORTA_ENC_B+/ABS_DATA+"/>
</signal>
<signal name="ABS_DATA-">
<contactref element="ABS_RMB20" pad="2"/>
<contactref element="U$1" pad="PORTA_ENC_B-/ABS_DATA-"/>
</signal>
<signal name="INC_ENC_A-">
<contactref element="INC_RMB20" pad="2"/>
<contactref element="U$1" pad="PORTB_ENC_A-/SIN-"/>
</signal>
<signal name="INC_ENC_A+">
<contactref element="INC_RMB20" pad="3"/>
<contactref element="U$1" pad="PORTB_ENC_A+/SIN+"/>
</signal>
<signal name="INC_ENC_B-">
<contactref element="INC_RMB20" pad="4"/>
<contactref element="U$1" pad="PORTB_ENC_B-/COS-"/>
</signal>
<signal name="INC_ENC_B+">
<contactref element="INC_RMB20" pad="5"/>
<contactref element="U$1" pad="PORTB_ENC_B+/COS+"/>
</signal>
<signal name="INC_ENC_INDEX-">
<contactref element="INC_RMB20" pad="6"/>
<contactref element="U$1" pad="PORTB_ENC_INDEX-/ANALOG_I-"/>
</signal>
<signal name="INC_ENC_INDEX+">
<contactref element="INC_RMB20" pad="7"/>
<contactref element="U$1" pad="PORTB_ENC_INDEX+/ANALOG_I+"/>
</signal>
<signal name="HA">
<contactref element="HALLS" pad="2"/>
<contactref element="U$1" pad="HA"/>
</signal>
<signal name="HB">
<contactref element="HALLS" pad="3"/>
<contactref element="U$1" pad="HB"/>
</signal>
<signal name="HC">
<contactref element="HALLS" pad="4"/>
<contactref element="U$1" pad="HC"/>
</signal>
<signal name="N$3">
<contactref element="RUN" pad="C"/>
<contactref element="U$1" pad="LED_ET_RUN"/>
</signal>
<signal name="N$4">
<contactref element="RUN" pad="A"/>
<contactref element="ERROR" pad="A"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="ERROR" pad="C"/>
<contactref element="U$1" pad="LED_ET_ERR"/>
</signal>
<signal name="N$2">
<contactref element="LED2" pad="C"/>
<contactref element="U$1" pad="LED2"/>
</signal>
<signal name="N$7">
<contactref element="LED1" pad="C"/>
<contactref element="U$1" pad="LED1"/>
</signal>
<signal name="N$9">
<contactref element="LED2" pad="A"/>
<contactref element="LED1" pad="A"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="AMP_LOAD_CELL+">
<contactref element="R22" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="U$1" pad="ANALOG1+"/>
</signal>
<signal name="LOCK_OUT_COMMAND">
<contactref element="U$1" pad="OUT1"/>
<contactref element="U$7" pad="1A"/>
</signal>
<signal name="LOCK_OUT_HALL">
<contactref element="LOCK" pad="5"/>
<contactref element="R19" pad="1"/>
<contactref element="U$1" pad="IN1"/>
<contactref element="U$7" pad="1B"/>
</signal>
<signal name="LOAD_CELL_EXT+">
<contactref element="C2" pad="1"/>
<contactref element="LOAD_CELL" pad="4"/>
<contactref element="LC_AMP" pad="16"/>
<contactref element="LC_AMP" pad="4"/>
</signal>
<signal name="LOAD_CELL_SIG+">
<contactref element="LOAD_CELL" pad="2"/>
<contactref element="U$5" pad="1"/>
</signal>
<signal name="LOAD_CELL_SIG-">
<contactref element="LOAD_CELL" pad="1"/>
<contactref element="U$4" pad="1"/>
</signal>
<signal name="N$21">
<contactref element="LC_AMP" pad="8"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="N$22">
<contactref element="LC_AMP" pad="9"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="UF_AMP_LOAD_CELL+">
<contactref element="LC_AMP" pad="11"/>
<contactref element="LC_AMP" pad="10"/>
<contactref element="U$3" pad="2"/>
</signal>
<signal name="LOCK_MOTOR_GND">
<contactref element="Q3" pad="3"/>
<contactref element="Q2" pad="3"/>
<contactref element="LOCK" pad="2"/>
<contactref element="D4" pad="A"/>
</signal>
<signal name="N$11">
<contactref element="Q3" pad="1"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="N$20">
<contactref element="R12" pad="2"/>
<contactref element="Q1" pad="2"/>
</signal>
<signal name="N$26">
<contactref element="Q1" pad="3"/>
<contactref element="Q2" pad="1"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="BRAKE">
<contactref element="Q1" pad="1"/>
<contactref element="U$7" pad="2Y"/>
</signal>
<signal name="LOCK_OUT">
<contactref element="R13" pad="1"/>
<contactref element="U$7" pad="2B"/>
<contactref element="U$7" pad="1Y"/>
</signal>
<signal name="OUT">
<contactref element="FAN_CON" pad="7"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="FAN_CON" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="R11" pad="2"/>
<contactref element="THERM1" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="R15" pad="1"/>
<contactref element="R16" pad="2"/>
<contactref element="FAN_CON" pad="3"/>
</signal>
<signal name="N$24">
<contactref element="FAN_CON" pad="2"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="N$28">
<contactref element="R17" pad="1"/>
<contactref element="FAN_CON" pad="6"/>
<contactref element="R18" pad="2"/>
</signal>
<signal name="N$27">
<contactref element="THERM2" pad="1"/>
<contactref element="FAN_CON" pad="5"/>
<contactref element="R20" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="R5" pad="2"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="N$6">
<contactref element="R8" pad="2"/>
<contactref element="D3" pad="A"/>
</signal>
<signal name="N$14">
<contactref element="R4" pad="2"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="N$15">
<contactref element="R7" pad="2"/>
<contactref element="D5" pad="A"/>
</signal>
<signal name="N$16">
<contactref element="D1" pad="C"/>
<contactref element="U$1" pad="PHY_IN_LINK_ACT"/>
</signal>
<signal name="N$17">
<contactref element="D3" pad="C"/>
<contactref element="U$1" pad="PHY_OUT_LINK_ACT"/>
</signal>
<signal name="N$18">
<contactref element="D2" pad="C"/>
<contactref element="U$1" pad="PHY_IN_SPEED"/>
</signal>
<signal name="N$19">
<contactref element="D5" pad="C"/>
<contactref element="U$1" pad="PHY_OUT_SPEED"/>
</signal>
<signal name="USB_VBUS">
<contactref element="USB" pad="1"/>
<contactref element="U$1" pad="USB_VBUS"/>
</signal>
<signal name="USBD+">
<contactref element="USB" pad="2"/>
<contactref element="U$1" pad="USBD+"/>
</signal>
<signal name="USBD-">
<contactref element="USB" pad="3"/>
<contactref element="U$1" pad="USBD-"/>
</signal>
<signal name="N$25">
<contactref element="R22" pad="2"/>
<contactref element="U$3" pad="1"/>
</signal>
<signal name="N$29">
<contactref element="U$5" pad="2"/>
<contactref element="LC_AMP" pad="6"/>
</signal>
<signal name="N$30">
<contactref element="U$4" pad="2"/>
<contactref element="LC_AMP" pad="7"/>
</signal>
<signal name="N$33">
<contactref element="R25" pad="1"/>
<contactref element="5V" pad="A"/>
</signal>
<signal name="N$34">
<contactref element="R24" pad="1"/>
<contactref element="15V" pad="A"/>
</signal>
<signal name="N$35">
<contactref element="R23" pad="1"/>
<contactref element="24V" pad="A"/>
</signal>
<signal name="N$36">
<contactref element="R21" pad="1"/>
<contactref element="48V" pad="A"/>
</signal>
<signal name="N$31">
<contactref element="OVERTEMP" pad="C"/>
<contactref element="R18" pad="1"/>
</signal>
<signal name="FOOT_SENSOR">
<contactref element="FOOT_SENSOR" pad="1"/>
<contactref element="U$1" pad="ANALOG_IN2"/>
</signal>
<signal name="M3">
<contactref element="U$1" pad="M3"/>
</signal>
<signal name="M2">
<contactref element="U$1" pad="M2"/>
</signal>
<signal name="M1">
<contactref element="U$1" pad="M1"/>
</signal>
<signal name="N$10">
<contactref element="U$2" pad="LOAD1"/>
<contactref element="FAN" pad="2"/>
</signal>
<signal name="N$32">
<contactref element="R2" pad="1"/>
<contactref element="U$2" pad="+LED"/>
</signal>
<signal name="N$8">
</signal>
<signal name="N$23">
</signal>
</signals>
</board>
</drawing>
</eagle>
