<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="31.801" y2="0" width="0" layer="20"/>
<wire x1="31.801" y1="0" x2="31.801" y2="15.23" width="0" layer="20"/>
<wire x1="31.801" y1="15.23" x2="0" y2="15.23" width="0" layer="20"/>
<wire x1="0" y1="15.23" x2="0" y2="0" width="0" layer="20"/>
<text>5V</text>
<text>3V3</text>
<text>GND</text>
<text>3V3</text>
<text>5V</text>
<text>A1</text>
<text>B1</text>
<text>Z1</text>
<text>GND</text>
<text>3V3</text>
<text>5V</text>
<text>A0</text>
<text>B0</text>
<text>Z0</text>
<text>GND</text>
<text>GND</text>
<text>A1</text>
<text>B1</text>
<text>Z1</text>
<text>5V</text>
<text>5V</text>
<text>A0</text>
<text>B0</text>
<text>Z0</text>
<text>GND</text>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
<description>&lt;p&gt;&lt;b&gt;Generic 2012 (0805) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X12">
<description>&lt;h3&gt;Plated Through Hole -12 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:12&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_12&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X03">
<description>&lt;h3&gt;Plated Through Hole - 3 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="con-jst-ph">
<description>&lt;b&gt;JST Connectors&lt;/b&gt; - PH 2.0 MM Series&lt;p&gt;
&lt;p&gt;THIS LIBRARY IS PROVIDED AS IS AND WITHOUT WARRANTY OF ANY KIND, EXPRESSED OR IMPLIED.&lt;br&gt;
USE AT YOUR OWN RISK!&lt;p&gt;
&lt;author&gt;Copyright (C) 2016, Bob Starr&lt;br&gt; http://www.bobstarr.net&lt;br&gt;&lt;/author&gt;</description>
<packages>
<package name="B5B-PH-K">
<description>&lt;b&gt;HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Hardware">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
This library contains board components that are not electrical in nature, such as stand-offs, magnets, and Actobotics. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="STAND-OFF">
<description>&lt;h3&gt;Standoff (#4 Screw)&lt;/h3&gt;
&lt;p&gt;This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components.&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;STAND-OFF&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Capacitors" package="0805" value="1.0uF">
<attribute name="PROD_ID" value="CAP-08064"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0805" value="1.0uF">
<attribute name="PROD_ID" value="CAP-08064"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="0805" value="1.0uF">
<attribute name="PROD_ID" value="CAP-08064"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0805" value="1.0uF">
<attribute name="PROD_ID" value="CAP-08064"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="0805" value="1.0uF">
<attribute name="PROD_ID" value="CAP-08064"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="0805" value="1.0uF">
<attribute name="PROD_ID" value="CAP-08064"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X12" value=""/>
<element name="P1" library="con-jst-ph" package="B5B-PH-K" value="B5B-PH-K">
<attribute name="LABEL" value=""/>
</element>
<element name="P2" library="con-jst-ph" package="B5B-PH-K" value="B5B-PH-K">
<attribute name="LABEL" value=""/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X03" value=""/>
<element name="H1" library="SparkFun-Hardware" package="STAND-OFF" value="STAND-OFF"/>
</elements>
<signals>
<signal name="A1">
<contactref element="J1" pad="10"/>
<contactref element="C6" pad="1"/>
<contactref element="P1" pad="2"/>
</signal>
<signal name="B1">
<contactref element="J1" pad="9"/>
<contactref element="C5" pad="1"/>
<contactref element="P1" pad="3"/>
</signal>
<signal name="Z1">
<contactref element="J1" pad="8"/>
<contactref element="C4" pad="1"/>
<contactref element="P1" pad="4"/>
</signal>
<signal name="A0">
<contactref element="J1" pad="4"/>
<contactref element="C3" pad="1"/>
<contactref element="P2" pad="2"/>
</signal>
<signal name="B0">
<contactref element="J1" pad="3"/>
<contactref element="C2" pad="1"/>
<contactref element="P2" pad="3"/>
</signal>
<signal name="Z0">
<contactref element="J1" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="P2" pad="4"/>
</signal>
<signal name="GND">
<contactref element="J1" pad="1"/>
<contactref element="J1" pad="7"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="J2" pad="1"/>
<contactref element="P2" pad="5"/>
<contactref element="P1" pad="5"/>
</signal>
<signal name="VCC">
<contactref element="J1" pad="5"/>
<contactref element="J1" pad="11"/>
<contactref element="J2" pad="2"/>
<contactref element="P1" pad="1"/>
<contactref element="P2" pad="1"/>
</signal>
<signal name="3V3">
<contactref element="J1" pad="12"/>
<contactref element="J2" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
