<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.0.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="15.24" y2="0" width="0" layer="20"/>
<wire x1="15.24" y1="0" x2="15.24" y2="20.32" width="0" layer="20"/>
<wire x1="15.24" y1="20.32" x2="0" y2="20.32" width="0" layer="20"/>
<wire x1="0" y1="20.32" x2="0" y2="0" width="0" layer="20"/>
<text>VMOT</text>
<text>GNDM</text>
<text>ENA</text>
<text>STP</text>
<text>DIR</text>
<text>+5V</text>
<text>GND</text>
<text>DIR</text>
<text>STP</text>
<text>SL</text>
<text>RES</text>
<text>MS3</text>
<text>MS2</text>
<text>MS1</text>
<text>ENA</text>
<text>GND</text>
<text>VDD</text>
<text>1B</text>
<text>1A</text>
<text>2A</text>
<text>2B</text>
<text>GM</text>
<text>VM</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="MOLEX-1X2">
<description>&lt;h3&gt;Molex 2-Pin Plated Through-Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/2pin_molex_set_19iv10.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="MOLEX-1X3">
<description>&lt;h3&gt;PTH - 3 Pin Vertical Molex Polarized Header&lt;/h3&gt;
&lt;p&gt;&lt;b&gt;Datasheet referenced for footprint:&lt;/b&gt;&lt;a href="http://www.4uconnector.com/online/object/4udrawing/01932.pdf"&gt; 4UCONN part # 01932 &lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:3&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X08">
<description>&lt;h3&gt;Plated Through Hole -8 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:8&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_08&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="GNDM_VMOT" library="SparkFun-Connectors" package="MOLEX-1X2" value="">
<attribute name="SF_ID" value="PRT-09918"/>
<attribute name="VALUE"/>
</element>
<element name="GND_+5V" library="SparkFun-Connectors" package="MOLEX-1X2" value="">
<attribute name="SF_ID" value="PRT-09918"/>
<attribute name="VALUE"/>
</element>
<element name="DIR_STP_ENA" library="SparkFun-Connectors" package="MOLEX-1X3" value="">
<attribute name="PROD_ID" value="CONN-08625"/>
<attribute name="SF_ID" value="PRT-08096"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="1X08" value="">
<attribute name="PROD_ID" value="CONN-08438"/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="SparkFun-Connectors" package="1X08" value="">
<attribute name="PROD_ID" value="CONN-08438"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="ENABLE">
<contactref element="J4" pad="8"/>
<contactref element="DIR_STP_ENA" pad="1"/>
</signal>
<signal name="STEP">
<contactref element="DIR_STP_ENA" pad="2"/>
<contactref element="J4" pad="2"/>
</signal>
<signal name="DIR">
<contactref element="J4" pad="1"/>
<contactref element="DIR_STP_ENA" pad="3"/>
</signal>
<signal name="VMOT">
<contactref element="GNDM_VMOT" pad="1"/>
<contactref element="J5" pad="8"/>
</signal>
<signal name="GNDMOT">
<contactref element="GNDM_VMOT" pad="2"/>
<contactref element="J5" pad="7"/>
</signal>
<signal name="VDD">
<contactref element="GND_+5V" pad="1"/>
<contactref element="J5" pad="2"/>
</signal>
<signal name="GND">
<contactref element="GND_+5V" pad="2"/>
<contactref element="J5" pad="1"/>
</signal>
<signal name="2B">
<contactref element="J5" pad="6"/>
</signal>
<signal name="2A">
<contactref element="J5" pad="5"/>
</signal>
<signal name="MS1">
<contactref element="J4" pad="7"/>
</signal>
<signal name="MS2">
<contactref element="J4" pad="6"/>
</signal>
<signal name="MS3">
<contactref element="J4" pad="5"/>
</signal>
<signal name="RESET">
<contactref element="J4" pad="4"/>
</signal>
<signal name="SLEEP">
<contactref element="J4" pad="3"/>
</signal>
<signal name="1A">
<contactref element="J5" pad="4"/>
</signal>
<signal name="1B">
<contactref element="J5" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
