<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="19.558" y1="0" x2="19.558" y2="41.402" width="0" layer="20"/>
<wire x1="19.558" y1="41.402" x2="0" y2="41.402" width="0" layer="20"/>
<wire x1="0" y1="0" x2="0" y2="41.402" width="0" layer="20"/>
<wire x1="19.558" y1="0" x2="0" y2="0" width="0" layer="20"/>
<text>CuriousTech.net</text>
<text>CuriousTech.net</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X08">
<description>&lt;h3&gt;Plated Through Hole -8 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:8&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_08&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X07">
<description>&lt;h3&gt;Plated Through Hole -7 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:7&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_07&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="relay">
<description>&lt;b&gt;Relays&lt;/b&gt;&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;Eichhoff
&lt;li&gt;Finder
&lt;li&gt;Fujitsu
&lt;li&gt;HAMLIN
&lt;li&gt;OMRON
&lt;li&gt;Matsushita
&lt;li&gt;NAiS
&lt;li&gt;Siemens
&lt;li&gt;Schrack
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOP04">
<description>&lt;b&gt;SOP 04 - 4.3x4.4mm RM 2.54mm&lt;/b&gt; AQY21, AQY22, AQY61 Series NAiS&lt;p&gt;Source: http://www.mew-europe.com/..  pti_en.pdf</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="5V" library="SparkFun-Connectors" package="1X08" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08438"/>
<attribute name="VALUE"/>
</element>
<element name="IO5" library="SparkFun-Connectors" package="1X08" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08438"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X07" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="+" library="SparkFun-Connectors" package="1X07" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="K1" library="relay" package="SOP04" value="AQY21SOP">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="POPULARITY" value="0"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="pinhead" package="1X02" value="">
<attribute name="POPULARITY" value="98"/>
<attribute name="VALUE"/>
</element>
<element name="BTN" library="pinhead" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="98"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="5V" pad="2"/>
<contactref element="K1" pad="2"/>
<contactref element="+" pad="2"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="CS">
<contactref element="J1" pad="3"/>
<contactref element="+" pad="3"/>
<contactref element="IO5" pad="3"/>
</signal>
<signal name="WR">
<contactref element="J1" pad="4"/>
<contactref element="+" pad="4"/>
<contactref element="5V" pad="4"/>
</signal>
<signal name="DI">
<contactref element="J1" pad="5"/>
<contactref element="+" pad="5"/>
<contactref element="IO5" pad="2"/>
</signal>
<signal name="BLK">
<contactref element="J1" pad="6"/>
<contactref element="+" pad="6"/>
</signal>
<signal name="+5V">
<contactref element="5V" pad="1"/>
</signal>
<signal name="KEY">
<contactref element="+" pad="7"/>
<contactref element="J1" pad="7"/>
</signal>
<signal name="N$3">
<contactref element="BTN" pad="1"/>
<contactref element="JP1" pad="1"/>
<contactref element="K1" pad="4"/>
</signal>
<signal name="N$4">
<contactref element="K1" pad="3"/>
<contactref element="JP1" pad="2"/>
<contactref element="BTN" pad="2"/>
</signal>
<signal name="BTN">
<contactref element="R7" pad="1"/>
<contactref element="5V" pad="5"/>
</signal>
<signal name="N$5">
<contactref element="K1" pad="1"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="UPS_5V">
<contactref element="+" pad="1"/>
<contactref element="J1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
