<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="0" y2="50.8" width="0.1524" layer="20"/>
<wire x1="0" y1="50.8" x2="76.2" y2="50.8" width="0.1524" layer="20"/>
<wire x1="76.2" y1="50.8" x2="76.2" y2="0" width="0.1524" layer="20"/>
<wire x1="76.2" y1="0" x2="0" y2="0" width="0.1524" layer="20"/>
<text>PB0/MOSI</text>
<text>GROUND</text>
<text>PB1/SCK</text>
<text>PB3/RESET</text>
<text>VCC</text>
<text>PB2</text>
<text>GND</text>
<text>VCC</text>
<text>GND</text>
<text>GND</text>
<text>VCC</text>
<text>VCC</text>
<text>PB3/RESET</text>
<text>RST</text>
<text>PB2</text>
<text>PB2</text>
<text>PB0</text>
<text>PB0/OC0A</text>
<text>PB1/OC0B</text>
<text>PB1</text>
<text>VCC</text>
<text>VCC</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>3 in</text>
<text>2 in</text>
<text>0.25"</text>
<text>0.25"</text>
<text>0.25"</text>
<text>0.25"</text>
<text>ATtiny10 Programming Breakout</text>
<text>Rev. 1</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X01">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:1&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_01&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X3-SHROUDED">
<description>&lt;h3&gt;Plated Through Hole - 2x3 Shrouded Header&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”https://www.sparkfun.com/datasheets/Prototyping/Shrouded-10pin.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X3">
<description>&lt;h3&gt;Plated Through Hole - 2x3&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Hardware">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
This library contains board components that are not electrical in nature, such as stand-offs, magnets, and Actobotics. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="STAND-OFF">
<description>&lt;h3&gt;Standoff (#4 Screw)&lt;/h3&gt;
&lt;p&gt;This is the mechanical footprint for a #4 phillips button head screw. Use the keepout ring to avoid running the screw head into surrounding components.&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;STAND-OFF&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="special-drill">
<description>&lt;b&gt;Special drills&lt;/b&gt;&lt;p&gt;
For drills bigger as 0.51602 Inch you must draw a circle in Layer 20 Dimension.&lt;br&gt;
See also HELP HOLE,</description>
<packages>
<package name="DRILL_0.2500">
<description>&lt;b&gt;1/4" Marker&lt;/b&gt; 250 thousands of an inch</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J1" library="SparkFun-Connectors" package="1X01" value="PB0/MOSI">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X01" value="GROUND">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X01" value="PB1/SCK">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J6" library="SparkFun-Connectors" package="1X01" value="PB3/RESET">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="SparkFun-Connectors" package="1X01" value="VCC">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="1X01" value="PB2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J7" library="SparkFun-Connectors" package="2X3-SHROUDED" value="ICSP">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-10681"/>
<attribute name="SF_ID" value="PRT_10877"/>
<attribute name="VALUE"/>
</element>
<element name="J8" library="SparkFun-Connectors" package="2X3" value="FEMALE 2x3">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-11566"/>
<attribute name="VALUE"/>
</element>
<element name="J9" library="SparkFun-Connectors" package="2X3" value="FEMALE 2x3">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-11566"/>
<attribute name="VALUE"/>
</element>
<element name="J10" library="SparkFun-Connectors" package="2X3" value="FEMALE 2x3">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-11566"/>
<attribute name="VALUE"/>
</element>
<element name="J11" library="SparkFun-Connectors" package="2X3" value="FEMALE 2x3">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-11566"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="SparkFun-Hardware" package="STAND-OFF" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="SparkFun-Hardware" package="STAND-OFF" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$3" library="SparkFun-Hardware" package="STAND-OFF" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$4" library="SparkFun-Hardware" package="STAND-OFF" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$5" library="special-drill" package="DRILL_0.2500" value=""/>
<element name="U$6" library="special-drill" package="DRILL_0.2500" value=""/>
<element name="U$7" library="special-drill" package="DRILL_0.2500" value=""/>
<element name="U$8" library="special-drill" package="DRILL_0.2500" value=""/>
<element name="J12" library="SparkFun-Connectors" package="2X3" value="FEMALE 2x3">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-11566"/>
<attribute name="VALUE"/>
</element>
<element name="J13" library="SparkFun-Connectors" package="2X3" value="FEMALE 2x3">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-11566"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="VCC">
<contactref element="J10" pad="4"/>
<contactref element="J11" pad="4"/>
<contactref element="J10" pad="3"/>
<contactref element="J11" pad="3"/>
<contactref element="J9" pad="3"/>
<contactref element="J9" pad="4"/>
<contactref element="J7" pad="4"/>
<contactref element="J5" pad="1"/>
</signal>
<signal name="GROUND">
<contactref element="J8" pad="3"/>
<contactref element="J8" pad="4"/>
<contactref element="J7" pad="3"/>
<contactref element="J2" pad="1"/>
<contactref element="J10" pad="2"/>
<contactref element="J10" pad="1"/>
<contactref element="J11" pad="2"/>
<contactref element="J11" pad="1"/>
<contactref element="J12" pad="5"/>
<contactref element="J12" pad="6"/>
<contactref element="J13" pad="5"/>
<contactref element="J13" pad="6"/>
</signal>
<signal name="PB0/MOSI">
<contactref element="J10" pad="6"/>
<contactref element="J8" pad="1"/>
<contactref element="J8" pad="2"/>
<contactref element="J7" pad="1"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="PB1/SCK">
<contactref element="J10" pad="5"/>
<contactref element="J8" pad="6"/>
<contactref element="J8" pad="5"/>
<contactref element="J7" pad="5"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="PB3/RESET">
<contactref element="J11" pad="6"/>
<contactref element="J9" pad="1"/>
<contactref element="J9" pad="2"/>
<contactref element="J7" pad="2"/>
<contactref element="J6" pad="1"/>
</signal>
<signal name="PB2">
<contactref element="J11" pad="5"/>
<contactref element="J9" pad="5"/>
<contactref element="J9" pad="6"/>
<contactref element="J7" pad="6"/>
<contactref element="J4" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="J12" pad="2"/>
<contactref element="J12" pad="4"/>
</signal>
<signal name="N$2">
<contactref element="J13" pad="2"/>
<contactref element="J13" pad="4"/>
</signal>
<signal name="N$3">
<contactref element="J12" pad="1"/>
<contactref element="J12" pad="3"/>
</signal>
<signal name="N$4">
<contactref element="J13" pad="1"/>
<contactref element="J13" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
