<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.0.1">
<drawing>
<board>
<plain>
<wire x1="2.54" y1="0" x2="104.14" y2="0" width="0" layer="20"/>
<wire x1="106.68" y1="2.54" x2="106.68" y2="31.75" width="0" layer="20"/>
<wire x1="104.14" y1="34.29" x2="2.54" y2="34.29" width="0" layer="20"/>
<wire x1="0" y1="31.75" x2="0" y2="2.54" width="0" layer="20"/>
<wire x1="2.54" y1="0" x2="0" y2="2.54" width="0" layer="20" curve="-90"/>
<wire x1="104.14" y1="0" x2="106.68" y2="2.54" width="0" layer="20" curve="90"/>
<wire x1="106.68" y1="31.75" x2="104.14" y2="34.29" width="0" layer="20" curve="90"/>
<wire x1="0" y1="31.75" x2="2.54" y2="34.29" width="0" layer="20" curve="-90"/>
<text>12V Monitor</text>
<text>5V Monitor</text>
<text>5V Out</text>
<text>P1</text>
<text>P2</text>
<text>Coin 1</text>
<text>Coin 2</text>
<text>Test</text>
<text>Service</text>
<text>8/5/17
v1.0</text>
</plain>
<libraries>
<library name="#mine">
<packages>
<package name="AMP_60">
<description>Footprint for a 60 Pin TE AMP Connector.</description>
</package>
<package name="DB_15_PLUG">
<description>Footprint for a Amphenol Commercial Products's L717SDA15PA4CH4F a through hole mount DB 15 connector.</description>
</package>
<package name="SWITCH_4">
<description>Footprint for a 4 leg tactile switch, specifically the 1825910-6 from TE Connectivity.</description>
</package>
<package name="JST_XH_2">
<description>A package for a 2 pin JST XH connector.</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.3">
<description>&lt;h3&gt;AXIAL-0.3&lt;/h3&gt;
&lt;p&gt;Commonly used for 1/4W through-hole resistors. 0.3" pitch between holes.&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="J$1" library="#mine" package="AMP_60" value="TE_AMP_60">
<attribute name="VALUE"/>
</element>
<element name="J$2" library="#mine" package="DB_15_PLUG" value="L717SDA15PA4CH4F">
<attribute name="VALUE"/>
</element>
<element name="J$3" library="#mine" package="DB_15_PLUG" value="L717SDA15PA4CH4F">
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="AXIAL-0.3" value="100">
<attribute name="PROD_ID" value="RES-12181"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="#mine" package="SWITCH_4" value="1825910-6">
<attribute name="VALUE"/>
</element>
<element name="U$2" library="#mine" package="SWITCH_4" value="1825910-6">
<attribute name="VALUE"/>
</element>
<element name="U$3" library="#mine" package="SWITCH_4" value="1825910-6">
<attribute name="VALUE"/>
</element>
<element name="U$4" library="#mine" package="SWITCH_4" value="1825910-6">
<attribute name="VALUE"/>
</element>
<element name="U$5" library="#mine" package="JST_XH_2" value="JST_XH">
<attribute name="VALUE"/>
</element>
<element name="U$6" library="#mine" package="JST_XH_2" value="JST_XH">
<attribute name="VALUE"/>
</element>
<element name="U$7" library="#mine" package="JST_XH_2" value="JST_XH">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="J$1" pad="9"/>
<contactref element="U$6" pad="P$2"/>
<contactref element="U$5" pad="P$2"/>
<contactref element="U$2" pad="P$3"/>
<contactref element="U$2" pad="P$4"/>
<contactref element="U$1" pad="P$3"/>
<contactref element="U$1" pad="P$4"/>
<contactref element="U$3" pad="P$3"/>
<contactref element="U$3" pad="P$4"/>
<contactref element="U$4" pad="P$3"/>
<contactref element="U$4" pad="P$4"/>
<contactref element="U$7" pad="P$2"/>
<contactref element="J$2" pad="P$1"/>
<contactref element="J$3" pad="P$1"/>
<contactref element="J$1" pad="10"/>
<contactref element="J$1" pad="11"/>
<contactref element="J$1" pad="12"/>
<contactref element="J$1" pad="13"/>
<contactref element="J$1" pad="14"/>
<contactref element="J$1" pad="15"/>
</signal>
<signal name="12V">
<contactref element="U$7" pad="P$1"/>
<contactref element="J$1" pad="59"/>
<contactref element="J$1" pad="60"/>
<contactref element="J$1" pad="58"/>
<contactref element="J$1" pad="57"/>
</signal>
<signal name="N$6">
<contactref element="U$2" pad="P$1"/>
<contactref element="U$2" pad="P$2"/>
<contactref element="J$1" pad="41"/>
</signal>
<signal name="N$7">
<contactref element="U$1" pad="P$1"/>
<contactref element="U$1" pad="P$2"/>
<contactref element="J$1" pad="43"/>
</signal>
<signal name="N$8">
<contactref element="U$3" pad="P$1"/>
<contactref element="U$3" pad="P$2"/>
<contactref element="J$1" pad="45"/>
<contactref element="J$2" pad="P$3"/>
</signal>
<signal name="N$9">
<contactref element="U$4" pad="P$1"/>
<contactref element="U$4" pad="P$2"/>
<contactref element="J$1" pad="46"/>
<contactref element="J$3" pad="P$3"/>
</signal>
<signal name="N$10">
<contactref element="R1" pad="P$1"/>
<contactref element="J$1" pad="49"/>
<contactref element="J$1" pad="50"/>
</signal>
<signal name="N$12">
<contactref element="J$1" pad="17"/>
<contactref element="J$2" pad="P$11"/>
</signal>
<signal name="N$13">
<contactref element="J$1" pad="18"/>
<contactref element="J$3" pad="P$11"/>
</signal>
<signal name="N$14">
<contactref element="J$1" pad="19"/>
<contactref element="J$2" pad="P$6"/>
</signal>
<signal name="N$15">
<contactref element="J$1" pad="20"/>
<contactref element="J$3" pad="P$6"/>
</signal>
<signal name="N$16">
<contactref element="J$1" pad="21"/>
<contactref element="J$2" pad="P$14"/>
</signal>
<signal name="N$17">
<contactref element="J$1" pad="22"/>
<contactref element="J$3" pad="P$14"/>
</signal>
<signal name="N$18">
<contactref element="J$1" pad="23"/>
<contactref element="J$2" pad="P$15"/>
</signal>
<signal name="N$19">
<contactref element="J$1" pad="24"/>
<contactref element="J$3" pad="P$15"/>
</signal>
<signal name="N$20">
<contactref element="J$1" pad="25"/>
<contactref element="J$2" pad="P$7"/>
</signal>
<signal name="N$21">
<contactref element="J$1" pad="26"/>
<contactref element="J$3" pad="P$7"/>
</signal>
<signal name="N$22">
<contactref element="J$1" pad="27"/>
<contactref element="J$2" pad="P$13"/>
</signal>
<signal name="N$23">
<contactref element="J$1" pad="28"/>
<contactref element="J$3" pad="P$13"/>
</signal>
<signal name="N$24">
<contactref element="J$1" pad="29"/>
<contactref element="J$2" pad="P$5"/>
</signal>
<signal name="N$25">
<contactref element="J$1" pad="30"/>
<contactref element="J$3" pad="P$5"/>
</signal>
<signal name="N$26">
<contactref element="J$1" pad="31"/>
<contactref element="J$2" pad="P$12"/>
</signal>
<signal name="N$27">
<contactref element="J$1" pad="32"/>
<contactref element="J$3" pad="P$12"/>
</signal>
<signal name="N$28">
<contactref element="J$1" pad="33"/>
<contactref element="J$2" pad="P$4"/>
</signal>
<signal name="N$29">
<contactref element="J$1" pad="34"/>
<contactref element="J$3" pad="P$4"/>
</signal>
<signal name="N$30">
<contactref element="J$1" pad="35"/>
<contactref element="J$2" pad="P$10"/>
</signal>
<signal name="N$31">
<contactref element="J$1" pad="36"/>
<contactref element="J$3" pad="P$10"/>
</signal>
<signal name="N$32">
<contactref element="J$1" pad="37"/>
<contactref element="J$2" pad="P$2"/>
</signal>
<signal name="N$33">
<contactref element="J$1" pad="38"/>
<contactref element="J$3" pad="P$2"/>
</signal>
<signal name="5V">
<contactref element="J$1" pad="1"/>
<contactref element="J$1" pad="2"/>
<contactref element="J$1" pad="5"/>
<contactref element="U$5" pad="P$1"/>
<contactref element="U$6" pad="P$1"/>
<contactref element="R1" pad="P$2"/>
<contactref element="J$2" pad="P$8"/>
<contactref element="J$3" pad="P$8"/>
<contactref element="J$1" pad="4"/>
<contactref element="J$1" pad="3"/>
<contactref element="J$1" pad="6"/>
<contactref element="J$1" pad="7"/>
<contactref element="J$1" pad="8"/>
</signal>
<signal name="N$1">
</signal>
<signal name="N$2">
</signal>
<signal name="N$3">
</signal>
<signal name="N$4">
</signal>
</signals>
</board>
</drawing>
</eagle>
