<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="101.27" y2="0" width="0" layer="20"/>
<wire x1="101.27" y1="0" x2="101.27" y2="15.23" width="0" layer="20"/>
<wire x1="101.27" y1="15.23" x2="0" y2="15.23" width="0" layer="20"/>
<wire x1="0" y1="15.23" x2="0" y2="0" width="0" layer="20"/>
<text>Barium</text>
</plain>
<libraries>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-TRICOLOR-5050">
<description>&lt;H3&gt;5050 SMD RGB LED&lt;/h3&gt;
5.0mm x 5.0mm, 2.6mm thickness</description>
</package>
<package name="0805">
</package>
<package name="1X03">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="LED1" library="SparkFun" package="LED-TRICOLOR-5050" value=""/>
<element name="R1" library="SparkFun" package="0805" value="150"/>
<element name="C1" library="SparkFun" package="0805" value="1u"/>
<element name="LED2" library="SparkFun" package="LED-TRICOLOR-5050" value=""/>
<element name="R2" library="SparkFun" package="0805" value="150"/>
<element name="C2" library="SparkFun" package="0805" value="1u"/>
<element name="LED3" library="SparkFun" package="LED-TRICOLOR-5050" value=""/>
<element name="R3" library="SparkFun" package="0805" value="150"/>
<element name="C3" library="SparkFun" package="0805" value="1u"/>
<element name="LED4" library="SparkFun" package="LED-TRICOLOR-5050" value=""/>
<element name="R4" library="SparkFun" package="0805" value="150"/>
<element name="C4" library="SparkFun" package="0805" value="1u"/>
<element name="LED5" library="SparkFun" package="LED-TRICOLOR-5050" value=""/>
<element name="R5" library="SparkFun" package="0805" value="150"/>
<element name="C5" library="SparkFun" package="0805" value="1u"/>
<element name="LED6" library="SparkFun" package="LED-TRICOLOR-5050" value=""/>
<element name="R6" library="SparkFun" package="0805" value="150"/>
<element name="C6" library="SparkFun" package="0805" value="1u"/>
<element name="LED7" library="SparkFun" package="LED-TRICOLOR-5050" value=""/>
<element name="R7" library="SparkFun" package="0805" value="150"/>
<element name="C7" library="SparkFun" package="0805" value="1u"/>
<element name="LED8" library="SparkFun" package="LED-TRICOLOR-5050" value=""/>
<element name="R8" library="SparkFun" package="0805" value="150"/>
<element name="C8" library="SparkFun" package="0805" value="1u"/>
<element name="LED9" library="SparkFun" package="LED-TRICOLOR-5050" value=""/>
<element name="R9" library="SparkFun" package="0805" value="150"/>
<element name="C9" library="SparkFun" package="0805" value="1u"/>
<element name="LED10" library="SparkFun" package="LED-TRICOLOR-5050" value=""/>
<element name="R10" library="SparkFun" package="0805" value="150"/>
<element name="C10" library="SparkFun" package="0805" value="1u"/>
<element name="LED11" library="SparkFun" package="LED-TRICOLOR-5050" value=""/>
<element name="R11" library="SparkFun" package="0805" value="150"/>
<element name="C11" library="SparkFun" package="0805" value="1u"/>
<element name="LED12" library="SparkFun" package="LED-TRICOLOR-5050" value=""/>
<element name="R12" library="SparkFun" package="0805" value="150"/>
<element name="C12" library="SparkFun" package="0805" value="1u"/>
<element name="JP1" library="SparkFun" package="1X03" value="0 L 5">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="LED1" pad="5-LR"/>
<contactref element="LED2" pad="3-MR"/>
</signal>
<signal name="GND">
<contactref element="LED1" pad="6-BL"/>
<contactref element="C1" pad="1"/>
<contactref element="LED2" pad="6-BL"/>
<contactref element="C2" pad="1"/>
<contactref element="LED3" pad="6-BL"/>
<contactref element="C3" pad="1"/>
<contactref element="LED4" pad="6-BL"/>
<contactref element="C4" pad="1"/>
<contactref element="LED5" pad="6-BL"/>
<contactref element="C5" pad="1"/>
<contactref element="LED6" pad="6-BL"/>
<contactref element="C6" pad="1"/>
<contactref element="LED7" pad="6-BL"/>
<contactref element="C7" pad="1"/>
<contactref element="LED8" pad="6-BL"/>
<contactref element="C8" pad="1"/>
<contactref element="LED9" pad="6-BL"/>
<contactref element="C9" pad="1"/>
<contactref element="LED10" pad="6-BL"/>
<contactref element="C10" pad="1"/>
<contactref element="LED11" pad="6-BL"/>
<contactref element="C11" pad="1"/>
<contactref element="LED12" pad="6-BL"/>
<contactref element="C12" pad="1"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="VCC">
<contactref element="LED1" pad="4-ML"/>
<contactref element="R1" pad="1"/>
<contactref element="LED2" pad="4-ML"/>
<contactref element="R2" pad="1"/>
<contactref element="LED3" pad="4-ML"/>
<contactref element="R3" pad="1"/>
<contactref element="LED4" pad="4-ML"/>
<contactref element="R4" pad="1"/>
<contactref element="LED5" pad="4-ML"/>
<contactref element="R5" pad="1"/>
<contactref element="LED6" pad="4-ML"/>
<contactref element="R6" pad="1"/>
<contactref element="LED7" pad="4-ML"/>
<contactref element="R7" pad="1"/>
<contactref element="LED8" pad="4-ML"/>
<contactref element="R8" pad="1"/>
<contactref element="LED9" pad="4-ML"/>
<contactref element="R9" pad="1"/>
<contactref element="LED10" pad="4-ML"/>
<contactref element="R10" pad="1"/>
<contactref element="LED11" pad="4-ML"/>
<contactref element="R11" pad="1"/>
<contactref element="LED12" pad="4-ML"/>
<contactref element="R12" pad="1"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="R1" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="LED1" pad="1-TR"/>
</signal>
<signal name="N$4">
<contactref element="R2" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="LED2" pad="1-TR"/>
</signal>
<signal name="N$6">
<contactref element="R3" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="LED3" pad="1-TR"/>
</signal>
<signal name="N$8">
<contactref element="R4" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="LED4" pad="1-TR"/>
</signal>
<signal name="N$10">
<contactref element="R5" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="LED5" pad="1-TR"/>
</signal>
<signal name="N$12">
<contactref element="R6" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="LED6" pad="1-TR"/>
</signal>
<signal name="N$14">
<contactref element="R7" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="LED7" pad="1-TR"/>
</signal>
<signal name="N$16">
<contactref element="R8" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="LED8" pad="1-TR"/>
</signal>
<signal name="N$18">
<contactref element="R9" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="LED9" pad="1-TR"/>
</signal>
<signal name="N$20">
<contactref element="R10" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="LED10" pad="1-TR"/>
</signal>
<signal name="N$22">
<contactref element="R11" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="LED11" pad="1-TR"/>
</signal>
<signal name="N$24">
<contactref element="R12" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="LED12" pad="1-TR"/>
</signal>
<signal name="N$2">
<contactref element="LED2" pad="5-LR"/>
<contactref element="LED3" pad="3-MR"/>
</signal>
<signal name="N$5">
<contactref element="LED3" pad="5-LR"/>
<contactref element="LED4" pad="3-MR"/>
</signal>
<signal name="LED_IN">
<contactref element="LED1" pad="3-MR"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="LED4" pad="5-LR"/>
<contactref element="LED5" pad="3-MR"/>
</signal>
<signal name="N$9">
<contactref element="LED5" pad="5-LR"/>
<contactref element="LED6" pad="3-MR"/>
</signal>
<signal name="N$11">
<contactref element="LED6" pad="5-LR"/>
<contactref element="LED7" pad="3-MR"/>
</signal>
<signal name="N$13">
<contactref element="LED8" pad="3-MR"/>
<contactref element="LED7" pad="5-LR"/>
</signal>
<signal name="N$15">
<contactref element="LED8" pad="5-LR"/>
<contactref element="LED9" pad="3-MR"/>
</signal>
<signal name="N$17">
<contactref element="LED9" pad="5-LR"/>
<contactref element="LED10" pad="3-MR"/>
</signal>
<signal name="N$21">
<contactref element="LED12" pad="3-MR"/>
<contactref element="LED11" pad="5-LR"/>
</signal>
<signal name="N$19">
<contactref element="LED11" pad="3-MR"/>
<contactref element="LED10" pad="5-LR"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
