<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.4.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="54.28" y2="0" width="0" layer="20"/>
<wire x1="54.28" y1="0" x2="54.28" y2="59.68" width="0" layer="20"/>
<wire x1="54.28" y1="59.68" x2="0" y2="59.68" width="0" layer="20"/>
<wire x1="0" y1="59.68" x2="0" y2="0" width="0" layer="20"/>
<text>VISCA Shield
for Cisco TelePresence
PrecisionHD</text>
<text>Rev 1.0</text>
</plain>
<libraries>
<library name="con-molex">
<description>&lt;b&gt;Molex Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="22-23-2021">
<description>&lt;b&gt;KK® 254 Solid Header, Vertical, with Friction Lock, 2 Circuits, Tin (Sn) Plating&lt;/b&gt;&lt;p&gt;&lt;a href =http://www.molex.com/pdm_docs/sd/022232021_sd.pdf&gt;Datasheet &lt;/a&gt;</description>
</package>
<package name="22-23-2031">
<description>&lt;b&gt;KK® 254 Solid Header, Vertical, with Friction Lock, 3 Circuits, Tin (Sn) Plating&lt;/b&gt;&lt;p&gt;&lt;a href =http://www.molex.com/pdm_docs/sd/022232031_sd.pdf&gt;Datasheet &lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Boards">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
This library contains footprints for SparkFun breakout boards, microcontrollers (Arduino, Particle, Teensy, etc.),  breadboards, non-RF modules, etc.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="UNO_R3_SHIELD">
<description>&lt;h3&gt;Arduino Uno-Compatible Footprint&lt;/h3&gt;
No holes, no ICSP connections.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count: 32&lt;/li&gt;
&lt;li&gt;Pin pitch: 0.1"&lt;/li&gt;
&lt;li&gt;Area:2.1x2.35"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;Arduino Uno R3 Shield&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Aesthetics&lt;/h3&gt;
This library contiains non-functional items such as logos, build/ordering notes, frame blocks, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DUMMY">
<description>&lt;h3&gt;Dummy Footprint&lt;/h3&gt;
&lt;p&gt;NOTHING HERE!!! For when you want a symbol with no package as an option against symbols with a package.&lt;/p&gt;

&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;BADGERHACK_LOGO&lt;/li&gt;
&lt;li&gt;FRAME-LETTER&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="RJHSE-5381">
<packages>
<package name="AMPHENOL_RJHSE-5381">
</package>
</packages>
</library>
<library name="BeagleBone_Black_Wireless">
<description>Generated from &lt;b&gt;BeagleBone_Black_Wireless.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="0204V">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 2.5 mm</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="12V" library="con-molex" package="22-23-2021" value="22-23-2021">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value="22-23-2021"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1462926"/>
<attribute name="OC_NEWARK" value="25C3832"/>
<attribute name="POPULARITY" value="40"/>
<attribute name="VALUE"/>
</element>
<element name="B1" library="SparkFun-Boards" package="UNO_R3_SHIELD" value="ARDUINO_UNO_R3_SHIELDBASIC">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FRAME1" library="SparkFun-Aesthetics" package="DUMMY" value="FRAME-LETTERNO_PACKAGE">
<attribute name="DESIGNER" value="Nobody"/>
<attribute name="VERSION" value="v01"/>
</element>
<element name="J1" library="RJHSE-5381" package="AMPHENOL_RJHSE-5381" value="RJHSE-5381">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" connector, mod jack, rt angle pcb, shielded, led1-g, led2-y, single port, rj-45 8 cont "/>
<attribute name="MF" value="Amphenol ICC"/>
<attribute name="MP" value="RJHSE-5381"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
<attribute name="VALUE"/>
</element>
<element name="PAN" library="con-molex" package="22-23-2031" value="22-23-2031">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value="22-23-2031"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1462950"/>
<attribute name="OC_NEWARK" value="30C0862"/>
<attribute name="POPULARITY" value="35"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="BeagleBone_Black_Wireless" package="0204V" value="10kohm">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="BeagleBone_Black_Wireless" package="0204V" value="10kohm">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="BeagleBone_Black_Wireless" package="0204V" value="10kohm">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="BeagleBone_Black_Wireless" package="0204V" value="10kohm">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="BeagleBone_Black_Wireless" package="0204V" value="10kohm">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="BeagleBone_Black_Wireless" package="0204V" value="10kohm">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="BeagleBone_Black_Wireless" package="0204V" value="10kohm">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="BeagleBone_Black_Wireless" package="0204V" value="10kohm">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="BeagleBone_Black_Wireless" package="0204V" value="10kohm">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="BeagleBone_Black_Wireless" package="0204V" value="10kohm">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TILT" library="con-molex" package="22-23-2031" value="22-23-2031">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value="22-23-2031"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1462950"/>
<attribute name="OC_NEWARK" value="30C0862"/>
<attribute name="POPULARITY" value="35"/>
<attribute name="VALUE"/>
</element>
<element name="X10" library="con-molex" package="22-23-2021" value="22-23-2021">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value="22-23-2021"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1462926"/>
<attribute name="OC_NEWARK" value="25C3832"/>
<attribute name="POPULARITY" value="40"/>
<attribute name="VALUE"/>
</element>
<element name="X11" library="con-molex" package="22-23-2021" value="22-23-2021">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value="22-23-2021"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1462926"/>
<attribute name="OC_NEWARK" value="25C3832"/>
<attribute name="POPULARITY" value="40"/>
<attribute name="VALUE"/>
</element>
<element name="X12" library="con-molex" package="22-23-2021" value="22-23-2021">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value="22-23-2021"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1462926"/>
<attribute name="OC_NEWARK" value="25C3832"/>
<attribute name="POPULARITY" value="40"/>
<attribute name="VALUE"/>
</element>
<element name="X13" library="con-molex" package="22-23-2021" value="22-23-2021">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value="22-23-2021"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1462926"/>
<attribute name="OC_NEWARK" value="25C3832"/>
<attribute name="POPULARITY" value="40"/>
<attribute name="VALUE"/>
</element>
<element name="X4" library="con-molex" package="22-23-2021" value="22-23-2021">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value="22-23-2021"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1462926"/>
<attribute name="OC_NEWARK" value="25C3832"/>
<attribute name="POPULARITY" value="40"/>
<attribute name="VALUE"/>
</element>
<element name="X5" library="con-molex" package="22-23-2021" value="22-23-2021">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value="22-23-2021"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1462926"/>
<attribute name="OC_NEWARK" value="25C3832"/>
<attribute name="POPULARITY" value="40"/>
<attribute name="VALUE"/>
</element>
<element name="X6" library="con-molex" package="22-23-2021" value="22-23-2021">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value="22-23-2021"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1462926"/>
<attribute name="OC_NEWARK" value="25C3832"/>
<attribute name="POPULARITY" value="40"/>
<attribute name="VALUE"/>
</element>
<element name="X7" library="con-molex" package="22-23-2021" value="22-23-2021">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value="22-23-2021"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1462926"/>
<attribute name="OC_NEWARK" value="25C3832"/>
<attribute name="POPULARITY" value="40"/>
<attribute name="VALUE"/>
</element>
<element name="X8" library="con-molex" package="22-23-2021" value="22-23-2021">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value="22-23-2021"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1462926"/>
<attribute name="OC_NEWARK" value="25C3832"/>
<attribute name="POPULARITY" value="40"/>
<attribute name="VALUE"/>
</element>
<element name="X9" library="con-molex" package="22-23-2021" value="22-23-2021">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value="22-23-2021"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1462926"/>
<attribute name="OC_NEWARK" value="25C3832"/>
<attribute name="POPULARITY" value="40"/>
<attribute name="VALUE"/>
</element>
<element name="ZOOM" library="con-molex" package="22-23-2031" value="22-23-2031">
<attribute name="MF" value="MOLEX"/>
<attribute name="MPN" value="22-23-2031"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1462950"/>
<attribute name="OC_NEWARK" value="30C0862"/>
<attribute name="POPULARITY" value="35"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="B1" pad="GND@2"/>
<contactref element="B1" pad="GND@1"/>
<contactref element="B1" pad="GND@0"/>
<contactref element="J1" pad="7"/>
<contactref element="J1" pad="2"/>
<contactref element="12V" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="R8" pad="1"/>
<contactref element="R9" pad="1"/>
<contactref element="R10" pad="1"/>
<contactref element="PAN" pad="1"/>
<contactref element="TILT" pad="1"/>
<contactref element="ZOOM" pad="1"/>
</signal>
<signal name="5V">
<contactref element="B1" pad="5V"/>
<contactref element="X4" pad="2"/>
<contactref element="X11" pad="2"/>
<contactref element="X12" pad="2"/>
<contactref element="X13" pad="2"/>
<contactref element="X5" pad="2"/>
<contactref element="X6" pad="2"/>
<contactref element="X7" pad="2"/>
<contactref element="X8" pad="2"/>
<contactref element="X9" pad="2"/>
<contactref element="X10" pad="2"/>
<contactref element="PAN" pad="3"/>
<contactref element="TILT" pad="3"/>
<contactref element="ZOOM" pad="3"/>
</signal>
<signal name="PAN">
<contactref element="B1" pad="A0"/>
<contactref element="PAN" pad="2"/>
</signal>
<signal name="TILT">
<contactref element="B1" pad="A1"/>
<contactref element="TILT" pad="2"/>
</signal>
<signal name="ZOOM">
<contactref element="B1" pad="A2"/>
<contactref element="ZOOM" pad="2"/>
</signal>
<signal name="12V">
<contactref element="J1" pad="1"/>
<contactref element="J1" pad="8"/>
<contactref element="12V" pad="2"/>
</signal>
<signal name="TX">
<contactref element="J1" pad="3"/>
<contactref element="B1" pad="D3"/>
</signal>
<signal name="RX">
<contactref element="J1" pad="6"/>
<contactref element="B1" pad="D2"/>
</signal>
<signal name="B1">
<contactref element="B1" pad="D4"/>
<contactref element="R1" pad="2"/>
<contactref element="X4" pad="1"/>
</signal>
<signal name="B2">
<contactref element="B1" pad="D5"/>
<contactref element="R2" pad="2"/>
<contactref element="X5" pad="1"/>
</signal>
<signal name="B3">
<contactref element="B1" pad="D6"/>
<contactref element="R3" pad="2"/>
<contactref element="X6" pad="1"/>
</signal>
<signal name="B4">
<contactref element="B1" pad="D7"/>
<contactref element="R4" pad="2"/>
<contactref element="X7" pad="1"/>
</signal>
<signal name="B5">
<contactref element="B1" pad="D8"/>
<contactref element="R5" pad="2"/>
<contactref element="X8" pad="1"/>
</signal>
<signal name="B6">
<contactref element="B1" pad="D9"/>
<contactref element="R6" pad="2"/>
<contactref element="X9" pad="1"/>
</signal>
<signal name="B7">
<contactref element="B1" pad="D10"/>
<contactref element="R7" pad="2"/>
<contactref element="X10" pad="1"/>
</signal>
<signal name="B8">
<contactref element="B1" pad="D11"/>
<contactref element="R8" pad="2"/>
<contactref element="X11" pad="1"/>
</signal>
<signal name="B9">
<contactref element="B1" pad="D12"/>
<contactref element="R9" pad="2"/>
<contactref element="X12" pad="1"/>
</signal>
<signal name="B10">
<contactref element="B1" pad="D13"/>
<contactref element="R10" pad="2"/>
<contactref element="X13" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
