<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="25.4" x2="38.1" y2="63.5" width="0.4064" layer="20" curve="-90"/>
<wire x1="38.1" y1="63.5" x2="76.2" y2="25.4" width="0.4064" layer="20" curve="-90"/>
<wire x1="76.2" y1="25.4" x2="69.85" y2="31.75" width="0.4064" layer="20" curve="-90"/>
<wire x1="69.85" y1="31.75" x2="63.5" y2="25.4" width="0.4064" layer="20" curve="-90"/>
<wire x1="63.5" y1="25.4" x2="57.15" y2="31.75" width="0.4064" layer="20" curve="-90"/>
<wire x1="57.15" y1="31.75" x2="50.8" y2="25.4" width="0.4064" layer="20" curve="-90"/>
<wire x1="50.8" y1="25.4" x2="44.45" y2="31.75" width="0.4064" layer="20" curve="-90"/>
<wire x1="31.75" y1="31.75" x2="25.4" y2="25.4" width="0.4064" layer="20" curve="-90"/>
<wire x1="25.4" y1="25.4" x2="19.05" y2="31.75" width="0.4064" layer="20" curve="-90"/>
<wire x1="19.05" y1="31.75" x2="12.7" y2="25.4" width="0.4064" layer="20" curve="-90"/>
<wire x1="12.7" y1="25.4" x2="6.35" y2="31.75" width="0.4064" layer="20" curve="-90"/>
<wire x1="6.35" y1="31.75" x2="0" y2="25.4" width="0.4064" layer="20" curve="-90"/>
<wire x1="35.56" y1="25.4" x2="35.56" y2="5.08" width="0.4064" layer="20"/>
<wire x1="35.56" y1="5.08" x2="30.48" y2="5.08" width="0.4064" layer="20" curve="-180"/>
<wire x1="30.48" y1="5.08" x2="25.4" y2="5.08" width="0.4064" layer="20" curve="180"/>
<wire x1="25.4" y1="5.08" x2="40.64" y2="5.08" width="0.4064" layer="20" curve="180"/>
<wire x1="40.64" y1="5.08" x2="40.64" y2="25.4" width="0.4064" layer="20"/>
<wire x1="40.64" y1="25.4" x2="44.45" y2="31.75" width="0.4064" layer="20" curve="-61.92752"/>
<wire x1="35.56" y1="25.4" x2="31.75" y2="31.75" width="0.4064" layer="20" curve="61.92752"/>
<polygon width="0.254" layer="20">
<vertex x="48.514" y="58.674"/>
<vertex x="45.974" y="55.88"/>
<vertex x="42.418" y="60.198"/>
<vertex x="42.672" y="61.214"/>
</polygon>
<polygon width="0.254" layer="20">
<vertex x="30.226" y="55.626"/>
<vertex x="27.432" y="58.42"/>
<vertex x="33.02" y="61.214"/>
<vertex x="33.782" y="60.198"/>
</polygon>
<wire x1="0.254" y1="25.908" x2="37.592" y2="63.246" width="0.8128" layer="20" curve="-90"/>
<wire x1="37.592" y1="63.246" x2="38.354" y2="63.246" width="0.8128" layer="20"/>
<wire x1="38.354" y1="63.246" x2="75.692" y2="25.908" width="0.8128" layer="20" curve="-90"/>
<text>@mpinner</text>
<text>v0.3</text>
<text>uvicorn</text>
<text>touchtech.io</text>
<text>run in the rain</text>
<text>run in the rain</text>
<text>run in the rain</text>
<text>run in the rain</text>
<text>run in the rain</text>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED5MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
5 mm, round</description>
</package>
</packages>
</library>
<library name="SparkFun-AnalogIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of analog ICs- DACs, ADCs, video chips, op-amps, and others.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt;Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; Fits JEDEC packages (narrow SOIC-8)</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
</packages>
</library>
<library name="matt">
<packages>
<package name="CR2032-SMD">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Capacitors" package="1206" value="1UF">
<attribute name="PROD_ID" value="445-8517-ND"/>
</element>
<element name="IC1" library="SparkFun-AnalogIC" package="SO08" value="">
<attribute name="PROD_ID" value="296-1857-5-ND"/>
</element>
<element name="R5" library="SparkFun-Passives" package="1206" value="1K"/>
<element name="R6" library="SparkFun-Passives" package="1206" value="470K"/>
<element name="U$1" library="matt" package="CR2032-SMD" value=""/>
<element name="U$2" library="matt" package="CR2032-SMD" value=""/>
<element name="D1" library="SparkFun-LED" package="LED5MM" value="WHITE-30mA">
<attribute name="PROD_ID" value="67-2062-ND"/>
</element>
<element name="D2" library="SparkFun-LED" package="LED5MM" value="WHITE-30mA">
<attribute name="PROD_ID" value="67-2062-ND"/>
</element>
<element name="D3" library="SparkFun-LED" package="LED5MM" value="WHITE-30mA">
<attribute name="PROD_ID" value="67-2062-ND"/>
</element>
<element name="R1" library="SparkFun-Passives" package="1206" value="100"/>
<element name="R2" library="SparkFun-Passives" package="1206" value="100"/>
<element name="R3" library="SparkFun-Passives" package="1206" value="100"/>
<element name="D4" library="SparkFun-LED" package="LED5MM" value="WHITE-30mA">
<attribute name="PROD_ID" value="67-2062-ND"/>
</element>
<element name="D5" library="SparkFun-LED" package="LED5MM" value="WHITE-30mA">
<attribute name="PROD_ID" value="67-2062-ND"/>
</element>
<element name="R4" library="SparkFun-Passives" package="1206" value="100"/>
<element name="R7" library="SparkFun-Passives" package="1206" value="100"/>
</elements>
<signals>
<signal name="GND">
<contactref element="IC1" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="U$1" pad="-"/>
<contactref element="D2" pad="K"/>
<contactref element="D3" pad="K"/>
<contactref element="D4" pad="K"/>
<contactref element="D5" pad="K"/>
<contactref element="D1" pad="K"/>
</signal>
<signal name="THRESHOLD">
<contactref element="C1" pad="2"/>
<contactref element="IC1" pad="6"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="IC1" pad="8"/>
<contactref element="IC1" pad="4"/>
<contactref element="R5" pad="2"/>
<contactref element="U$2" pad="+$1"/>
<contactref element="R2" pad="2"/>
<contactref element="R3" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="DISCHARGE">
<contactref element="IC1" pad="7"/>
<contactref element="R6" pad="1"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="U$1" pad="+$2"/>
<contactref element="U$2" pad="-"/>
<contactref element="U$1" pad="+$1"/>
</signal>
<signal name="N$3">
<contactref element="IC1" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="IC1" pad="3"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="1"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="N$5">
<contactref element="D2" pad="A"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="D3" pad="A"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="D4" pad="A"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="D5" pad="A"/>
<contactref element="R7" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
