<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.2.2">
<drawing>
<board>
<plain>
<wire x1="40.64" y1="60.96" x2="40.64" y2="41.91" width="0.1524" layer="20"/>
<wire x1="40.64" y1="41.91" x2="57.15" y2="41.91" width="0.1524" layer="20"/>
<wire x1="57.15" y1="41.91" x2="57.15" y2="60.96" width="0.1524" layer="20"/>
<wire x1="57.15" y1="60.96" x2="40.64" y2="60.96" width="0.1524" layer="20"/>
<text>A0</text>
<text>A1</text>
<text>A2</text>
<text>GND</text>
<text>VDD</text>
<text>MLCR</text>
<text>A0</text>
<text>GND</text>
<text>A1</text>
<text>A2</text>
<text>VDD</text>
<text>MLCR</text>
<text>PIC10F322</text>
<text>18DEC18</text>
<text>V1</text>
</plain>
<libraries>
<library name="MICROCHIP">
<packages>
<package name="SOT23-6">
</package>
</packages>
</library>
<library name="TAG-CONNECT">
<packages>
<package name="PLUG-OF-NAILS">
</package>
</packages>
</library>
<library name="OST">
<packages>
<package name="OSTVN06">
</package>
</packages>
</library>
<library name="KEMET">
<packages>
<package name="0603_B">
</package>
</packages>
</library>
<library name="DIALIGHT">
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="Stackpole">
<packages>
<package name="0603">
<description>From Stackpole datasheet: https://www.seielect.com/Catalog/SEI-RMCF_RMCP.pdf</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="MICROCHIP" package="SOT23-6" value="PIC10F322">
<attribute name="NAME"/>
</element>
<element name="U$2" library="TAG-CONNECT" package="PLUG-OF-NAILS" value="PIC_ICPH"/>
<element name="U$3" library="OST" package="OSTVN06" value="M0606"/>
<element name="C1" library="KEMET" package="0603_B" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$4" library="DIALIGHT" package="0805" value="LED0805"/>
<element name="R1" library="Stackpole" package="0603" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="A0">
<contactref element="U$3" pad="1"/>
<contactref element="U$1" pad="1"/>
<contactref element="U$2" pad="4"/>
</signal>
<signal name="A1">
<contactref element="U$3" pad="3"/>
<contactref element="U$1" pad="3"/>
<contactref element="U$2" pad="5"/>
</signal>
<signal name="A2">
<contactref element="U$3" pad="4"/>
<contactref element="U$1" pad="4"/>
<contactref element="U$4" pad="A"/>
</signal>
<signal name="VDD">
<contactref element="U$2" pad="2"/>
<contactref element="U$3" pad="5"/>
<contactref element="U$1" pad="5"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="MLCR">
<contactref element="U$1" pad="6"/>
<contactref element="U$2" pad="1"/>
<contactref element="U$3" pad="6"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="1"/>
<contactref element="U$3" pad="2"/>
<contactref element="U$1" pad="2"/>
<contactref element="U$2" pad="3"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U$4" pad="K"/>
<contactref element="R1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
