<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.5.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="36" y2="0" width="0" layer="20"/>
<wire x1="36" y1="0" x2="36" y2="80" width="0" layer="20"/>
<wire x1="36" y1="80" x2="0" y2="80" width="0" layer="20"/>
<wire x1="0" y1="80" x2="0" y2="0" width="0" layer="20"/>
<text>HvA NameTag</text>
<text>Designed by: Nick Leijenhorst</text>
</plain>
<libraries>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SPARKFUN-DIGITALIC_TQFP44">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="USB-MINIB-OLD">
<description>&lt;b&gt;USB Series Mini-B Surface Mounted&lt;/b&gt;</description>
</package>
<package name="JST-2-SMD">
<description>2mm SMD side-entry connector. tDocu layer indicates the actual physical plastic housing. +/- indicate SparkFun standard batteries and wiring.</description>
</package>
<package name="1X16_LONGPADS">
</package>
<package name="2X3">
</package>
</packages>
</library>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="EIA3216">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE_SWITCH_SMD">
</package>
<package name="KPS-1290">
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-1206">
</package>
</packages>
</library>
<library name="SparkFun-FreqCtrl">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find crystals and oscillators and other things that go "tick".&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CRYSTAL-SMD-5X3">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="ATMEGA32U4" library="SparkFun-DigitalIC" package="SPARKFUN-DIGITALIC_TQFP44" value="ATMEGA32U4TQFP">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="USB-MINIB-OLD" value="USBOLD">
<attribute name="VALUE"/>
</element>
<element name="IC1" library="SparkFun-PowerIC" package="SOT23-5" value="MCP73831">
<attribute name="PROD_ID" value="IC-09995"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0805" value="2K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Passives" package="0805" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Passives" package="0805" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun-Passives" package="0805" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="JST-2-SMD" value="">
<attribute name="PROD_ID" value="CONN-08352"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="EIA3216" value="10uF">
<attribute name="PROD_ID" value="CAP-00811"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="EIA3216" value="10uF">
<attribute name="PROD_ID" value="CAP-00811"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="SparkFun-Passives" package="0805" value="22p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="SparkFun-Passives" package="0805" value="22p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RESET" library="SparkFun-Electromechanical" package="TACTILE_SWITCH_SMD" value="">
<attribute name="PROD_ID" value="SWCH-08247"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="1X16_LONGPADS" value="M16LONGPADS">
<attribute name="VALUE"/>
</element>
<element name="CHARGING" library="SparkFun-LED" package="LED-1206" value="RED">
<attribute name="PROD_ID" value="DIO-00809"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0805" value="330">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="USB_PWR" library="SparkFun-LED" package="LED-1206" value="BLUE">
<attribute name="PROD_ID" value="DIO-09911"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0805" value="330">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="DEBUG" library="SparkFun-LED" package="LED-1206" value="GREEN">
<attribute name="PROD_ID" value="DIO-00862"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="0805" value="330">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SWITCH" library="SparkFun-Electromechanical" package="KPS-1290" value="SWITCH_SPDT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="SparkFun-Passives" package="0805" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="0805" value="22">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="0805" value="22">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MODE" library="SparkFun-Electromechanical" package="TACTILE_SWITCH_SMD" value="">
<attribute name="PROD_ID" value="SWCH-08247"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="8MHZ" library="SparkFun-FreqCtrl" package="CRYSTAL-SMD-5X3" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="AVR_ISP" library="SparkFun-Connectors" package="2X3" value="AVR_SPI_PRG_6PTH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="SparkFun-Resistors" package="0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="SparkFun-Resistors" package="0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="VBUS">
<contactref element="ATMEGA32U4" pad="7"/>
<contactref element="ATMEGA32U4" pad="2"/>
<contactref element="JP1" pad="VBUS"/>
<contactref element="C2" pad="1"/>
<contactref element="IC1" pad="4"/>
<contactref element="C4" pad="A"/>
<contactref element="CHARGING" pad="A"/>
<contactref element="USB_PWR" pad="A"/>
</signal>
<signal name="GND">
<contactref element="JP1" pad="GND"/>
<contactref element="ATMEGA32U4" pad="43"/>
<contactref element="ATMEGA32U4" pad="5"/>
<contactref element="ATMEGA32U4" pad="15"/>
<contactref element="ATMEGA32U4" pad="23"/>
<contactref element="ATMEGA32U4" pad="35"/>
<contactref element="ATMEGA32U4" pad="33"/>
<contactref element="IC1" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="J1" pad="1"/>
<contactref element="C5" pad="C"/>
<contactref element="C4" pad="C"/>
<contactref element="RESET" pad="4"/>
<contactref element="C6" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="JP2" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="MODE" pad="4"/>
<contactref element="AVR_ISP" pad="6"/>
<contactref element="R9" pad="1"/>
</signal>
<signal name="D-">
<contactref element="JP1" pad="D-"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="D+">
<contactref element="JP1" pad="D+"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="V_BATT">
<contactref element="IC1" pad="3"/>
<contactref element="C5" pad="A"/>
<contactref element="J1" pad="2"/>
<contactref element="SWITCH" pad="P"/>
</signal>
<signal name="N$2">
<contactref element="IC1" pad="5"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="ATMEGA32U4" pad="6"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="ATMEGA32U4" pad="17"/>
<contactref element="C6" pad="2"/>
<contactref element="8MHZ" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="ATMEGA32U4" pad="16"/>
<contactref element="C7" pad="2"/>
<contactref element="8MHZ" pad="1"/>
</signal>
<signal name="D6">
<contactref element="JP2" pad="4"/>
<contactref element="ATMEGA32U4" pad="27"/>
</signal>
<signal name="D7">
<contactref element="JP2" pad="5"/>
<contactref element="ATMEGA32U4" pad="1"/>
</signal>
<signal name="D8">
<contactref element="JP2" pad="6"/>
<contactref element="ATMEGA32U4" pad="28"/>
</signal>
<signal name="D9">
<contactref element="JP2" pad="11"/>
<contactref element="ATMEGA32U4" pad="29"/>
</signal>
<signal name="D10">
<contactref element="JP2" pad="12"/>
<contactref element="ATMEGA32U4" pad="30"/>
</signal>
<signal name="D11">
<contactref element="JP2" pad="13"/>
<contactref element="ATMEGA32U4" pad="12"/>
</signal>
<signal name="D12">
<contactref element="JP2" pad="14"/>
<contactref element="ATMEGA32U4" pad="26"/>
</signal>
<signal name="N$6">
<contactref element="R3" pad="2"/>
<contactref element="IC1" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="CHARGING" pad="C"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="USB_PWR" pad="C"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="DEBUG" pad="C"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="ATMEGA32U4" pad="32"/>
<contactref element="DEBUG" pad="A"/>
</signal>
<signal name="N$12">
<contactref element="ATMEGA32U4" pad="42"/>
<contactref element="C8" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="SWITCH" pad="O"/>
<contactref element="JP2" pad="2"/>
<contactref element="ATMEGA32U4" pad="14"/>
<contactref element="ATMEGA32U4" pad="44"/>
<contactref element="ATMEGA32U4" pad="24"/>
<contactref element="ATMEGA32U4" pad="34"/>
<contactref element="C3" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="AVR_ISP" pad="2"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="R7" pad="1"/>
<contactref element="ATMEGA32U4" pad="3"/>
</signal>
<signal name="N$13">
<contactref element="R6" pad="1"/>
<contactref element="ATMEGA32U4" pad="4"/>
</signal>
<signal name="N$14">
<contactref element="ATMEGA32U4" pad="19"/>
<contactref element="MODE" pad="2"/>
</signal>
<signal name="MOSI">
<contactref element="AVR_ISP" pad="4"/>
<contactref element="ATMEGA32U4" pad="10"/>
</signal>
<signal name="RESET">
<contactref element="AVR_ISP" pad="5"/>
<contactref element="ATMEGA32U4" pad="13"/>
<contactref element="R2" pad="2"/>
<contactref element="RESET" pad="2"/>
</signal>
<signal name="SCK">
<contactref element="AVR_ISP" pad="3"/>
<contactref element="ATMEGA32U4" pad="9"/>
</signal>
<signal name="MISO">
<contactref element="AVR_ISP" pad="1"/>
<contactref element="ATMEGA32U4" pad="11"/>
</signal>
<signal name="N$1">
<contactref element="R8" pad="1"/>
<contactref element="R9" pad="2"/>
<contactref element="ATMEGA32U4" pad="36"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
