<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="2.54" y1="2.54" x2="22.86" y2="2.54" width="0" layer="20"/>
<wire x1="22.86" y1="2.54" x2="22.86" y2="22.86" width="0" layer="20"/>
<wire x1="22.86" y1="22.86" x2="2.54" y2="22.86" width="0" layer="20"/>
<wire x1="2.54" y1="22.86" x2="2.54" y2="2.54" width="0" layer="20"/>
<text>PSYCHOHOLICS</text>
<text>SAINTCON 2017</text>
</plain>
<libraries>
<library name="SYNShop">
<packages>
<package name="GULLWING_LED">
</package>
<package name="0402-RES">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO08-EIAJ">
<description>Fits EIAJ packages (wide version of the SOIC-8).</description>
</package>
</packages>
</library>
<library name="darknet_parts_library">
<packages>
<package name="AVRISP-POGO">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="LED1" library="SYNShop" package="GULLWING_LED" value=""/>
<element name="LED2" library="SYNShop" package="GULLWING_LED" value=""/>
<element name="LED3" library="SYNShop" package="GULLWING_LED" value=""/>
<element name="R1" library="SYNShop" package="0603-RES" value=""/>
<element name="R2" library="SYNShop" package="0603-RES" value=""/>
<element name="R3" library="SYNShop" package="0603-RES" value=""/>
<element name="U$1" library="SparkFun" package="SO08-EIAJ" value="ATTINY45"/>
<element name="ISP1" library="darknet_parts_library" package="AVRISP-POGO" value="AVRISPPOGO"/>
<element name="R4" library="SYNShop" package="0402-RES" value=""/>
</elements>
<signals>
<signal name="VCC">
<contactref element="U$1" pad="8"/>
<contactref element="ISP1" pad="2"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="GND">
<contactref element="LED3" pad="C"/>
<contactref element="LED2" pad="C"/>
<contactref element="LED1" pad="C"/>
<contactref element="U$1" pad="4"/>
<contactref element="ISP1" pad="6"/>
</signal>
<signal name="N$9">
<contactref element="R3" pad="2"/>
<contactref element="LED3" pad="A"/>
</signal>
<signal name="N$10">
<contactref element="R2" pad="2"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="N$11">
<contactref element="R1" pad="2"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="PB3">
<contactref element="R2" pad="1"/>
<contactref element="U$1" pad="2"/>
</signal>
<signal name="PB2">
<contactref element="R1" pad="1"/>
<contactref element="U$1" pad="7"/>
<contactref element="ISP1" pad="3"/>
</signal>
<signal name="PB4">
<contactref element="R3" pad="1"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="N$12">
</signal>
<signal name="N$13">
</signal>
<signal name="N$18">
</signal>
<signal name="N$21">
</signal>
<signal name="N$26">
</signal>
<signal name="RESET">
<contactref element="U$1" pad="1"/>
<contactref element="ISP1" pad="5"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="MOSI">
<contactref element="U$1" pad="5"/>
<contactref element="ISP1" pad="4"/>
</signal>
<signal name="MISO">
<contactref element="U$1" pad="6"/>
<contactref element="ISP1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
