<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="22.86" y2="0" width="0" layer="20"/>
<wire x1="22.86" y1="0" x2="22.86" y2="25.39" width="0" layer="20"/>
<wire x1="22.86" y1="25.39" x2="0" y2="25.39" width="0" layer="20"/>
<wire x1="0" y1="25.39" x2="0" y2="0" width="0" layer="20"/>
<text>CR2032
  PCB
SAVER</text>
<text> MTG
REV A</text>
</plain>
<libraries>
<library name="SparkFun">
<description>Spark Fun Electronics' preferred foot prints. &lt;b&gt;Not to be used for commercial purposes.&lt;/b&gt; We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.</description>
<packages>
<package name="BATTCOM_20MM_PTH">
</package>
<package name="1X01">
</package>
<package name="1X02">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="CR2032" library="SparkFun" package="BATTCOM_20MM_PTH" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="N1" library="SparkFun" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="P2" library="SparkFun" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="P1" library="SparkFun" package="1X02" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="P3" library="SparkFun" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="P4" library="SparkFun" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="N2" library="SparkFun" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="N3" library="SparkFun" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GROUND">
<contactref element="CR2032" pad="2"/>
<contactref element="N1" pad="1"/>
<contactref element="N2" pad="1"/>
<contactref element="N3" pad="1"/>
</signal>
<signal name="3V">
<contactref element="P1" pad="1"/>
<contactref element="P1" pad="2"/>
<contactref element="CR2032" pad="1"/>
<contactref element="P2" pad="2"/>
<contactref element="P2" pad="1"/>
<contactref element="P3" pad="1"/>
<contactref element="P4" pad="1"/>
</signal>
<signal name="N$1">
</signal>
<signal name="N$2">
</signal>
<signal name="N$3">
</signal>
<signal name="N$4">
</signal>
<signal name="N$5">
</signal>
<signal name="N$6">
</signal>
<signal name="N$7">
</signal>
<signal name="N$8">
</signal>
</signals>
</board>
</drawing>
</eagle>
