<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="40.5892" y2="0" width="0" layer="20"/>
<wire x1="40.5892" y1="0" x2="40.5892" y2="32.8168" width="0" layer="20"/>
<wire x1="40.5892" y1="32.8168" x2="0" y2="32.8168" width="0" layer="20"/>
<wire x1="0" y1="32.8168" x2="0" y2="0" width="0" layer="20"/>
<text>Copyright (c) 2020
Feb 2020 v1 Rev1</text>
<text>M1B  M1A  M2A  M2B</text>
<text>GND +12V +5V</text>
<text>SE66 Sec Hull
Board</text>
<text>JLCJLCJLCJLC</text>
<text>GND +5V +5V</text>
<text>M2B M2A M1A M1B</text>
<text>+12V +12V GND</text>
<hole x="20.2946" y="16.4084" drill="10.16"/>
<text>MTR
IN</text>
<text>PWR
IN</text>
<text>MTR OUT</text>
<text>+12V OUT</text>
<text>+12V OUT</text>
</plain>
<libraries>
<library name="Ross Library">
<packages>
<package name="1X3-TERM-BLK-3.5MM-TOP_ENTRY(OST)">
</package>
<package name="1X4-TERM-BLK-3.5MM-TOP_ENTRY(OST)">
</package>
<package name="1X2-TERM-BLK-3.5MM">
</package>
<package name="1X2-TERM-BLK">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="PWR_IN" library="Ross Library" package="1X3-TERM-BLK-3.5MM-TOP_ENTRY(OST)" value="1X3-TERM-BLK-3.5MM-TOP_ENTRY(OST)"/>
<element name="PWR_OUT1" library="Ross Library" package="1X3-TERM-BLK-3.5MM-TOP_ENTRY(OST)" value="1X3-TERM-BLK-3.5MM-TOP_ENTRY(OST)"/>
<element name="MTR_IN" library="Ross Library" package="1X4-TERM-BLK-3.5MM-TOP_ENTRY(OST)" value="1X4-TERM-BLK-3.5MM-TOP_ENTRY(OST)"/>
<element name="PWR_OUT4" library="Ross Library" package="1X3-TERM-BLK-3.5MM-TOP_ENTRY(OST)" value="1X3-TERM-BLK-3.5MM-TOP_ENTRY(OST)"/>
<element name="PWR_OUT2" library="Ross Library" package="1X2-TERM-BLK-3.5MM" value="1X2-TERM-BLK-3.5MM"/>
<element name="PWR_OUT3" library="Ross Library" package="1X2-TERM-BLK-3.5MM" value="1X2-TERM-BLK-3.5MM"/>
<element name="MTR_OUT1" library="Ross Library" package="1X2-TERM-BLK" value="1X2-TERM-BLK"/>
<element name="MTR_OUT2" library="Ross Library" package="1X2-TERM-BLK" value="1X2-TERM-BLK"/>
</elements>
<signals>
<signal name="GND">
<contactref element="PWR_IN" pad="1"/>
<contactref element="PWR_OUT1" pad="1"/>
<contactref element="PWR_OUT4" pad="1"/>
</signal>
<signal name="+12V">
<contactref element="PWR_IN" pad="2"/>
<contactref element="PWR_OUT4" pad="2"/>
<contactref element="PWR_OUT4" pad="3"/>
<contactref element="PWR_OUT2" pad="1"/>
<contactref element="PWR_OUT2" pad="2"/>
<contactref element="PWR_OUT3" pad="1"/>
<contactref element="PWR_OUT3" pad="2"/>
</signal>
<signal name="+5V">
<contactref element="PWR_IN" pad="3"/>
<contactref element="PWR_OUT1" pad="3"/>
<contactref element="PWR_OUT1" pad="2"/>
</signal>
<signal name="M2B">
<contactref element="MTR_IN" pad="4"/>
<contactref element="MTR_OUT1" pad="2"/>
</signal>
<signal name="M2A">
<contactref element="MTR_IN" pad="3"/>
<contactref element="MTR_OUT1" pad="1"/>
</signal>
<signal name="M1A">
<contactref element="MTR_IN" pad="2"/>
<contactref element="MTR_OUT2" pad="2"/>
</signal>
<signal name="M1B">
<contactref element="MTR_IN" pad="1"/>
<contactref element="MTR_OUT2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
