<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.4.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="50.724" y2="0" width="0" layer="20"/>
<wire x1="50.724" y1="0" x2="50.724" y2="50.79" width="0" layer="20"/>
<wire x1="50.724" y1="50.79" x2="0" y2="50.79" width="0" layer="20"/>
<wire x1="0" y1="50.79" x2="0" y2="0" width="0" layer="20"/>
<hole x="48.26" y="48.26" drill="2.8"/>
<hole x="2.54" y="2.54" drill="2.8"/>
<hole x="2.54" y="48.26" drill="2.8"/>
<hole x="48.26" y="2.54" drill="2.8"/>
<text>+</text>
<text>+</text>
<text>Xbee IR Dimmer v0.4</text>
<text>BecomingMaker.com</text>
</plain>
<libraries>
<library name="rcl-ez">
<packages>
<package name="C025-025X050">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.5 mm, outline 2.5 x 5 mm</description>
</package>
<package name="E2,5-5">
<description>&lt;b&gt;ELECTROLYTIC CAPACITOR&lt;/b&gt;&lt;p&gt;
grid 2.54 mm, diameter 5 mm</description>
</package>
</packages>
</library>
<library name="minimidi">
<packages>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
</packages>
</library>
<library name="ulink">
<packages>
<package name="TO92">
<description>&lt;b&gt;VOLTAGE REGULATOR&lt;/b&gt;</description>
</package>
<package name="XBEE">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X3-SHROUDED">
</package>
</packages>
</library>
<library name="transistor-power">
<description>&lt;b&gt;Power Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TO220BV">
<description>&lt;b&gt;Molded Package&lt;/b&gt;&lt;p&gt;
grid 2.54 mm</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AXIAL-0.4">
<description>1/4W Resistor, 0.4" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
<package name="CPOL-RADIAL-100UF-25V">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE-PTH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Atmel_By_element14_Batch_1-00">
<description>Developed by element14 :&lt;br&gt;
element14 CAD Library consolidation.ulp
at 27/07/2012 14:02:49</description>
<packages>
<package name="DIP254P762X533-8">
</package>
</packages>
</library>
<library name="SparkFun-Sensors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find sensors- accelerometers, gyros, compasses, magnetometers, light sensors, imagers, temp sensors, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="BRM-2508">
</package>
</packages>
</library>
<library name="con-wago-500">
<description>&lt;b&gt;Wago Screw Clamps&lt;/b&gt;&lt;p&gt;
Grid 5.00 mm&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="W237-102">
<description>&lt;b&gt;WAGO SCREW CLAMP&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="MyParts">
<packages>
<package name="DSN-MINI-360-HORIZ">
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DO35-10">
<description>&lt;B&gt;DIODE&lt;/B&gt;&lt;p&gt;
diameter 2 mm, horizontal, grid 10.16 mm</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C2" library="rcl-ez" package="C025-025X050" value="0.1uF">
<attribute name="VALUE"/>
</element>
<element name="C3" library="rcl-ez" package="E2,5-5" value="1uF">
<attribute name="VALUE"/>
</element>
<element name="RSSI" library="minimidi" package="LED3MM" value="Red">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ASC" library="minimidi" package="LED3MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="ulink" package="TO92" value="3.3v">
<attribute name="VALUE"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="2X3-SHROUDED" value="">
<attribute name="PROD_ID" value="CONN-10681"/>
</element>
<element name="Q1" library="transistor-power" package="TO220BV" value="MOSFET">
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Passives" package="AXIAL-0.4" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Passives" package="AXIAL-0.4" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Passives" package="AXIAL-0.4" value="87K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Passives" package="AXIAL-0.4" value="22K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Passives" package="AXIAL-0.4" value="4.7K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun-Passives" package="AXIAL-0.4" value="47">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="UP" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="SWITCH-MOMENTARY-2PTH">
<attribute name="PROD_ID" value=" SWCH-08441"/>
<attribute name="NAME"/>
</element>
<element name="DOWN" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="SWITCH-MOMENTARY-2PTH">
<attribute name="PROD_ID" value=" SWCH-08441"/>
<attribute name="NAME"/>
</element>
<element name="ATTINY85" library="Atmel_By_element14_Batch_1-00" package="DIP254P762X533-8" value="ATTINY85-20PU">
<attribute name="OC_FARNELL" value="1455162"/>
<attribute name="OC_NEWARK" value="58M3796"/>
<attribute name="MPN" value="ATTINY85-20PU"/>
<attribute name="SUPPLIER" value="Atmel"/>
<attribute name="PACKAGE" value="PDIP-8"/>
<attribute name="NAME"/>
</element>
<element name="IR" library="SparkFun-Sensors" package="BRM-2508" value="IR">
<attribute name="NAME"/>
</element>
<element name="X1" library="con-wago-500" package="W237-102" value="PWR">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="70K9898"/>
<attribute name="MPN" value="237-102"/>
<attribute name="MF" value=""/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="X2" library="con-wago-500" package="W237-102" value="LOAD">
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="70K9898"/>
<attribute name="MPN" value="237-102"/>
<attribute name="MF" value=""/>
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="XBEE" library="ulink" package="XBEE" value="XBEE">
<attribute name="NAME"/>
</element>
<element name="12V/5V" library="MyParts" package="DSN-MINI-360-HORIZ" value="DSN-MINI-360"/>
<element name="R9" library="SparkFun-Passives" package="AXIAL-0.4" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="SparkFun-Passives" package="AXIAL-0.4" value="1K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Passives" package="CPOL-RADIAL-100UF-25V" value="47uF">
<attribute name="VALUE"/>
<attribute name="NAME"/>
</element>
<element name="D1" library="diode" package="DO35-10" value="BAT42">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun-Passives" package="AXIAL-0.4" value="200">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IRLED" library="minimidi" package="LED3MM" value="Green">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="rcl-ez" package="C025-025X050" value="0.1uF">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="C2" pad="2"/>
<contactref element="IC1" pad="1"/>
<contactref element="C3" pad="-"/>
<contactref element="XBEE" pad="10"/>
<contactref element="ATTINY85" pad="4"/>
<contactref element="JP1" pad="6"/>
<contactref element="UP" pad="3"/>
<contactref element="DOWN" pad="1"/>
<contactref element="IR" pad="2"/>
<contactref element="XBEE" pad="14"/>
<contactref element="Q1" pad="S"/>
<contactref element="R4" pad="P$1"/>
<contactref element="12V/5V" pad="1"/>
<contactref element="12V/5V" pad="4"/>
<contactref element="R9" pad="P$1"/>
<contactref element="R10" pad="P$1"/>
<contactref element="X1" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="XBEE" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="IC1" pad="3"/>
<contactref element="C3" pad="+"/>
<contactref element="XBEE" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="ASC" pad="K"/>
<contactref element="R10" pad="P$2"/>
</signal>
<signal name="N$9">
<contactref element="XBEE" pad="15"/>
<contactref element="ASC" pad="A"/>
</signal>
<signal name="N$16">
<contactref element="XBEE" pad="18"/>
<contactref element="R3" pad="P$2"/>
<contactref element="R5" pad="P$2"/>
</signal>
<signal name="TX">
<contactref element="XBEE" pad="2"/>
<contactref element="R1" pad="P$2"/>
</signal>
<signal name="N$1">
<contactref element="RSSI" pad="A"/>
<contactref element="XBEE" pad="6"/>
</signal>
<signal name="12V">
<contactref element="12V/5V" pad="2"/>
<contactref element="X1" pad="1"/>
<contactref element="X2" pad="2"/>
</signal>
<signal name="5V">
<contactref element="IC1" pad="2"/>
<contactref element="ATTINY85" pad="8"/>
<contactref element="JP1" pad="2"/>
<contactref element="R6" pad="P$2"/>
<contactref element="D1" pad="C"/>
<contactref element="R7" pad="P$1"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="MOSI">
<contactref element="ATTINY85" pad="5"/>
<contactref element="R1" pad="P$1"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="MISO">
<contactref element="ATTINY85" pad="6"/>
<contactref element="DOWN" pad="3"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="RESET">
<contactref element="JP1" pad="5"/>
<contactref element="ATTINY85" pad="1"/>
</signal>
<signal name="SCK">
<contactref element="ATTINY85" pad="7"/>
<contactref element="JP1" pad="3"/>
<contactref element="IR" pad="1"/>
<contactref element="IRLED" pad="K"/>
</signal>
<signal name="N$21">
<contactref element="Q1" pad="G"/>
<contactref element="R2" pad="P$1"/>
</signal>
<signal name="N$22">
<contactref element="R5" pad="P$1"/>
<contactref element="R4" pad="P$2"/>
</signal>
<signal name="N$25">
<contactref element="Q1" pad="D"/>
<contactref element="X2" pad="1"/>
</signal>
<signal name="N$24">
<contactref element="UP" pad="1"/>
<contactref element="ATTINY85" pad="2"/>
</signal>
<signal name="N$7">
<contactref element="IR" pad="3"/>
<contactref element="R6" pad="P$1"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="RSSI" pad="K"/>
<contactref element="R9" pad="P$2"/>
</signal>
<signal name="N$2">
</signal>
<signal name="N$4">
<contactref element="R3" pad="P$1"/>
<contactref element="ATTINY85" pad="3"/>
<contactref element="R2" pad="P$2"/>
</signal>
<signal name="N$3">
<contactref element="D1" pad="A"/>
<contactref element="12V/5V" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="R7" pad="P$2"/>
<contactref element="IRLED" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
