<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.5.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="47.732" y2="0" width="0" layer="20"/>
<wire x1="47.732" y1="0" x2="47.732" y2="22.149" width="0" layer="20"/>
<wire x1="47.732" y1="22.149" x2="0" y2="22.149" width="0" layer="20"/>
<wire x1="0" y1="22.149" x2="0" y2="0" width="0" layer="20"/>
<text>ATMEGA328P Bootloader/Uploader - Rev 1</text>
<text>bootload - upload</text>
</plain>
<libraries>
<library name="capacitor-wima">
<description>&lt;b&gt;WIMA Capacitors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="C2.5-2">
<description>&lt;B&gt;MKS2&lt;/B&gt;, 5 x 2.5 mm, grid 2.54 mm</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X06">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="LED3MM">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
3 mm, round</description>
</package>
<package name="EG1218">
</package>
<package name="0204/7">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
type 0204, grid 7.5 mm</description>
</package>
</packages>
</library>
<library name="SparkFun-IC-Microcontroller">
<description>&lt;h3&gt;SparkFun Microcontrollers&lt;/h3&gt;
This library contains microcontrollers.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="DIP28">
<description>Standard 28-pin DIP package.&lt;br&gt;
IC needs to have legs bent before insertion.</description>
</package>
</packages>
</library>
<library name="SparkFun-Clocks">
<description>&lt;h3&gt;SparkFun Clocks, Oscillators and Resonators&lt;/h3&gt;
This library contains the real-time clocks, oscillators, resonators, and crystals we use. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="HC49US">
<description>&lt;h3&gt;HC49/US 11.6x4.6mm PTH Crystal&lt;/h3&gt;
&lt;p&gt;&lt;a href="https://www.digikey.com/Web%20Export/Supplier%20Content/Citizen_300/PDF/Citizen_HC49US.pdf?redirected=1"&gt;Example Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Retired">
<description>&lt;h3&gt;SparkFun Electronics' Retired foot prints&lt;/h3&gt;
In this library you'll find all manner of retired footprints for resistors, capacitors, board names, ICs, etc., that are &lt;b&gt; no longer used&lt;/b&gt; in our catalog.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE-PTH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="capacitor-wima" package="C2.5-2" value="22pF">
<attribute name="VALUE"/>
</element>
<element name="C2" library="capacitor-wima" package="C2.5-2" value="22pF">
<attribute name="VALUE"/>
</element>
<element name="C3" library="capacitor-wima" package="C2.5-2" value="0.1uF">
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X02" value="RST">
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X06" value="BOOT - gnd vcc vcc sck miso mosi">
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X06" value="FTDI - gnd gnd vcc rx tx rst">
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="SparkFun-IC-Microcontroller" package="DIP28" value="ATMEGA328P">
<attribute name="PROD_ID" value="IC-09136"/>
<attribute name="VALUE"/>
</element>
<element name="Y1" library="SparkFun-Clocks" package="HC49US" value="16MHz">
<attribute name="VALUE"/>
</element>
<element name="RESET" library="SparkFun-Retired" package="TACTILE-PTH" value="">
<attribute name="NAME"/>
</element>
<element name="PWR" library="adafruit" package="LED3MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BLINK" library="adafruit" package="LED3MM" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="S2" library="adafruit" package="EG1218" value="bootload - upload"/>
<element name="R1" library="adafruit" package="0204/7" value="10kohm">
<attribute name="VALUE"/>
</element>
<element name="R2" library="adafruit" package="0204/7" value="330ohm">
<attribute name="VALUE"/>
</element>
<element name="R3" library="adafruit" package="0204/7" value="330ohm">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$2">
<contactref element="PWR" pad="K"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="U1" pad="20"/>
<contactref element="U1" pad="21"/>
<contactref element="U1" pad="7"/>
<contactref element="J2" pad="3"/>
<contactref element="J2" pad="2"/>
<contactref element="J3" pad="3"/>
<contactref element="PWR" pad="A"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="Y1" pad="2"/>
<contactref element="U1" pad="9"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="Y1" pad="1"/>
<contactref element="U1" pad="10"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="RESET">
<contactref element="U1" pad="1"/>
<contactref element="J1" pad="2"/>
<contactref element="J1" pad="1"/>
<contactref element="RESET" pad="1"/>
<contactref element="S2" pad="P"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="SCK">
<contactref element="U1" pad="19"/>
<contactref element="J2" pad="4"/>
<contactref element="BLINK" pad="A"/>
</signal>
<signal name="MISO">
<contactref element="U1" pad="18"/>
<contactref element="J2" pad="5"/>
</signal>
<signal name="MOSI">
<contactref element="U1" pad="17"/>
<contactref element="J2" pad="6"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="U1" pad="8"/>
<contactref element="U1" pad="22"/>
<contactref element="C2" pad="2"/>
<contactref element="J2" pad="1"/>
<contactref element="J3" pad="2"/>
<contactref element="J3" pad="1"/>
<contactref element="RESET" pad="3"/>
<contactref element="R3" pad="1"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="RX">
<contactref element="U1" pad="2"/>
<contactref element="J3" pad="4"/>
</signal>
<signal name="TX">
<contactref element="U1" pad="3"/>
<contactref element="J3" pad="5"/>
</signal>
<signal name="N$3">
<contactref element="C3" pad="1"/>
<contactref element="S2" pad="S"/>
</signal>
<signal name="FTDI-RST">
<contactref element="C3" pad="2"/>
<contactref element="J3" pad="6"/>
</signal>
<signal name="N$1">
<contactref element="BLINK" pad="K"/>
<contactref element="R3" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
